## golden top Board Configuration

www.terasic.com
Copyright © 2003-2023 Terasic Inc. All Rights Reserved.

### Pin Assignments:

##

CLOCK
Name | Location | Direction | IO Standard
--- | --- | --- | ---
CLK_100_B2B_p | BF68 | input | 1.2V TRUE DIFFERENTIAL SIGNALING
CLK_50_5A | CH128 | input | 3.3-V LVCMOS
CLK_50_6A | BP22 | input | 3.3-V LVCMOS
CLK_50_6C | D8 | input | 3.3-V LVCMOS

##

Buttons
Name | Location | Direction | IO Standard
--- | --- | --- | ---
CPU_RESET_n | BU52 | input | 1.2 V
BUTTON[0] | H8 | input | 3.3-V LVCMOS
BUTTON[1] | C2 | input | 3.3-V LVCMOS
BUTTON[2] | D4 | input | 3.3-V LVCMOS
BUTTON[3] | F4 | input | 3.3-V LVCMOS

##

Swtiches
Name | Location | Direction | IO Standard
--- | --- | --- | ---
SW[0] | CK4 | input | 3.3-V LVCMOS
SW[1] | CH4 | input | 3.3-V LVCMOS
SW[2] | K8 | input | 3.3-V LVCMOS
SW[3] | F8 | input | 3.3-V LVCMOS

##

LED
Name | Location | Direction | IO Standard
--- | --- | --- | ---
LED[0] | BF120 | output | 3.3-V LVCMOS
LED[1] | B39 | output | 3.3-V LVCMOS
LED[2] | B4 | output | 3.3-V LVCMOS
LED[3] | A11 | output | 3.3-V LVCMOS

##

DDR4A
Name | Location | Direction | IO Standard
--- | --- | --- | ---
DDR4A_REFCLK_p | AB117 | input | 1.2V TRUE DIFFERENTIAL SIGNALING
DDR4A_A[0] | T114 | output | SSTL-12
DDR4A_A[1] | P114 | output | SSTL-12
DDR4A_A[2] | V117 | output | SSTL-12
DDR4A_A[3] | T117 | output | SSTL-12
DDR4A_A[4] | M114 | output | SSTL-12
DDR4A_A[5] | K114 | output | SSTL-12
DDR4A_A[6] | V108 | output | SSTL-12
DDR4A_A[7] | T108 | output | SSTL-12
DDR4A_A[8] | T105 | output | SSTL-12
DDR4A_A[9] | P105 | output | SSTL-12
DDR4A_A[10] | M105 | output | SSTL-12
DDR4A_A[11] | K105 | output | SSTL-12
DDR4A_A[12] | AG111 | output | SSTL-12
DDR4A_A[13] | Y114 | output | SSTL-12
DDR4A_A[14] | AB114 | output | SSTL-12
DDR4A_A[15] | AK107 | output | SSTL-12
DDR4A_A[16] | AK104 | output | SSTL-12
DDR4A_BA[0] | AB108 | output | SSTL-12
DDR4A_BA[1] | Y105 | output | SSTL-12
DDR4A_BG[0] | AB105 | output | SSTL-12
DDR4A_CK | H108 | output | DIFFERENTIAL 1.2-V SSTL
DDR4A_CK_n | F108 | output | DIFFERENTIAL 1.2-V SSTL
DDR4A_CKE | F105 | output | SSTL-12
DDR4A_DQS[0] | B122 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS[1] | AG90 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS[2] | K95 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS[3] | F95 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS_n[0] | A125 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS_n[1] | AG93 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS_n[2] | M95 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS_n[3] | D95 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQ[0] | B128 | inout | 1.2-V POD
DDR4A_DQ[1] | A116 | inout | 1.2-V POD
DDR4A_DQ[2] | B130 | inout | 1.2-V POD
DDR4A_DQ[3] | B116 | inout | 1.2-V POD
DDR4A_DQ[4] | A130 | inout | 1.2-V POD
DDR4A_DQ[5] | B113 | inout | 1.2-V POD
DDR4A_DQ[6] | A128 | inout | 1.2-V POD
DDR4A_DQ[7] | A113 | inout | 1.2-V POD
DDR4A_DQ[8] | AG100 | inout | 1.2-V POD
DDR4A_DQ[9] | Y98 | inout | 1.2-V POD
DDR4A_DQ[10] | AC100 | inout | 1.2-V POD
DDR4A_DQ[11] | AG104 | inout | 1.2-V POD
DDR4A_DQ[12] | AC96 | inout | 1.2-V POD
DDR4A_DQ[13] | Y95 | inout | 1.2-V POD
DDR4A_DQ[14] | Y87 | inout | 1.2-V POD
DDR4A_DQ[15] | Y84 | inout | 1.2-V POD
DDR4A_DQ[16] | V98 | inout | 1.2-V POD
DDR4A_DQ[17] | T98 | inout | 1.2-V POD
DDR4A_DQ[18] | P95 | inout | 1.2-V POD
DDR4A_DQ[19] | T95 | inout | 1.2-V POD
DDR4A_DQ[20] | K84 | inout | 1.2-V POD
DDR4A_DQ[21] | M84 | inout | 1.2-V POD
DDR4A_DQ[22] | T84 | inout | 1.2-V POD
DDR4A_DQ[23] | P84 | inout | 1.2-V POD
DDR4A_DQ[24] | H98 | inout | 1.2-V POD
DDR4A_DQ[25] | M98 | inout | 1.2-V POD
DDR4A_DQ[26] | K87 | inout | 1.2-V POD
DDR4A_DQ[27] | K98 | inout | 1.2-V POD
DDR4A_DQ[28] | F98 | inout | 1.2-V POD
DDR4A_DQ[29] | F84 | inout | 1.2-V POD
DDR4A_DQ[30] | M87 | inout | 1.2-V POD
DDR4A_DQ[31] | D84 | inout | 1.2-V POD
DDR4A_DBI_n[0] | B119 | inout | 1.2-V POD
DDR4A_DBI_n[1] | AC90 | inout | 1.2-V POD
DDR4A_DBI_n[2] | V87 | inout | 1.2-V POD
DDR4A_DBI_n[3] | H87 | inout | 1.2-V POD
DDR4A_CS_n | K117 | output | SSTL-12
DDR4A_RESET_n | H117 | output | SSTL-12
DDR4A_ODT | F114 | output | SSTL-12
DDR4A_PAR | K108 | output | SSTL-12
DDR4A_ALERT_n | Y108 | input | 1.2 V
DDR4A_ACT_n | M117 | output | SSTL-12
DDR4A_RZQ | AK111 | input | 1.2 V

##

DDR4B
Name | Location | Direction | IO Standard
--- | --- | --- | ---
DDR4B_REFCLK_p | AC68 | input | 1.2V TRUE DIFFERENTIAL SIGNALING
DDR4B_A[0] | P74 | output | SSTL-12
DDR4B_A[1] | T74 | output | SSTL-12
DDR4B_A[2] | V77 | output | SSTL-12
DDR4B_A[3] | T77 | output | SSTL-12
DDR4B_A[4] | M74 | output | SSTL-12
DDR4B_A[5] | K74 | output | SSTL-12
DDR4B_A[6] | V67 | output | SSTL-12
DDR4B_A[7] | T67 | output | SSTL-12
DDR4B_A[8] | M65 | output | SSTL-12
DDR4B_A[9] | K65 | output | SSTL-12
DDR4B_A[10] | T65 | output | SSTL-12
DDR4B_A[11] | P65 | output | SSTL-12
DDR4B_A[12] | AG79 | output | SSTL-12
DDR4B_A[13] | AG72 | output | SSTL-12
DDR4B_A[14] | AG75 | output | SSTL-12
DDR4B_A[15] | AG83 | output | SSTL-12
DDR4B_A[16] | AC83 | output | SSTL-12
DDR4B_BA[0] | Y74 | output | SSTL-12
DDR4B_BA[1] | Y67 | output | SSTL-12
DDR4B_BG[0] | Y65 | output | SSTL-12
DDR4B_CK | H67 | output | DIFFERENTIAL 1.2-V SSTL
DDR4B_CK_n | F67 | output | DIFFERENTIAL 1.2-V SSTL
DDR4B_CKE | M67 | output | SSTL-12
DDR4B_DQS[0] | A80 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS[1] | F55 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS[2] | K55 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS[3] | AG57 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS_n[0] | B76 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS_n[1] | D55 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS_n[2] | M55 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS_n[3] | AG53 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQ[0] | A82 | inout | 1.2-V POD
DDR4B_DQ[1] | B70 | inout | 1.2-V POD
DDR4B_DQ[2] | A85 | inout | 1.2-V POD
DDR4B_DQ[3] | B85 | inout | 1.2-V POD
DDR4B_DQ[4] | B82 | inout | 1.2-V POD
DDR4B_DQ[5] | B66 | inout | 1.2-V POD
DDR4B_DQ[6] | A70 | inout | 1.2-V POD
DDR4B_DQ[7] | A66 | inout | 1.2-V POD
DDR4B_DQ[8] | F58 | inout | 1.2-V POD
DDR4B_DQ[9] | D44 | inout | 1.2-V POD
DDR4B_DQ[10] | H58 | inout | 1.2-V POD
DDR4B_DQ[11] | F47 | inout | 1.2-V POD
DDR4B_DQ[12] | K58 | inout | 1.2-V POD
DDR4B_DQ[13] | F44 | inout | 1.2-V POD
DDR4B_DQ[14] | M58 | inout | 1.2-V POD
DDR4B_DQ[15] | H47 | inout | 1.2-V POD
DDR4B_DQ[16] | P55 | inout | 1.2-V POD
DDR4B_DQ[17] | T55 | inout | 1.2-V POD
DDR4B_DQ[18] | V58 | inout | 1.2-V POD
DDR4B_DQ[19] | T58 | inout | 1.2-V POD
DDR4B_DQ[20] | P44 | inout | 1.2-V POD
DDR4B_DQ[21] | T44 | inout | 1.2-V POD
DDR4B_DQ[22] | K44 | inout | 1.2-V POD
DDR4B_DQ[23] | M44 | inout | 1.2-V POD
DDR4B_DQ[24] | Y55 | inout | 1.2-V POD
DDR4B_DQ[25] | AC61 | inout | 1.2-V POD
DDR4B_DQ[26] | Y44 | inout | 1.2-V POD
DDR4B_DQ[27] | AG61 | inout | 1.2-V POD
DDR4B_DQ[28] | Y58 | inout | 1.2-V POD
DDR4B_DQ[29] | AG64 | inout | 1.2-V POD
DDR4B_DQ[30] | Y47 | inout | 1.2-V POD
DDR4B_DQ[31] | AC64 | inout | 1.2-V POD
DDR4B_DBI_n[0] | B73 | inout | 1.2-V POD
DDR4B_DBI_n[1] | M47 | inout | 1.2-V POD
DDR4B_DBI_n[2] | V47 | inout | 1.2-V POD
DDR4B_DBI_n[3] | AC53 | inout | 1.2-V POD
DDR4B_CS_n | F77 | output | SSTL-12
DDR4B_RESET_n | M77 | output | SSTL-12
DDR4B_ODT | D74 | output | SSTL-12
DDR4B_PAR | D65 | output | SSTL-12
DDR4B_ALERT_n | Y77 | input | 1.2 V
DDR4B_ACT_n | H77 | output | SSTL-12
DDR4B_RZQ | AC79 | input | 1.2 V

##

HDMI
Name | Location | Direction | IO Standard
--- | --- | --- | ---
HDMI_LRCLK | BP112 | inout | 3.3-V LVCMOS
HDMI_MCLK | BM118 | inout | 3.3-V LVCMOS
HDMI_SCLK | BM112 | inout | 3.3-V LVCMOS
HDMI_TX_CLK | BF104 | output | 3.3-V LVCMOS
HDMI_TX_HS | BR109 | output | 3.3-V LVCMOS
HDMI_TX_VS | BE107 | output | 3.3-V LVCMOS
HDMI_TX_D[0] | CD134 | output | 3.3-V LVCMOS
HDMI_TX_D[1] | CD135 | output | 3.3-V LVCMOS
HDMI_TX_D[2] | CG134 | output | 3.3-V LVCMOS
HDMI_TX_D[3] | CG135 | output | 3.3-V LVCMOS
HDMI_TX_D[4] | CH132 | output | 3.3-V LVCMOS
HDMI_TX_D[5] | CF132 | output | 3.3-V LVCMOS
HDMI_TX_D[6] | CF128 | output | 3.3-V LVCMOS
HDMI_TX_D[7] | CK134 | output | 3.3-V LVCMOS
HDMI_TX_D[8] | CL125 | output | 3.3-V LVCMOS
HDMI_TX_D[9] | CF121 | output | 3.3-V LVCMOS
HDMI_TX_D[10] | CF118 | output | 3.3-V LVCMOS
HDMI_TX_D[11] | BU118 | output | 3.3-V LVCMOS
HDMI_TX_D[12] | BR118 | output | 3.3-V LVCMOS
HDMI_TX_D[13] | CA118 | output | 3.3-V LVCMOS
HDMI_TX_D[14] | BW118 | output | 3.3-V LVCMOS
HDMI_TX_D[15] | CL128 | output | 3.3-V LVCMOS
HDMI_TX_D[16] | CL130 | output | 3.3-V LVCMOS
HDMI_TX_D[17] | CK125 | output | 3.3-V LVCMOS
HDMI_TX_D[18] | CK128 | output | 3.3-V LVCMOS
HDMI_TX_D[19] | BF111 | output | 3.3-V LVCMOS
HDMI_TX_D[20] | BH109 | output | 3.3-V LVCMOS
HDMI_TX_D[21] | BE115 | output | 3.3-V LVCMOS
HDMI_TX_D[22] | BF115 | output | 3.3-V LVCMOS
HDMI_TX_D[23] | BU109 | output | 3.3-V LVCMOS
HDMI_TX_DE | BK109 | output | 3.3-V LVCMOS
HDMI_I2C_SCL | BR112 | inout | 3.3-V LVCMOS
HDMI_I2C_SDA | BM109 | inout | 3.3-V LVCMOS
HDMI_TX_INT | BE111 | input | 3.3-V LVCMOS
HDMI_I2S | BK118 | inout | 3.3-V LVCMOS

##

ENET
Name | Location | Direction | IO Standard
--- | --- | --- | ---
ENET_88E2110_TX_p | AL129 | output | HIGH SPEED DIFFERENTIAL I/O
ENET_88E2110_TX_n | AL126 | output | HIGH SPEED DIFFERENTIAL I/O
ENET_88E2110_RX_p | AK135 | input | HIGH SPEED DIFFERENTIAL I/O
ENET_88E2110_RX_n | AK133 | input | HIGH SPEED DIFFERENTIAL I/O
ENET_88E2110_REFCLK_125M_p | AT120 | input | CURRENT MODE LOGIC (CML)
ENET_88E2110_INT_n | A20 | input | 3.3-V LVCMOS
ENET_88E2110_MDC | B14 | output | 3.3-V LVCMOS
ENET_88E2110_MDIO | A14 | inout | 3.3-V LVCMOS
ENET_88E2110_RESET_n | B11 | output | 3.3-V LVCMOS

##

SI5340B
Name | Location | Direction | IO Standard
--- | --- | --- | ---
SI5340B_I2C_SCL | A51 | inout | 1.2 V
SI5340B_I2C_SDA | B51 | inout | 1.2 V
SI5340B_OE_n | A54 | output | 1.2 V
SI5340B_RST_n | B54 | output | 1.2 V

##

SI5391B
Name | Location | Direction | IO Standard
--- | --- | --- | ---
SI5391B_I2C_SCL | B42 | inout | 1.2 V
SI5391B_I2C_SDA | A45 | inout | 1.2 V
SI5391B_OE_n | B45 | output | 1.2 V
SI5391B_RST_n | A48 | output | 1.2 V

##

GPIO
Name | Location | Direction | IO Standard
--- | --- | --- | ---
GPIO[0] | BK31 | inout | 3.3-V LVCMOS
GPIO[1] | BU28 | inout | 3.3-V LVCMOS
GPIO[2] | BF25 | inout | 3.3-V LVCMOS
GPIO[3] | BP31 | inout | 3.3-V LVCMOS
GPIO[4] | BR28 | inout | 3.3-V LVCMOS
GPIO[5] | BR31 | inout | 3.3-V LVCMOS
GPIO[6] | BU31 | inout | 3.3-V LVCMOS
GPIO[7] | BM28 | inout | 3.3-V LVCMOS
GPIO[8] | BW28 | inout | 3.3-V LVCMOS
GPIO[9] | BM31 | inout | 3.3-V LVCMOS
GPIO[10] | BK28 | inout | 3.3-V LVCMOS
GPIO[11] | BR22 | inout | 3.3-V LVCMOS
GPIO[12] | CH12 | inout | 3.3-V LVCMOS
GPIO[13] | BU22 | inout | 3.3-V LVCMOS
GPIO[14] | BW19 | inout | 3.3-V LVCMOS
GPIO[15] | BH28 | inout | 3.3-V LVCMOS
GPIO[16] | BM22 | inout | 3.3-V LVCMOS
GPIO[17] | CF12 | inout | 3.3-V LVCMOS
GPIO[18] | BK19 | inout | 3.3-V LVCMOS
GPIO[19] | CF9 | inout | 3.3-V LVCMOS
GPIO[20] | BF21 | inout | 3.3-V LVCMOS
GPIO[21] | BE21 | inout | 3.3-V LVCMOS
GPIO[22] | BE43 | inout | 3.3-V LVCMOS
GPIO[23] | BF40 | inout | 3.3-V LVCMOS
GPIO[24] | BE25 | inout | 3.3-V LVCMOS
GPIO[25] | BF32 | inout | 3.3-V LVCMOS
GPIO[26] | BF36 | inout | 3.3-V LVCMOS
GPIO[27] | BF29 | inout | 3.3-V LVCMOS
GPIO[28] | CJ2 | inout | 3.3-V LVCMOS
GPIO[29] | BF16 | inout | 3.3-V LVCMOS
GPIO[30] | BH19 | inout | 3.3-V LVCMOS
GPIO[31] | BK22 | inout | 3.3-V LVCMOS
GPIO[32] | BM19 | inout | 3.3-V LVCMOS
GPIO[33] | BU19 | inout | 3.3-V LVCMOS
GPIO[34] | BR19 | inout | 3.3-V LVCMOS
GPIO[35] | CK2 | inout | 3.3-V LVCMOS

##

TMD
Name | Location | Direction | IO Standard
--- | --- | --- | ---
TMD_D[0] | F18 | inout | 3.3-V LVCMOS
TMD_D[1] | F15 | inout | 3.3-V LVCMOS
TMD_D[2] | F27 | inout | 3.3-V LVCMOS
TMD_D[3] | F24 | inout | 3.3-V LVCMOS
TMD_D[4] | H27 | inout | 3.3-V LVCMOS
TMD_D[5] | D24 | inout | 3.3-V LVCMOS
TMD_D[6] | H18 | inout | 3.3-V LVCMOS
TMD_D[7] | D15 | inout | 3.3-V LVCMOS

##

FMCP
Name | Location | Direction | IO Standard
--- | --- | --- | ---
FMCP_CLK2_BIDIR_p | CF49 | inout | 1.2 V
FMCP_CLK2_BIDIR_n | CH49 | inout | 1.2 V
FMCP_CLK3_BIDIR_p | BW49 | inout | 1.2 V
FMCP_CLK3_BIDIR_n | CA49 | inout | 1.2 V
FMCP_DP_C2M_p[0] | BY7 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_C2M_p[1] | BT7 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_C2M_p[2] | BL7 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_C2M_p[3] | BG7 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_C2M_p[4] | BE7 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_C2M_p[5] | BC7 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_C2M_p[6] | BA7 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_C2M_p[7] | AW7 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_C2M_p[8] | AU7 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_C2M_p[9] | AR7 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_C2M_p[10] | AN7 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_C2M_p[11] | AL7 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_C2M_n[0] | BY10 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_C2M_n[1] | BT10 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_C2M_n[2] | BL10 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_C2M_n[3] | BG10 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_C2M_n[4] | BE10 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_C2M_n[5] | BC10 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_C2M_n[6] | BA10 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_C2M_n[7] | AW10 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_C2M_n[8] | AU10 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_C2M_n[9] | AR10 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_C2M_n[10] | AN10 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_C2M_n[11] | AL10 | output | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_p[0] | CB1 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_p[1] | BV1 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_p[2] | BN1 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_p[3] | BJ1 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_p[4] | BF1 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_p[5] | BD1 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_p[6] | BB1 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_p[7] | AY1 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_p[8] | AV1 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_p[9] | AT1 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_p[10] | AP1 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_p[11] | AM1 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_n[0] | CB3 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_n[1] | BV3 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_n[2] | BN3 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_n[3] | BJ3 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_n[4] | BF3 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_n[5] | BD3 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_n[6] | BB3 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_n[7] | AY3 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_n[8] | AV3 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_n[9] | AT3 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_n[10] | AP3 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_DP_M2C_n[11] | AM3 | input | HIGH SPEED DIFFERENTIAL I/O
FMCP_HA_p[0] | BM69 | inout | 1.2 V
FMCP_HA_p[1] | BM71 | inout | 1.2 V
FMCP_HA_p[2] | BH62 | inout | 1.2 V
FMCP_HA_p[3] | BR69 | inout | 1.2 V
FMCP_HA_p[4] | BW69 | inout | 1.2 V
FMCP_HA_p[5] | BU59 | inout | 1.2 V
FMCP_HA_p[6] | BH69 | inout | 1.2 V
FMCP_HA_p[7] | CH69 | inout | 1.2 V
FMCP_HA_p[8] | CF59 | inout | 1.2 V
FMCP_HA_p[9] | BW59 | inout | 1.2 V
FMCP_HA_p[10] | CA62 | inout | 1.2 V
FMCP_HA_p[11] | BM59 | inout | 1.2 V
FMCP_HA_p[12] | BM62 | inout | 1.2 V
FMCP_HA_p[13] | CF62 | inout | 1.2 V
FMCP_HA_p[14] | CC71 | inout | 1.2 V
FMCP_HA_p[15] | CF71 | inout | 1.2 V
FMCP_HA_p[16] | BU62 | inout | 1.2 V
FMCP_HA_p[17] | BF75 | inout | 1.2 V
FMCP_HA_p[18] | BE83 | inout | 1.2 V
FMCP_HA_p[19] | BE79 | inout | 1.2 V
FMCP_HA_p[20] | BR71 | inout | 1.2 V
FMCP_HA_p[21] | BF93 | inout | 1.2 V
FMCP_HA_p[22] | BF86 | inout | 1.2 V
FMCP_HA_p[23] | BE96 | inout | 1.2 V
FMCP_HA_n[0] | BK69 | inout | 1.2 V
FMCP_HA_n[1] | BP71 | inout | 1.2 V
FMCP_HA_n[2] | BH59 | inout | 1.2 V
FMCP_HA_n[3] | BU69 | inout | 1.2 V
FMCP_HA_n[4] | CA69 | inout | 1.2 V
FMCP_HA_n[5] | BR59 | inout | 1.2 V
FMCP_HA_n[6] | BH71 | inout | 1.2 V
FMCP_HA_n[7] | CF69 | inout | 1.2 V
FMCP_HA_n[8] | CH59 | inout | 1.2 V
FMCP_HA_n[9] | CA59 | inout | 1.2 V
FMCP_HA_n[10] | CC62 | inout | 1.2 V
FMCP_HA_n[11] | BK59 | inout | 1.2 V
FMCP_HA_n[12] | BP62 | inout | 1.2 V
FMCP_HA_n[13] | CH62 | inout | 1.2 V
FMCP_HA_n[14] | CA71 | inout | 1.2 V
FMCP_HA_n[15] | CH71 | inout | 1.2 V
FMCP_HA_n[16] | BR62 | inout | 1.2 V
FMCP_HA_n[17] | BF72 | inout | 1.2 V
FMCP_HA_n[18] | BF83 | inout | 1.2 V
FMCP_HA_n[19] | BE75 | inout | 1.2 V
FMCP_HA_n[20] | BU71 | inout | 1.2 V
FMCP_HA_n[21] | BF90 | inout | 1.2 V
FMCP_HA_n[22] | BE86 | inout | 1.2 V
FMCP_HA_n[23] | BE93 | inout | 1.2 V
FMCP_HB_p[0] | BR81 | inout | 1.2 V
FMCP_HB_p[1] | BW78 | inout | 1.2 V
FMCP_HB_p[2] | CL91 | inout | 1.2 V
FMCP_HB_p[3] | BM81 | inout | 1.2 V
FMCP_HB_p[4] | BK89 | inout | 1.2 V
FMCP_HB_p[5] | CF81 | inout | 1.2 V
FMCP_HB_p[6] | BR92 | inout | 1.2 V
FMCP_HB_p[7] | BH89 | inout | 1.2 V
FMCP_HB_p[8] | CH89 | inout | 1.2 V
FMCP_HB_p[9] | CK97 | inout | 1.2 V
FMCP_HB_p[10] | CL88 | inout | 1.2 V
FMCP_HB_p[11] | BR89 | inout | 1.2 V
FMCP_HB_p[12] | CH78 | inout | 1.2 V
FMCP_HB_p[13] | BR78 | inout | 1.2 V
FMCP_HB_p[14] | CK76 | inout | 1.2 V
FMCP_HB_p[15] | CK85 | inout | 1.2 V
FMCP_HB_p[16] | CA81 | inout | 1.2 V
FMCP_HB_p[17] | BM78 | inout | 1.2 V
FMCP_HB_p[18] | BH81 | inout | 1.2 V
FMCP_HB_p[19] | CK80 | inout | 1.2 V
FMCP_HB_p[20] | CC92 | inout | 1.2 V
FMCP_HB_p[21] | CF92 | inout | 1.2 V
FMCP_HB_n[0] | BU81 | inout | 1.2 V
FMCP_HB_n[1] | CA78 | inout | 1.2 V
FMCP_HB_n[2] | CK94 | inout | 1.2 V
FMCP_HB_n[3] | BP81 | inout | 1.2 V
FMCP_HB_n[4] | BM89 | inout | 1.2 V
FMCP_HB_n[5] | CH81 | inout | 1.2 V
FMCP_HB_n[6] | BU92 | inout | 1.2 V
FMCP_HB_n[7] | BH92 | inout | 1.2 V
FMCP_HB_n[8] | CF89 | inout | 1.2 V
FMCP_HB_n[9] | CL97 | inout | 1.2 V
FMCP_HB_n[10] | CK88 | inout | 1.2 V
FMCP_HB_n[11] | BU89 | inout | 1.2 V
FMCP_HB_n[12] | CF78 | inout | 1.2 V
FMCP_HB_n[13] | BU78 | inout | 1.2 V
FMCP_HB_n[14] | CL76 | inout | 1.2 V
FMCP_HB_n[15] | CL85 | inout | 1.2 V
FMCP_HB_n[16] | CC81 | inout | 1.2 V
FMCP_HB_n[17] | BK78 | inout | 1.2 V
FMCP_HB_n[18] | BH78 | inout | 1.2 V
FMCP_HB_n[19] | CL82 | inout | 1.2 V
FMCP_HB_n[20] | CA92 | inout | 1.2 V
FMCP_HB_n[21] | CH92 | inout | 1.2 V
FMCP_LA_p[0] | BK38 | inout | 1.2 V
FMCP_LA_p[1] | BE61 | inout | 1.2 V
FMCP_LA_p[2] | BF57 | inout | 1.2 V
FMCP_LA_p[3] | CK8 | inout | 1.2 V
FMCP_LA_p[4] | BF50 | inout | 1.2 V
FMCP_LA_p[5] | CL14 | inout | 1.2 V
FMCP_LA_p[6] | CK11 | inout | 1.2 V
FMCP_LA_p[7] | BE64 | inout | 1.2 V
FMCP_LA_p[8] | BE46 | inout | 1.2 V
FMCP_LA_p[9] | CF19 | inout | 1.2 V
FMCP_LA_p[10] | CF22 | inout | 1.2 V
FMCP_LA_p[11] | BM52 | inout | 1.2 V
FMCP_LA_p[12] | BP41 | inout | 1.2 V
FMCP_LA_p[13] | CC22 | inout | 1.2 V
FMCP_LA_p[14] | BH38 | inout | 1.2 V
FMCP_LA_p[15] | BH49 | inout | 1.2 V
FMCP_LA_p[16] | BK49 | inout | 1.2 V
FMCP_LA_p[17] | BR49 | inout | 1.2 V
FMCP_LA_p[18] | CK30 | inout | 1.2 V
FMCP_LA_p[19] | CK66 | inout | 1.2 V
FMCP_LA_p[20] | CK63 | inout | 1.2 V
FMCP_LA_p[21] | CK33 | inout | 1.2 V
FMCP_LA_p[22] | CA38 | inout | 1.2 V
FMCP_LA_p[23] | BR38 | inout | 1.2 V
FMCP_LA_p[24] | CC41 | inout | 1.2 V
FMCP_LA_p[25] | CH41 | inout | 1.2 V
FMCP_LA_p[26] | CK39 | inout | 1.2 V
FMCP_LA_p[27] | CK35 | inout | 1.2 V
FMCP_LA_p[28] | CC52 | inout | 1.2 V
FMCP_LA_p[29] | CF52 | inout | 1.2 V
FMCP_LA_p[30] | CL56 | inout | 1.2 V
FMCP_LA_p[31] | CL51 | inout | 1.2 V
FMCP_LA_p[32] | CK73 | inout | 1.2 V
FMCP_LA_p[33] | CK56 | inout | 1.2 V
FMCP_LA_n[0] | BM38 | inout | 1.2 V
FMCP_LA_n[1] | BE57 | inout | 1.2 V
FMCP_LA_n[2] | BF53 | inout | 1.2 V
FMCP_LA_n[3] | CL6 | inout | 1.2 V
FMCP_LA_n[4] | BE50 | inout | 1.2 V
FMCP_LA_n[5] | CL11 | inout | 1.2 V
FMCP_LA_n[6] | CL8 | inout | 1.2 V
FMCP_LA_n[7] | BF64 | inout | 1.2 V
FMCP_LA_n[8] | BF46 | inout | 1.2 V
FMCP_LA_n[9] | CC19 | inout | 1.2 V
FMCP_LA_n[10] | CH22 | inout | 1.2 V
FMCP_LA_n[11] | BP52 | inout | 1.2 V
FMCP_LA_n[12] | BM41 | inout | 1.2 V
FMCP_LA_n[13] | CA22 | inout | 1.2 V
FMCP_LA_n[14] | BH41 | inout | 1.2 V
FMCP_LA_n[15] | BH52 | inout | 1.2 V
FMCP_LA_n[16] | BM49 | inout | 1.2 V
FMCP_LA_n[17] | BU49 | inout | 1.2 V
FMCP_LA_n[18] | CL26 | inout | 1.2 V
FMCP_LA_n[19] | CL70 | inout | 1.2 V
FMCP_LA_n[20] | CL66 | inout | 1.2 V
FMCP_LA_n[21] | CL30 | inout | 1.2 V
FMCP_LA_n[22] | BW38 | inout | 1.2 V
FMCP_LA_n[23] | BU38 | inout | 1.2 V
FMCP_LA_n[24] | CA41 | inout | 1.2 V
FMCP_LA_n[25] | CF41 | inout | 1.2 V
FMCP_LA_n[26] | CL39 | inout | 1.2 V
FMCP_LA_n[27] | CL35 | inout | 1.2 V
FMCP_LA_n[28] | CA52 | inout | 1.2 V
FMCP_LA_n[29] | CH52 | inout | 1.2 V
FMCP_LA_n[30] | CL60 | inout | 1.2 V
FMCP_LA_n[31] | CK54 | inout | 1.2 V
FMCP_LA_n[32] | CL73 | inout | 1.2 V
FMCP_LA_n[33] | CL54 | inout | 1.2 V
FMCP_CLK_M2C_p[0] | CH38 | input | 1.2V TRUE DIFFERENTIAL SIGNALING
FMCP_CLK_M2C_p[1] | BP92 | input | 1.2V TRUE DIFFERENTIAL SIGNALING
FMCP_GBTCLK_M2C_p[0] | BB16 | input | CURRENT MODE LOGIC (CML)
FMCP_GBTCLK_M2C_p[1] | AV16 | input | CURRENT MODE LOGIC (CML)
FMCP_GBTCLK_M2C_p[2] | AP16 | input | CURRENT MODE LOGIC (CML)
FMCP_REFCLK_C2M_p | BR41 | output | DIFFERENTIAL 1.2-V SSTL
FMCP_REFCLK_M2C_p | CK48 | input | 1.2V TRUE DIFFERENTIAL SIGNALING
FMCP_REFCLK_p[0] | BC29 | input | CURRENT MODE LOGIC (CML)
FMCP_REFCLK_p[1] | AY16 | input | CURRENT MODE LOGIC (CML)
FMCP_REFCLK_p[2] | AT16 | input | CURRENT MODE LOGIC (CML)
FMCP_RES0 | BE29 | input | 3.3-V LVCMOS
FMCP_SCL | BH118 | inout | 3.3-V LVCMOS
FMCP_SDA | BK112 | inout | 3.3-V LVCMOS
FMCP_SYNC_C2M_p | CL42 | output | DIFFERENTIAL 1.2-V SSTL
FMCP_SYNC_M2C_p | BW89 | input | 1.2V TRUE DIFFERENTIAL SIGNALING

##

PCIE
Name | Location | Direction | IO Standard
--- | --- | --- | ---
PCIE_TX_p[0] | BY129 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_p[1] | BT129 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_p[2] | BL129 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_p[3] | BG129 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_n[0] | BY126 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_n[1] | BT126 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_n[2] | BL126 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_n[3] | BG126 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_p[0] | BV135 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_p[1] | BN135 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_p[2] | BJ135 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_p[3] | BF135 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_n[0] | BV133 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_n[1] | BN133 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_n[2] | BJ133 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_n[3] | BF133 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_OB_REFCLK_p | BC111 | input | CURRENT MODE LOGIC (CML)
PCIE_REFCLK_p | BB120 | input | CURRENT MODE LOGIC (CML)
PCIE_PERST_n | BF107 | input | 3.3-V LVCMOS
PCIE_WAKE_n | D34 | output | 3.3-V LVCMOS

##

QSFP
Name | Location | Direction | IO Standard
--- | --- | --- | ---
QSFP_TX_p[0] | BE129 | output | HIGH SPEED DIFFERENTIAL I/O
QSFP_TX_p[1] | BC129 | output | HIGH SPEED DIFFERENTIAL I/O
QSFP_TX_p[2] | BA129 | output | HIGH SPEED DIFFERENTIAL I/O
QSFP_TX_p[3] | AW129 | output | HIGH SPEED DIFFERENTIAL I/O
QSFP_TX_n[0] | BE126 | output | HIGH SPEED DIFFERENTIAL I/O
QSFP_TX_n[1] | BC126 | output | HIGH SPEED DIFFERENTIAL I/O
QSFP_TX_n[2] | BA126 | output | HIGH SPEED DIFFERENTIAL I/O
QSFP_TX_n[3] | AW126 | output | HIGH SPEED DIFFERENTIAL I/O
QSFP_RX_p[0] | BD135 | input | HIGH SPEED DIFFERENTIAL I/O
QSFP_RX_p[1] | BB135 | input | HIGH SPEED DIFFERENTIAL I/O
QSFP_RX_p[2] | AY135 | input | HIGH SPEED DIFFERENTIAL I/O
QSFP_RX_p[3] | AV135 | input | HIGH SPEED DIFFERENTIAL I/O
QSFP_RX_n[0] | BD133 | input | HIGH SPEED DIFFERENTIAL I/O
QSFP_RX_n[1] | BB133 | input | HIGH SPEED DIFFERENTIAL I/O
QSFP_RX_n[2] | AY133 | input | HIGH SPEED DIFFERENTIAL I/O
QSFP_RX_n[3] | AV133 | input | HIGH SPEED DIFFERENTIAL I/O
CIPRI_REFCLK_p | AY120 | input | CURRENT MODE LOGIC (CML)
QSFP_REFCLK_p | AV120 | input | CURRENT MODE LOGIC (CML)
QSFP_INTERRUPT_n | A39 | input | 3.3-V LVCMOS
QSFP_LP_MODE | A33 | output | 3.3-V LVCMOS
QSFP_MOD_PRS_n | B35 | input | 3.3-V LVCMOS
QSFP_MOD_SEL_n | B26 | output | 3.3-V LVCMOS
QSFP_RST_n | B30 | output | 3.3-V LVCMOS
QSFP_SCL | A30 | inout | 3.3-V LVCMOS
QSFP_SDA | A35 | inout | 3.3-V LVCMOS

##

CAM
Name | Location | Direction | IO Standard
--- | --- | --- | ---
CAM_RZQ | BR52 | input | 1.2 V

##

CAM1
Name | Location | Direction | IO Standard
--- | --- | --- | ---
CAM1_CLK_p | CK17 | input | DPHY
CAM1_CLK_n | CL17 | input | DPHY
CAM1_D_p[0] | CL23 | input | DPHY
CAM1_D_p[1] | CL20 | input | DPHY
CAM1_D_n[0] | CK26 | input | DPHY
CAM1_D_n[1] | CK20 | input | DPHY
CAM1_I2C_SCL | J2 | inout | 3.3-V LVCMOS
CAM1_I2C_SDA | G2 | inout | 3.3-V LVCMOS
CAM1_GPIO | K4 | inout | 3.3-V LVCMOS

##

CAM2
Name | Location | Direction | IO Standard
--- | --- | --- | ---
CAM2_CLK_p | CF28 | input | DPHY
CAM2_CLK_n | CC28 | input | DPHY
CAM2_D_p[0] | CH31 | input | DPHY
CAM2_D_p[1] | CA31 | input | DPHY
CAM2_D_n[0] | CF31 | input | DPHY
CAM2_D_n[1] | CC31 | input | DPHY
CAM2_I2C_SCL | A8 | inout | 3.3-V LVCMOS
CAM2_I2C_SDA | G1 | inout | 3.3-V LVCMOS
CAM2_GPIO | J1 | inout | 3.3-V LVCMOS

##

HPS
Name | Location | Direction | IO Standard
--- | --- | --- | ---
HPS_ENET_MDC | AG115 | output | 1.8 V
HPS_ENET_MDIO | R134 | inout | 1.8 V
HPS_ENET_RX_CLK | M124 | input | 1.8 V
HPS_ENET_RX_CTL | AB127 | input | 1.8 V
HPS_ENET_RX_DATA[0] | H127 | input | 1.8 V
HPS_ENET_RX_DATA[1] | AB124 | input | 1.8 V
HPS_ENET_RX_DATA[2] | F124 | input | 1.8 V
HPS_ENET_RX_DATA[3] | D124 | input | 1.8 V
HPS_ENET_TX_CLK | M127 | output | 1.8 V
HPS_ENET_TX_CTL | K127 | output | 1.8 V
HPS_ENET_TX_DATA[0] | K124 | output | 1.8 V
HPS_ENET_TX_DATA[1] | Y127 | output | 1.8 V
HPS_ENET_TX_DATA[2] | F127 | output | 1.8 V
HPS_ENET_TX_DATA[3] | Y124 | output | 1.8 V
HPS_GPIO[0] | U135 | inout | 1.8 V
HPS_GPIO[1] | W135 | inout | 1.8 V
HPS_GPIO[2] | N135 | inout | 1.8 V
HPS_GPIO[3] | AK120 | inout | 1.8 V
HPS_GPIO[4] | T132 | inout | 1.8 V
HPS_I2C_SCL | AL120 | inout | 1.8 V
HPS_I2C_SDA | U134 | inout | 1.8 V
HPS_KEY | B134 | inout | 1.8 V
HPS_LED | AG123 | inout | 1.8 V
HPS_OSC_CLK | N134 | input | 1.8 V
HPS_SDMMC_CLK | D132 | output | 1.8 V
HPS_SDMMC_CMD | AB132 | inout | 1.8 V
HPS_SDMMC_DATA[0] | E135 | inout | 1.8 V
HPS_SDMMC_DATA[1] | F132 | inout | 1.8 V
HPS_SDMMC_DATA[2] | AA135 | inout | 1.8 V
HPS_SDMMC_DATA[3] | V127 | inout | 1.8 V
HPS_SDMMC_DATA[4] | T127 | inout | 1.8 V
HPS_SDMMC_DATA[5] | Y132 | inout | 1.8 V
HPS_SDMMC_DATA[6] | T124 | inout | 1.8 V
HPS_SDMMC_DATA[7] | P124 | inout | 1.8 V
HPS_UART_RX | AK115 | input | 1.8 V
HPS_UART_TX | W134 | output | 1.8 V
HPS_USB3_REFCLK_100M_p | AP120 | input | CURRENT MODE LOGIC (CML)
HPS_USB3_SS_RX_n | AM133 | input | HIGH SPEED DIFFERENTIAL I/O
HPS_USB3_SS_RX_p | AM135 | input | HIGH SPEED DIFFERENTIAL I/O
HPS_USB3_SS_TX_n | AN126 | output | HIGH SPEED DIFFERENTIAL I/O
HPS_USB3_SS_TX_p | AN129 | output | HIGH SPEED DIFFERENTIAL I/O
HPS_USB_CLK | P132 | input | 1.8 V
HPS_USB_DATA[0] | AD135 | inout | 1.8 V
HPS_USB_DATA[1] | M132 | inout | 1.8 V
HPS_USB_DATA[2] | K132 | inout | 1.8 V
HPS_USB_DATA[3] | AG129 | inout | 1.8 V
HPS_USB_DATA[4] | J134 | inout | 1.8 V
HPS_USB_DATA[5] | AG120 | inout | 1.8 V
HPS_USB_DATA[6] | G134 | inout | 1.8 V
HPS_USB_DATA[7] | G135 | inout | 1.8 V
HPS_USB_DIR | J135 | input | 1.8 V
HPS_USB_ID | A60 | input | 1.2 V
HPS_USB_NXT | AD134 | input | 1.8 V
HPS_USB_STP | L135 | output | 1.8 V
HPS_USB_VBUS_CTRL | A63 | output | 1.2 V
HPS_USB_VBUS_DET | B60 | input | 1.2 V
HPS_USB_VBUS_FLT_n | B56 | input | 1.2 V

##

INFO
Name | Location | Direction | IO Standard
--- | --- | --- | ---
INFO_SPI_SCLK | A17 | output | 3.3-V LVCMOS
INFO_SPI_MISO | B23 | input | 3.3-V LVCMOS
INFO_SPI_MOSI | B20 | output | 3.3-V LVCMOS
INFO_SPI_CS_n | A23 | output | 3.3-V LVCMOS