## AG27 Board Configuration

www.terasic.com
Copyright © 2003-2022 Terasic Inc. All Rights Reserved.

### Pin Assignments:

##

CLOCK
Name | Location | Direction | IO Standard
--- | --- | --- | ---
CLK_100_B2B_p | LB60 | input | True Differential Signaling
CLK_30M72 | KJ27 | input | 1.2 V
CLK_50_B3B | U51 | input | 1.2 V
CLK_50_B3C | N45 | input | 1.2 V
CLK_FROM_SI5397A_p[0] | KC31 | input | True Differential Signaling
CLK_FROM_SI5397A_p[1] | J41 | input | True Differential Signaling
CLK_TO_SI5397A_p[0] | KF28 | output | DIFFERENTIAL 1.2-V POD
CLK_TO_SI5397A_p[1] | KU30 | output | DIFFERENTIAL 1.2-V POD
UFL_CLKIN | KU56 | input | 1.2 V

##

Buttons
Name | Location | Direction | IO Standard
--- | --- | --- | ---
CPU_RESET_n | B47 | input | 1.2 V
BUTTON[0] | U47 | input | 1.2 V
BUTTON[1] | N47 | input | 1.2 V

##

Swtiches
Name | Location | Direction | IO Standard
--- | --- | --- | ---
SW[0] | L48 | input | 1.2 V
SW[1] | W48 | input | 1.2 V

##

LED
Name | Location | Direction | IO Standard
--- | --- | --- | ---
LED_BRACKET[0] | N49 | output | 1.2 V
LED_BRACKET[1] | L52 | output | 1.2 V
LED_BRACKET[2] | L50 | output | 1.2 V
LED_BRACKET[3] | U49 | output | 1.2 V
LED[0] | H48 | output | 1.2 V
LED[1] | J47 | output | 1.2 V
LED[2] | W50 | output | 1.2 V
LED[3] | N51 | output | 1.2 V

##

DDR4 I2C
Name | Location | Direction | IO Standard
--- | --- | --- | ---
DDR4_SCL | W46 | inout | 1.2 V
DDR4_SDA | W42 | inout | 1.2 V

##

QSFPDD Reserved Clock
Name | Location | Direction | IO Standard
--- | --- | --- | ---
QSFPDDRSV_REFCLK_p | HL74 | input | CURRENT MODE LOGIC (CML)

##

DDR4A
Name | Location | Direction | IO Standard
--- | --- | --- | ---
DDR4A_REFCLK_p | AA31 | input | True Differential Signaling
DDR4A_A[0] | N33 | output | SSTL-12
DDR4A_A[1] | L34 | output | SSTL-12
DDR4A_A[2] | U33 | output | SSTL-12
DDR4A_A[3] | W34 | output | SSTL-12
DDR4A_A[4] | N31 | output | SSTL-12
DDR4A_A[5] | L32 | output | SSTL-12
DDR4A_A[6] | U31 | output | SSTL-12
DDR4A_A[7] | W32 | output | SSTL-12
DDR4A_A[8] | N29 | output | SSTL-12
DDR4A_A[9] | L30 | output | SSTL-12
DDR4A_A[10] | U29 | output | SSTL-12
DDR4A_A[11] | W30 | output | SSTL-12
DDR4A_A[12] | AK32 | output | SSTL-12
DDR4A_A[13] | AA29 | output | SSTL-12
DDR4A_A[14] | AD30 | output | SSTL-12
DDR4A_A[15] | AN29 | output | SSTL-12
DDR4A_A[16] | AK30 | output | SSTL-12
DDR4A_BA[0] | AD28 | output | SSTL-12
DDR4A_BA[1] | AN27 | output | SSTL-12
DDR4A_BG[0] | AK28 | output | SSTL-12
DDR4A_BG[1] | AV37 | output | SSTL-12
DDR4A_CK | AV33 | output | DIFFERENTIAL 1.2-V SSTL
DDR4A_CK_n | AT34 | output | DIFFERENTIAL 1.2-V SSTL
DDR4A_CKE | BC35 | output | SSTL-12
DDR4A_DQS[0] | N5 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS[1] | B13 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS[2] | B25 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS[3] | B31 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS[4] | N37 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS[5] | AA41 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS[6] | AV41 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS[7] | AA35 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS[8] | AV29 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS_n[0] | L7 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS_n[1] | D15 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS_n[2] | D26 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS_n[3] | D32 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS_n[4] | L38 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS_n[5] | AD42 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS_n[6] | AT42 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS_n[7] | AD36 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQS_n[8] | AT30 | inout | DIFFERENTIAL 1.2-V POD
DDR4A_DQ[0] | W4 | inout | 1.2-V POD
DDR4A_DQ[1] | L4 | inout | 1.2-V POD
DDR4A_DQ[2] | U9 | inout | 1.2-V POD
DDR4A_DQ[3] | W11 | inout | 1.2-V POD
DDR4A_DQ[4] | U2 | inout | 1.2-V POD
DDR4A_DQ[5] | N2 | inout | 1.2-V POD
DDR4A_DQ[6] | N9 | inout | 1.2-V POD
DDR4A_DQ[7] | L11 | inout | 1.2-V POD
DDR4A_DQ[8] | H11 | inout | 1.2-V POD
DDR4A_DQ[9] | D11 | inout | 1.2-V POD
DDR4A_DQ[10] | B17 | inout | 1.2-V POD
DDR4A_DQ[11] | H19 | inout | 1.2-V POD
DDR4A_DQ[12] | H7 | inout | 1.2-V POD
DDR4A_DQ[13] | J9 | inout | 1.2-V POD
DDR4A_DQ[14] | D19 | inout | 1.2-V POD
DDR4A_DQ[15] | J17 | inout | 1.2-V POD
DDR4A_DQ[16] | B21 | inout | 1.2-V POD
DDR4A_DQ[17] | D23 | inout | 1.2-V POD
DDR4A_DQ[18] | D28 | inout | 1.2-V POD
DDR4A_DQ[19] | B27 | inout | 1.2-V POD
DDR4A_DQ[20] | J21 | inout | 1.2-V POD
DDR4A_DQ[21] | H23 | inout | 1.2-V POD
DDR4A_DQ[22] | H28 | inout | 1.2-V POD
DDR4A_DQ[23] | J27 | inout | 1.2-V POD
DDR4A_DQ[24] | B29 | inout | 1.2-V POD
DDR4A_DQ[25] | D30 | inout | 1.2-V POD
DDR4A_DQ[26] | J33 | inout | 1.2-V POD
DDR4A_DQ[27] | D34 | inout | 1.2-V POD
DDR4A_DQ[28] | H30 | inout | 1.2-V POD
DDR4A_DQ[29] | J29 | inout | 1.2-V POD
DDR4A_DQ[30] | B33 | inout | 1.2-V POD
DDR4A_DQ[31] | H34 | inout | 1.2-V POD
DDR4A_DQ[32] | N35 | inout | 1.2-V POD
DDR4A_DQ[33] | L40 | inout | 1.2-V POD
DDR4A_DQ[34] | U39 | inout | 1.2-V POD
DDR4A_DQ[35] | W40 | inout | 1.2-V POD
DDR4A_DQ[36] | U35 | inout | 1.2-V POD
DDR4A_DQ[37] | W36 | inout | 1.2-V POD
DDR4A_DQ[38] | N39 | inout | 1.2-V POD
DDR4A_DQ[39] | L36 | inout | 1.2-V POD
DDR4A_DQ[40] | AA43 | inout | 1.2-V POD
DDR4A_DQ[41] | AA39 | inout | 1.2-V POD
DDR4A_DQ[42] | AK40 | inout | 1.2-V POD
DDR4A_DQ[43] | AK44 | inout | 1.2-V POD
DDR4A_DQ[44] | AD40 | inout | 1.2-V POD
DDR4A_DQ[45] | AN39 | inout | 1.2-V POD
DDR4A_DQ[46] | AN43 | inout | 1.2-V POD
DDR4A_DQ[47] | AD44 | inout | 1.2-V POD
DDR4A_DQ[48] | AV43 | inout | 1.2-V POD
DDR4A_DQ[49] | AT44 | inout | 1.2-V POD
DDR4A_DQ[50] | BC39 | inout | 1.2-V POD
DDR4A_DQ[51] | BC43 | inout | 1.2-V POD
DDR4A_DQ[52] | AV39 | inout | 1.2-V POD
DDR4A_DQ[53] | AT40 | inout | 1.2-V POD
DDR4A_DQ[54] | BF40 | inout | 1.2-V POD
DDR4A_DQ[55] | BF44 | inout | 1.2-V POD
DDR4A_DQ[56] | AD34 | inout | 1.2-V POD
DDR4A_DQ[57] | AA37 | inout | 1.2-V POD
DDR4A_DQ[58] | AN33 | inout | 1.2-V POD
DDR4A_DQ[59] | AK34 | inout | 1.2-V POD
DDR4A_DQ[60] | AD38 | inout | 1.2-V POD
DDR4A_DQ[61] | AN37 | inout | 1.2-V POD
DDR4A_DQ[62] | AA33 | inout | 1.2-V POD
DDR4A_DQ[63] | AK38 | inout | 1.2-V POD
DDR4A_DQ[64] | BF28 | inout | 1.2-V POD
DDR4A_DQ[65] | BF32 | inout | 1.2-V POD
DDR4A_DQ[66] | AT32 | inout | 1.2-V POD
DDR4A_DQ[67] | AT28 | inout | 1.2-V POD
DDR4A_DQ[68] | BC31 | inout | 1.2-V POD
DDR4A_DQ[69] | AV31 | inout | 1.2-V POD
DDR4A_DQ[70] | BC27 | inout | 1.2-V POD
DDR4A_DQ[71] | AV27 | inout | 1.2-V POD
DDR4A_DBI_n[0] | U5 | inout | 1.2-V POD
DDR4A_DBI_n[1] | J13 | inout | 1.2-V POD
DDR4A_DBI_n[2] | J25 | inout | 1.2-V POD
DDR4A_DBI_n[3] | J31 | inout | 1.2-V POD
DDR4A_DBI_n[4] | U37 | inout | 1.2-V POD
DDR4A_DBI_n[5] | AN41 | inout | 1.2-V POD
DDR4A_DBI_n[6] | BC41 | inout | 1.2-V POD
DDR4A_DBI_n[7] | AN35 | inout | 1.2-V POD
DDR4A_DBI_n[8] | BC29 | inout | 1.2-V POD
DDR4A_CS_n | BC37 | output | SSTL-12
DDR4A_RESET_n | AT38 | output | 1.2 V
DDR4A_ODT | AV35 | output | SSTL-12
DDR4A_PAR | BF34 | output | SSTL-12
DDR4A_ALERT_n | AA27 | input | 1.2 V
DDR4A_ACT_n | BF38 | output | SSTL-12
DDR4A_EVENT_n | N41 | input | 1.2 V
DDR4A_RZQ | AN31 | input | 1.2 V

##

DDR4B
Name | Location | Direction | IO Standard
--- | --- | --- | ---
DDR4B_REFCLK_p | AG63 | input | True Differential Signaling
DDR4B_A[0] | N59 | output | SSTL-12
DDR4B_A[1] | L60 | output | SSTL-12
DDR4B_A[2] | U59 | output | SSTL-12
DDR4B_A[3] | W60 | output | SSTL-12
DDR4B_A[4] | N61 | output | SSTL-12
DDR4B_A[5] | L62 | output | SSTL-12
DDR4B_A[6] | U61 | output | SSTL-12
DDR4B_A[7] | W62 | output | SSTL-12
DDR4B_A[8] | N63 | output | SSTL-12
DDR4B_A[9] | L64 | output | SSTL-12
DDR4B_A[10] | U63 | output | SSTL-12
DDR4B_A[11] | W64 | output | SSTL-12
DDR4B_A[12] | AT64 | output | SSTL-12
DDR4B_A[13] | AG65 | output | SSTL-12
DDR4B_A[14] | AK66 | output | SSTL-12
DDR4B_A[15] | AV65 | output | SSTL-12
DDR4B_A[16] | AT66 | output | SSTL-12
DDR4B_BA[0] | AK70 | output | SSTL-12
DDR4B_BA[1] | AV68 | output | SSTL-12
DDR4B_BG[0] | AT70 | output | SSTL-12
DDR4B_BG[1] | B59 | output | SSTL-12
DDR4B_CK[0] | B63 | output | DIFFERENTIAL 1.2-V SSTL
DDR4B_CK[1] | BJ68 | output | DIFFERENTIAL 1.2-V SSTL
DDR4B_CK_n[0] | D64 | output | DIFFERENTIAL 1.2-V SSTL
DDR4B_CK_n[1] | BM70 | output | DIFFERENTIAL 1.2-V SSTL
DDR4B_CKE[0] | J61 | output | SSTL-12
DDR4B_CKE[1] | H62 | output | SSTL-12
DDR4B_DQS[0] | AV47 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS[1] | AA53 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS[2] | AV53 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS[3] | AA47 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS[4] | N55 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS[5] | AA59 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS[6] | BJ59 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS[7] | AV59 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS[8] | B55 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS_n[0] | AT48 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS_n[1] | AD54 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS_n[2] | AT54 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS_n[3] | AD48 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS_n[4] | L56 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS_n[5] | AD60 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS_n[6] | BM60 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS_n[7] | AT60 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQS_n[8] | D56 | inout | DIFFERENTIAL 1.2-V POD
DDR4B_DQ[0] | BF50 | inout | 1.2-V POD
DDR4B_DQ[1] | BC49 | inout | 1.2-V POD
DDR4B_DQ[2] | AV45 | inout | 1.2-V POD
DDR4B_DQ[3] | AT46 | inout | 1.2-V POD
DDR4B_DQ[4] | AT50 | inout | 1.2-V POD
DDR4B_DQ[5] | AV49 | inout | 1.2-V POD
DDR4B_DQ[6] | BC45 | inout | 1.2-V POD
DDR4B_DQ[7] | BF46 | inout | 1.2-V POD
DDR4B_DQ[8] | AA51 | inout | 1.2-V POD
DDR4B_DQ[9] | AK52 | inout | 1.2-V POD
DDR4B_DQ[10] | AK56 | inout | 1.2-V POD
DDR4B_DQ[11] | AD56 | inout | 1.2-V POD
DDR4B_DQ[12] | AN51 | inout | 1.2-V POD
DDR4B_DQ[13] | AN55 | inout | 1.2-V POD
DDR4B_DQ[14] | AA55 | inout | 1.2-V POD
DDR4B_DQ[15] | AD52 | inout | 1.2-V POD
DDR4B_DQ[16] | BC51 | inout | 1.2-V POD
DDR4B_DQ[17] | AV51 | inout | 1.2-V POD
DDR4B_DQ[18] | AT56 | inout | 1.2-V POD
DDR4B_DQ[19] | AV55 | inout | 1.2-V POD
DDR4B_DQ[20] | BC55 | inout | 1.2-V POD
DDR4B_DQ[21] | BF52 | inout | 1.2-V POD
DDR4B_DQ[22] | BF56 | inout | 1.2-V POD
DDR4B_DQ[23] | AT52 | inout | 1.2-V POD
DDR4B_DQ[24] | AK50 | inout | 1.2-V POD
DDR4B_DQ[25] | AK46 | inout | 1.2-V POD
DDR4B_DQ[26] | AA45 | inout | 1.2-V POD
DDR4B_DQ[27] | AA49 | inout | 1.2-V POD
DDR4B_DQ[28] | AD46 | inout | 1.2-V POD
DDR4B_DQ[29] | AN45 | inout | 1.2-V POD
DDR4B_DQ[30] | AN49 | inout | 1.2-V POD
DDR4B_DQ[31] | AD50 | inout | 1.2-V POD
DDR4B_DQ[32] | N53 | inout | 1.2-V POD
DDR4B_DQ[33] | L54 | inout | 1.2-V POD
DDR4B_DQ[34] | U57 | inout | 1.2-V POD
DDR4B_DQ[35] | W58 | inout | 1.2-V POD
DDR4B_DQ[36] | U53 | inout | 1.2-V POD
DDR4B_DQ[37] | W54 | inout | 1.2-V POD
DDR4B_DQ[38] | N57 | inout | 1.2-V POD
DDR4B_DQ[39] | L58 | inout | 1.2-V POD
DDR4B_DQ[40] | AK58 | inout | 1.2-V POD
DDR4B_DQ[41] | AA57 | inout | 1.2-V POD
DDR4B_DQ[42] | AN61 | inout | 1.2-V POD
DDR4B_DQ[43] | AN57 | inout | 1.2-V POD
DDR4B_DQ[44] | AA61 | inout | 1.2-V POD
DDR4B_DQ[45] | AD58 | inout | 1.2-V POD
DDR4B_DQ[46] | AD62 | inout | 1.2-V POD
DDR4B_DQ[47] | AK62 | inout | 1.2-V POD
DDR4B_DQ[48] | BV62 | inout | 1.2-V POD
DDR4B_DQ[49] | CA61 | inout | 1.2-V POD
DDR4B_DQ[50] | CA57 | inout | 1.2-V POD
DDR4B_DQ[51] | BV58 | inout | 1.2-V POD
DDR4B_DQ[52] | BM62 | inout | 1.2-V POD
DDR4B_DQ[53] | BJ61 | inout | 1.2-V POD
DDR4B_DQ[54] | BJ57 | inout | 1.2-V POD
DDR4B_DQ[55] | BM58 | inout | 1.2-V POD
DDR4B_DQ[56] | BC61 | inout | 1.2-V POD
DDR4B_DQ[57] | AV61 | inout | 1.2-V POD
DDR4B_DQ[58] | BF58 | inout | 1.2-V POD
DDR4B_DQ[59] | AV57 | inout | 1.2-V POD
DDR4B_DQ[60] | BF62 | inout | 1.2-V POD
DDR4B_DQ[61] | AT62 | inout | 1.2-V POD
DDR4B_DQ[62] | BC57 | inout | 1.2-V POD
DDR4B_DQ[63] | AT58 | inout | 1.2-V POD
DDR4B_DQ[64] | B57 | inout | 1.2-V POD
DDR4B_DQ[65] | B53 | inout | 1.2-V POD
DDR4B_DQ[66] | D54 | inout | 1.2-V POD
DDR4B_DQ[67] | J57 | inout | 1.2-V POD
DDR4B_DQ[68] | H54 | inout | 1.2-V POD
DDR4B_DQ[69] | J53 | inout | 1.2-V POD
DDR4B_DQ[70] | H58 | inout | 1.2-V POD
DDR4B_DQ[71] | D58 | inout | 1.2-V POD
DDR4B_DBI_n[0] | BC47 | inout | 1.2-V POD
DDR4B_DBI_n[1] | AN53 | inout | 1.2-V POD
DDR4B_DBI_n[2] | BC53 | inout | 1.2-V POD
DDR4B_DBI_n[3] | AN47 | inout | 1.2-V POD
DDR4B_DBI_n[4] | U55 | inout | 1.2-V POD
DDR4B_DBI_n[5] | AN59 | inout | 1.2-V POD
DDR4B_DBI_n[6] | CA59 | inout | 1.2-V POD
DDR4B_DBI_n[7] | BC59 | inout | 1.2-V POD
DDR4B_DBI_n[8] | J55 | inout | 1.2-V POD
DDR4B_CS_n[0] | J59 | output | SSTL-12
DDR4B_CS_n[1] | J63 | output | SSTL-12
DDR4B_RESET_n | D60 | output | 1.2 V
DDR4B_ODT[0] | B61 | output | SSTL-12
DDR4B_ODT[1] | D62 | output | SSTL-12
DDR4B_PAR | H64 | output | SSTL-12
DDR4B_ALERT_n | AG68 | input | 1.2 V
DDR4B_ACT_n | H60 | output | SSTL-12
DDR4B_EVENT_n | H52 | input | 1.2 V
DDR4B_C[0] | BC63 | output | SSTL-12
DDR4B_C[1] | AY64 | output | SSTL-12
DDR4B_RZQ | AV63 | input | 1.2 V

##

DDR4C
Name | Location | Direction | IO Standard
--- | --- | --- | ---
DDR4C_REFCLK_p | KU36 | input | True Differential Signaling
DDR4C_A[0] | LH42 | output | SSTL-12
DDR4C_A[1] | LL43 | output | SSTL-12
DDR4C_A[2] | KW43 | output | SSTL-12
DDR4C_A[3] | LB42 | output | SSTL-12
DDR4C_A[4] | LH40 | output | SSTL-12
DDR4C_A[5] | LL41 | output | SSTL-12
DDR4C_A[6] | LB40 | output | SSTL-12
DDR4C_A[7] | KW41 | output | SSTL-12
DDR4C_A[8] | LH38 | output | SSTL-12
DDR4C_A[9] | LL39 | output | SSTL-12
DDR4C_A[10] | KW39 | output | SSTL-12
DDR4C_A[11] | LB38 | output | SSTL-12
DDR4C_A[12] | KF36 | output | SSTL-12
DDR4C_A[13] | KU34 | output | SSTL-12
DDR4C_A[14] | KR35 | output | SSTL-12
DDR4C_A[15] | KF34 | output | SSTL-12
DDR4C_A[16] | KJ35 | output | SSTL-12
DDR4C_BA[0] | KR33 | output | SSTL-12
DDR4C_BA[1] | KJ33 | output | SSTL-12
DDR4C_BG[0] | KF32 | output | SSTL-12
DDR4C_BG[1] | KR43 | output | SSTL-12
DDR4C_CK[0] | KR39 | output | DIFFERENTIAL 1.2-V SSTL
DDR4C_CK[1] | JP32 | output | DIFFERENTIAL 1.2-V SSTL
DDR4C_CK_n[0] | KU38 | output | DIFFERENTIAL 1.2-V SSTL
DDR4C_CK_n[1] | JL33 | output | DIFFERENTIAL 1.2-V SSTL
DDR4C_CKE[0] | KF40 | output | SSTL-12
DDR4C_CKE[1] | KJ41 | output | SSTL-12
DDR4C_DQS[0] | LH34 | inout | DIFFERENTIAL 1.2-V POD
DDR4C_DQS[1] | MH30 | inout | DIFFERENTIAL 1.2-V POD
DDR4C_DQS[2] | MH11 | inout | DIFFERENTIAL 1.2-V POD
DDR4C_DQS[3] | LW17 | inout | DIFFERENTIAL 1.2-V POD
DDR4C_DQS[4] | LW33 | inout | DIFFERENTIAL 1.2-V POD
DDR4C_DQS[5] | MH23 | inout | DIFFERENTIAL 1.2-V POD
DDR4C_DQS[6] | LW5 | inout | DIFFERENTIAL 1.2-V POD
DDR4C_DQS[7] | LW27 | inout | DIFFERENTIAL 1.2-V POD
DDR4C_DQS[8] | LH28 | inout | DIFFERENTIAL 1.2-V POD
DDR4C_DQS_n[0] | LL35 | inout | DIFFERENTIAL 1.2-V POD
DDR4C_DQS_n[1] | MK31 | inout | DIFFERENTIAL 1.2-V POD
DDR4C_DQS_n[2] | MK13 | inout | DIFFERENTIAL 1.2-V POD
DDR4C_DQS_n[3] | MA19 | inout | DIFFERENTIAL 1.2-V POD
DDR4C_DQS_n[4] | MA34 | inout | DIFFERENTIAL 1.2-V POD
DDR4C_DQS_n[5] | MK25 | inout | DIFFERENTIAL 1.2-V POD
DDR4C_DQS_n[6] | MA7 | inout | DIFFERENTIAL 1.2-V POD
DDR4C_DQS_n[7] | MA28 | inout | DIFFERENTIAL 1.2-V POD
DDR4C_DQS_n[8] | LL29 | inout | DIFFERENTIAL 1.2-V POD
DDR4C_DQ[0] | LB32 | inout | 1.2-V POD
DDR4C_DQ[1] | LB36 | inout | 1.2-V POD
DDR4C_DQ[2] | LL33 | inout | 1.2-V POD
DDR4C_DQ[3] | LH32 | inout | 1.2-V POD
DDR4C_DQ[4] | KW33 | inout | 1.2-V POD
DDR4C_DQ[5] | KW37 | inout | 1.2-V POD
DDR4C_DQ[6] | LL37 | inout | 1.2-V POD
DDR4C_DQ[7] | LH36 | inout | 1.2-V POD
DDR4C_DQ[8] | MK29 | inout | 1.2-V POD
DDR4C_DQ[9] | MD32 | inout | 1.2-V POD
DDR4C_DQ[10] | MC33 | inout | 1.2-V POD
DDR4C_DQ[11] | MD28 | inout | 1.2-V POD
DDR4C_DQ[12] | MC29 | inout | 1.2-V POD
DDR4C_DQ[13] | MK33 | inout | 1.2-V POD
DDR4C_DQ[14] | MH28 | inout | 1.2-V POD
DDR4C_DQ[15] | MH32 | inout | 1.2-V POD
DDR4C_DQ[16] | MD7 | inout | 1.2-V POD
DDR4C_DQ[17] | MC17 | inout | 1.2-V POD
DDR4C_DQ[18] | MC9 | inout | 1.2-V POD
DDR4C_DQ[19] | MD15 | inout | 1.2-V POD
DDR4C_DQ[20] | MF5 | inout | 1.2-V POD
DDR4C_DQ[21] | MH15 | inout | 1.2-V POD
DDR4C_DQ[22] | MH7 | inout | 1.2-V POD
DDR4C_DQ[23] | MK17 | inout | 1.2-V POD
DDR4C_DQ[24] | MA15 | inout | 1.2-V POD
DDR4C_DQ[25] | MA23 | inout | 1.2-V POD
DDR4C_DQ[26] | LN15 | inout | 1.2-V POD
DDR4C_DQ[27] | LR21 | inout | 1.2-V POD
DDR4C_DQ[28] | LR13 | inout | 1.2-V POD
DDR4C_DQ[29] | LW13 | inout | 1.2-V POD
DDR4C_DQ[30] | LN23 | inout | 1.2-V POD
DDR4C_DQ[31] | LW21 | inout | 1.2-V POD
DDR4C_DQ[32] | MA36 | inout | 1.2-V POD
DDR4C_DQ[33] | LW35 | inout | 1.2-V POD
DDR4C_DQ[34] | LW31 | inout | 1.2-V POD
DDR4C_DQ[35] | LR31 | inout | 1.2-V POD
DDR4C_DQ[36] | LR35 | inout | 1.2-V POD
DDR4C_DQ[37] | LN36 | inout | 1.2-V POD
DDR4C_DQ[38] | MA32 | inout | 1.2-V POD
DDR4C_DQ[39] | LN32 | inout | 1.2-V POD
DDR4C_DQ[40] | MK21 | inout | 1.2-V POD
DDR4C_DQ[41] | MD26 | inout | 1.2-V POD
DDR4C_DQ[42] | MH19 | inout | 1.2-V POD
DDR4C_DQ[43] | MC21 | inout | 1.2-V POD
DDR4C_DQ[44] | MC27 | inout | 1.2-V POD
DDR4C_DQ[45] | MK27 | inout | 1.2-V POD
DDR4C_DQ[46] | MD19 | inout | 1.2-V POD
DDR4C_DQ[47] | MH26 | inout | 1.2-V POD
DDR4C_DQ[48] | LR9 | inout | 1.2-V POD
DDR4C_DQ[49] | LW9 | inout | 1.2-V POD
DDR4C_DQ[50] | MA4 | inout | 1.2-V POD
DDR4C_DQ[51] | LW2 | inout | 1.2-V POD
DDR4C_DQ[52] | MA11 | inout | 1.2-V POD
DDR4C_DQ[53] | LN11 | inout | 1.2-V POD
DDR4C_DQ[54] | MC5 | inout | 1.2-V POD
DDR4C_DQ[55] | LU4 | inout | 1.2-V POD
DDR4C_DQ[56] | LN26 | inout | 1.2-V POD
DDR4C_DQ[57] | MA26 | inout | 1.2-V POD
DDR4C_DQ[58] | LR29 | inout | 1.2-V POD
DDR4C_DQ[59] | LN30 | inout | 1.2-V POD
DDR4C_DQ[60] | LW25 | inout | 1.2-V POD
DDR4C_DQ[61] | LR25 | inout | 1.2-V POD
DDR4C_DQ[62] | LW29 | inout | 1.2-V POD
DDR4C_DQ[63] | MA30 | inout | 1.2-V POD
DDR4C_DQ[64] | KW27 | inout | 1.2-V POD
DDR4C_DQ[65] | LH30 | inout | 1.2-V POD
DDR4C_DQ[66] | LL31 | inout | 1.2-V POD
DDR4C_DQ[67] | LH26 | inout | 1.2-V POD
DDR4C_DQ[68] | LB26 | inout | 1.2-V POD
DDR4C_DQ[69] | LL27 | inout | 1.2-V POD
DDR4C_DQ[70] | LB30 | inout | 1.2-V POD
DDR4C_DQ[71] | KW31 | inout | 1.2-V POD
DDR4C_DBI_n[0] | LB34 | inout | 1.2-V POD
DDR4C_DBI_n[1] | MD30 | inout | 1.2-V POD
DDR4C_DBI_n[2] | MD11 | inout | 1.2-V POD
DDR4C_DBI_n[3] | LR17 | inout | 1.2-V POD
DDR4C_DBI_n[4] | LR33 | inout | 1.2-V POD
DDR4C_DBI_n[5] | MD23 | inout | 1.2-V POD
DDR4C_DBI_n[6] | LR5 | inout | 1.2-V POD
DDR4C_DBI_n[7] | LR27 | inout | 1.2-V POD
DDR4C_DBI_n[8] | LB28 | inout | 1.2-V POD
DDR4C_CS_n[0] | KF42 | output | SSTL-12
DDR4C_CS_n[1] | KF38 | output | SSTL-12
DDR4C_RESET_n | KU42 | output | 1.2 V
DDR4C_ODT[0] | KU40 | output | SSTL-12
DDR4C_ODT[1] | KR41 | output | SSTL-12
DDR4C_PAR | KJ39 | output | SSTL-12
DDR4C_ALERT_n | KU32 | input | 1.2 V
DDR4C_ACT_n | KJ43 | output | SSTL-12
DDR4C_EVENT_n | JY26 | input | 1.2 V
DDR4C_C[0] | KC37 | output | SSTL-12
DDR4C_C[1] | JY36 | output | SSTL-12
DDR4C_RZQ | KJ37 | input | 1.2 V

##

DDR4D
Name | Location | Direction | IO Standard
--- | --- | --- | ---
DDR4D_REFCLK_p | MA44 | input | True Differential Signaling
DDR4D_A[0] | KR45 | output | SSTL-12
DDR4D_A[1] | KU44 | output | SSTL-12
DDR4D_A[2] | KJ45 | output | SSTL-12
DDR4D_A[3] | KF44 | output | SSTL-12
DDR4D_A[4] | KU46 | output | SSTL-12
DDR4D_A[5] | KR47 | output | SSTL-12
DDR4D_A[6] | KF46 | output | SSTL-12
DDR4D_A[7] | KJ47 | output | SSTL-12
DDR4D_A[8] | KR49 | output | SSTL-12
DDR4D_A[9] | KU48 | output | SSTL-12
DDR4D_A[10] | KF48 | output | SSTL-12
DDR4D_A[11] | KJ49 | output | SSTL-12
DDR4D_A[12] | LR43 | output | SSTL-12
DDR4D_A[13] | LW45 | output | SSTL-12
DDR4D_A[14] | MA46 | output | SSTL-12
DDR4D_A[15] | LR45 | output | SSTL-12
DDR4D_A[16] | LN46 | output | SSTL-12
DDR4D_BA[0] | LW47 | output | SSTL-12
DDR4D_BA[1] | LN48 | output | SSTL-12
DDR4D_BG[0] | LR47 | output | SSTL-12
DDR4D_BG[1] | LH44 | output | SSTL-12
DDR4D_CK[0] | LH48 | output | DIFFERENTIAL 1.2-V SSTL
DDR4D_CK[1] | LR53 | output | DIFFERENTIAL 1.2-V SSTL
DDR4D_CK_n[0] | LL49 | output | DIFFERENTIAL 1.2-V SSTL
DDR4D_CK_n[1] | LN54 | output | DIFFERENTIAL 1.2-V SSTL
DDR4D_CKE[0] | LB46 | output | SSTL-12
DDR4D_CKE[1] | KW47 | output | SSTL-12
DDR4D_DQS[0] | LH52 | inout | DIFFERENTIAL 1.2-V POD
DDR4D_DQS[1] | MH60 | inout | DIFFERENTIAL 1.2-V POD
DDR4D_DQS[2] | MH54 | inout | DIFFERENTIAL 1.2-V POD
DDR4D_DQS[3] | LW57 | inout | DIFFERENTIAL 1.2-V POD
DDR4D_DQS[4] | MH48 | inout | DIFFERENTIAL 1.2-V POD
DDR4D_DQS[5] | MH36 | inout | DIFFERENTIAL 1.2-V POD
DDR4D_DQS[6] | MH42 | inout | DIFFERENTIAL 1.2-V POD
DDR4D_DQS[7] | LW39 | inout | DIFFERENTIAL 1.2-V POD
DDR4D_DQS[8] | KU52 | inout | DIFFERENTIAL 1.2-V POD
DDR4D_DQS_n[0] | LL53 | inout | DIFFERENTIAL 1.2-V POD
DDR4D_DQS_n[1] | MK61 | inout | DIFFERENTIAL 1.2-V POD
DDR4D_DQS_n[2] | MK55 | inout | DIFFERENTIAL 1.2-V POD
DDR4D_DQS_n[3] | MA58 | inout | DIFFERENTIAL 1.2-V POD
DDR4D_DQS_n[4] | MK49 | inout | DIFFERENTIAL 1.2-V POD
DDR4D_DQS_n[5] | MK37 | inout | DIFFERENTIAL 1.2-V POD
DDR4D_DQS_n[6] | MK43 | inout | DIFFERENTIAL 1.2-V POD
DDR4D_DQS_n[7] | MA40 | inout | DIFFERENTIAL 1.2-V POD
DDR4D_DQS_n[8] | KR53 | inout | DIFFERENTIAL 1.2-V POD
DDR4D_DQ[0] | LL55 | inout | 1.2-V POD
DDR4D_DQ[1] | LB54 | inout | 1.2-V POD
DDR4D_DQ[2] | LH50 | inout | 1.2-V POD
DDR4D_DQ[3] | LH54 | inout | 1.2-V POD
DDR4D_DQ[4] | KW51 | inout | 1.2-V POD
DDR4D_DQ[5] | LB50 | inout | 1.2-V POD
DDR4D_DQ[6] | LL51 | inout | 1.2-V POD
DDR4D_DQ[7] | KW55 | inout | 1.2-V POD
DDR4D_DQ[8] | MC63 | inout | 1.2-V POD
DDR4D_DQ[9] | MH62 | inout | 1.2-V POD
DDR4D_DQ[10] | MK59 | inout | 1.2-V POD
DDR4D_DQ[11] | MH58 | inout | 1.2-V POD
DDR4D_DQ[12] | MD62 | inout | 1.2-V POD
DDR4D_DQ[13] | MC59 | inout | 1.2-V POD
DDR4D_DQ[14] | MK63 | inout | 1.2-V POD
DDR4D_DQ[15] | MD58 | inout | 1.2-V POD
DDR4D_DQ[16] | MD56 | inout | 1.2-V POD
DDR4D_DQ[17] | MK57 | inout | 1.2-V POD
DDR4D_DQ[18] | MH52 | inout | 1.2-V POD
DDR4D_DQ[19] | MD52 | inout | 1.2-V POD
DDR4D_DQ[20] | MC57 | inout | 1.2-V POD
DDR4D_DQ[21] | MC53 | inout | 1.2-V POD
DDR4D_DQ[22] | MK53 | inout | 1.2-V POD
DDR4D_DQ[23] | MH56 | inout | 1.2-V POD
DDR4D_DQ[24] | LN60 | inout | 1.2-V POD
DDR4D_DQ[25] | MA60 | inout | 1.2-V POD
DDR4D_DQ[26] | LR55 | inout | 1.2-V POD
DDR4D_DQ[27] | LW55 | inout | 1.2-V POD
DDR4D_DQ[28] | LN56 | inout | 1.2-V POD
DDR4D_DQ[29] | LW59 | inout | 1.2-V POD
DDR4D_DQ[30] | MA56 | inout | 1.2-V POD
DDR4D_DQ[31] | LR59 | inout | 1.2-V POD
DDR4D_DQ[32] | MK51 | inout | 1.2-V POD
DDR4D_DQ[33] | MC47 | inout | 1.2-V POD
DDR4D_DQ[34] | MD46 | inout | 1.2-V POD
DDR4D_DQ[35] | MK47 | inout | 1.2-V POD
DDR4D_DQ[36] | MC51 | inout | 1.2-V POD
DDR4D_DQ[37] | MH50 | inout | 1.2-V POD
DDR4D_DQ[38] | MH46 | inout | 1.2-V POD
DDR4D_DQ[39] | MD50 | inout | 1.2-V POD
DDR4D_DQ[40] | MH34 | inout | 1.2-V POD
DDR4D_DQ[41] | MK39 | inout | 1.2-V POD
DDR4D_DQ[42] | MC35 | inout | 1.2-V POD
DDR4D_DQ[43] | MD38 | inout | 1.2-V POD
DDR4D_DQ[44] | MK35 | inout | 1.2-V POD
DDR4D_DQ[45] | MC39 | inout | 1.2-V POD
DDR4D_DQ[46] | MD34 | inout | 1.2-V POD
DDR4D_DQ[47] | MH38 | inout | 1.2-V POD
DDR4D_DQ[48] | MC45 | inout | 1.2-V POD
DDR4D_DQ[49] | MK41 | inout | 1.2-V POD
DDR4D_DQ[50] | MH40 | inout | 1.2-V POD
DDR4D_DQ[51] | MD40 | inout | 1.2-V POD
DDR4D_DQ[52] | MH44 | inout | 1.2-V POD
DDR4D_DQ[53] | MK45 | inout | 1.2-V POD
DDR4D_DQ[54] | MD44 | inout | 1.2-V POD
DDR4D_DQ[55] | MC41 | inout | 1.2-V POD
DDR4D_DQ[56] | LR37 | inout | 1.2-V POD
DDR4D_DQ[57] | LN42 | inout | 1.2-V POD
DDR4D_DQ[58] | LN38 | inout | 1.2-V POD
DDR4D_DQ[59] | LR41 | inout | 1.2-V POD
DDR4D_DQ[60] | LW37 | inout | 1.2-V POD
DDR4D_DQ[61] | MA38 | inout | 1.2-V POD
DDR4D_DQ[62] | LW41 | inout | 1.2-V POD
DDR4D_DQ[63] | MA42 | inout | 1.2-V POD
DDR4D_DQ[64] | KR55 | inout | 1.2-V POD
DDR4D_DQ[65] | KU54 | inout | 1.2-V POD
DDR4D_DQ[66] | KJ51 | inout | 1.2-V POD
DDR4D_DQ[67] | KF50 | inout | 1.2-V POD
DDR4D_DQ[68] | KJ55 | inout | 1.2-V POD
DDR4D_DQ[69] | KF54 | inout | 1.2-V POD
DDR4D_DQ[70] | KU50 | inout | 1.2-V POD
DDR4D_DQ[71] | KR51 | inout | 1.2-V POD
DDR4D_DBI_n[0] | LB52 | inout | 1.2-V POD
DDR4D_DBI_n[1] | MD60 | inout | 1.2-V POD
DDR4D_DBI_n[2] | MD54 | inout | 1.2-V POD
DDR4D_DBI_n[3] | LR57 | inout | 1.2-V POD
DDR4D_DBI_n[4] | MD48 | inout | 1.2-V POD
DDR4D_DBI_n[5] | MD36 | inout | 1.2-V POD
DDR4D_DBI_n[6] | MD42 | inout | 1.2-V POD
DDR4D_DBI_n[7] | LR39 | inout | 1.2-V POD
DDR4D_DBI_n[8] | KF52 | inout | 1.2-V POD
DDR4D_CS_n[0] | LB44 | output | SSTL-12
DDR4D_CS_n[1] | KW49 | output | SSTL-12
DDR4D_RESET_n | LL45 | output | 1.2 V
DDR4D_ODT[0] | LH46 | output | SSTL-12
DDR4D_ODT[1] | LL47 | output | SSTL-12
DDR4D_PAR | LB48 | output | SSTL-12
DDR4D_ALERT_n | MA48 | input | 1.2 V
DDR4D_ACT_n | KW45 | output | SSTL-12
DDR4D_EVENT_n | KJ61 | input | 1.2 V
DDR4D_C[0] | MA50 | output | SSTL-12
DDR4D_C[1] | LW49 | output | SSTL-12
DDR4D_RZQ | LN44 | input | 1.2 V

##

SI52204
Name | Location | Direction | IO Standard
--- | --- | --- | ---
SI52204_I2C_SCL | B43 | inout | 1.2 V
SI52204_I2C_SDA | L46 | inout | 1.2 V

##

SI5397A
Name | Location | Direction | IO Standard
--- | --- | --- | ---
SI5397A_I2C_SCL | B51 | inout | 1.2 V
SI5397A_I2C_SDA | D48 | inout | 1.2 V
SI5397A_INTR_n | U45 | input | 1.2 V
SI5397A_LOL_A | J43 | input | 1.2 V
SI5397A_LOL_B | D42 | input | 1.2 V
SI5397A_LOL_C | B41 | input | 1.2 V
SI5397A_LOL_D | H44 | input | 1.2 V
SI5397A_LOS_XAXB | D44 | input | 1.2 V
SI5397A_OE_n | D50 | output | 1.2 V
SI5397A_RST_n | J49 | output | 1.2 V

##

GPIO
Name | Location | Direction | IO Standard
--- | --- | --- | ---
GPIO_CLK[0] | KR29 | input | 1.2 V
GPIO_CLK[1] | KF26 | input | 1.2 V
GPIO_P[0] | KU28 | inout | 1.2 V
GPIO_P[1] | JY28 | inout | 1.2 V
GPIO_P[2] | KU26 | inout | 1.2 V
GPIO_P[3] | JP26 | inout | 1.2 V

##

PCIE
Name | Location | Direction | IO Standard
--- | --- | --- | ---
PCIE_TX_p[0] | DL74 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_p[1] | DB77 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_p[2] | CW74 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_p[3] | CJ77 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_p[4] | CF74 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_p[5] | BU77 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_p[6] | BP74 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_p[7] | BE77 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_p[8] | BB74 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_p[9] | AM77 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_p[10] | AJ74 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_p[11] | Y77 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_p[12] | V74 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_p[13] | K74 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_p[14] | C71 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_p[15] | M71 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_n[0] | DH73 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_n[1] | DE76 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_n[2] | CT73 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_n[3] | CM76 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_n[4] | CC73 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_n[5] | BY76 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_n[6] | BL73 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_n[7] | BH76 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_n[8] | AW73 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_n[9] | AR76 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_n[10] | AF73 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_n[11] | AC76 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_n[12] | T73 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_n[13] | G73 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_n[14] | E69 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_TX_n[15] | P69 | output | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_p[0] | DE82 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_p[1] | CW80 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_p[2] | CM82 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_p[3] | CF80 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_p[4] | BY82 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_p[5] | BP80 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_p[6] | BH82 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_p[7] | BB80 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_p[8] | AR82 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_p[9] | AJ80 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_p[10] | AC82 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_p[11] | V80 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_p[12] | P82 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_p[13] | K80 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_p[14] | M77 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_p[15] | C77 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_n[0] | DB83 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_n[1] | CT79 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_n[2] | CJ83 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_n[3] | CC79 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_n[4] | BU83 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_n[5] | BL79 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_n[6] | BE83 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_n[7] | AW79 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_n[8] | AM83 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_n[9] | AF79 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_n[10] | Y83 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_n[11] | T79 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_n[12] | M83 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_n[13] | G79 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_n[14] | P76 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_RX_n[15] | E76 | input | HIGH SPEED DIFFERENTIAL I/O
PCIE_CLKREQ_n | B49 | output | 1.2 V
PCIE_REFCLK_14C_p[0] | DR68 | input | HCSL
PCIE_REFCLK_14C_p[1] | CU68 | input | HCSL
PCIE_PERST_n | CD58 | input | 1.0 V
PCIE_WAKE_n | W52 | output | 1.2 V

##

QSFPDDA
Name | Location | Direction | IO Standard
--- | --- | --- | ---
QSFPDDA_TX_p[0] | MB71 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_TX_p[1] | MJ74 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_TX_p[2] | LY74 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_TX_p[3] | LM74 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_TX_p[4] | LD77 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_TX_p[5] | LA74 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_TX_p[6] | KL77 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_TX_p[7] | KH74 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_TX_n[0] | ME69 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_TX_n[1] | MG73 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_TX_n[2] | LV73 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_TX_n[3] | LK73 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_TX_n[4] | LG76 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_TX_n[5] | KV73 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_TX_n[6] | KP76 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_TX_n[7] | KE73 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_RX_p[0] | MB77 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_RX_p[1] | LP77 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_RX_p[2] | LY80 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_RX_p[3] | LP83 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_RX_p[4] | LM80 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_RX_p[5] | LD83 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_RX_p[6] | LA80 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_RX_p[7] | KL83 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_RX_n[0] | ME76 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_RX_n[1] | LT76 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_RX_n[2] | LV79 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_RX_n[3] | LT82 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_RX_n[4] | LK79 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_RX_n[5] | LG82 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_RX_n[6] | KV79 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_RX_n[7] | KP82 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDA_REFCLK_p | HJ68 | input | CURRENT MODE LOGIC (CML)
QSFPDDA_INITMODE | KR59 | output | 1.2 V
QSFPDDA_INTERRUPT_n | KJ59 | input | 1.2 V
QSFPDDA_MOD_PRS_n | KF56 | input | 1.2 V
QSFPDDA_MOD_SEL_n | LH58 | output | 1.2 V
QSFPDDA_RST_n | KU60 | output | 1.2 V
QSFPDDA_SCL | KR61 | inout | 1.2 V
QSFPDDA_SDA | KU58 | inout | 1.2 V

##

QSFPDDB
Name | Location | Direction | IO Standard
--- | --- | --- | ---
QSFPDDB_TX_p[0] | JW77 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_TX_p[1] | JT74 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_TX_p[2] | JG77 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_TX_p[3] | HP77 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_TX_p[4] | HL80 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_TX_p[5] | HB77 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_TX_p[6] | GW80 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_TX_p[7] | GG78 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_TX_n[0] | KB76 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_TX_n[1] | JN73 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_TX_n[2] | JK76 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_TX_n[3] | HU76 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_TX_n[4] | HH79 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_TX_n[5] | HE76 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_TX_n[6] | GT79 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_TX_n[7] | GK77 | output | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_RX_p[0] | KH80 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_RX_p[1] | JW83 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_RX_p[2] | JT80 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_RX_p[3] | JG83 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_RX_p[4] | JD80 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_RX_p[5] | HP83 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_RX_p[6] | HB83 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_RX_p[7] | GK83 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_RX_n[0] | KE79 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_RX_n[1] | KB82 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_RX_n[2] | JN79 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_RX_n[3] | JK82 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_RX_n[4] | JA79 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_RX_n[5] | HU82 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_RX_n[6] | HE82 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_RX_n[7] | GN82 | input | HIGH SPEED DIFFERENTIAL I/O
QSFPDDB_REFCLK_p | JD74 | input | CURRENT MODE LOGIC (CML)
QSFPDDB_INITMODE | LL59 | output | 1.2 V
QSFPDDB_INTERRUPT_n | LL57 | input | 1.2 V
QSFPDDB_MOD_PRS_n | KW57 | input | 1.2 V
QSFPDDB_MOD_SEL_n | LH56 | output | 1.2 V
QSFPDDB_RST_n | KJ57 | output | 1.2 V
QSFPDDB_SCL | LB58 | inout | 1.2 V
QSFPDDB_SDA | LB56 | inout | 1.2 V

##

CXL
Name | Location | Direction | IO Standard
--- | --- | --- | ---
CXL_SMBCLK | JL31 | inout | 1.2V
CXL_SMBDAT | JP30 | inout | 1.2V
CXL_TX_p[0] | FK20 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_p[1] | FN14 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_p[2] | GB20 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_p[3] | GE14 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_p[4] | GR20 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_p[5] | GV14 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_p[6] | HG20 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_p[7] | HK14 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_p[8] | HW20 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_p[9] | JC14 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_p[10] | JM20 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_p[11] | JR14 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_p[12] | KD20 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_p[13] | KG14 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_p[14] | KT20 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_p[15] | KY14 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_n[0] | FG22 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_n[1] | FT16 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_n[2] | FW22 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_n[3] | GJ16 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_n[4] | GM22 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_n[5] | HA16 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_n[6] | HD22 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_n[7] | HN16 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_n[8] | HT22 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_n[9] | JF16 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_n[10] | JJ22 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_n[11] | JV16 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_n[12] | KA22 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_n[13] | KK16 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_n[14] | KN22 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_TX_n[15] | LC16 | output | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_p[0] | FK8 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_p[1] | FN1 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_p[2] | GB8 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_p[3] | GE1 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_p[4] | GR8 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_p[5] | GV1 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_p[6] | HG8 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_p[7] | HK1 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_p[8] | HW8 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_p[9] | JC1 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_p[10] | JM8 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_p[11] | JR1 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_p[12] | KD8 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_p[13] | KG1 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_p[14] | KT8 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_p[15] | KY1 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_n[0] | FG10 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_n[1] | FT3 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_n[2] | FW10 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_n[3] | GJ3 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_n[4] | GM10 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_n[5] | HA3 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_n[6] | HD10 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_n[7] | HN3 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_n[8] | HT10 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_n[9] | JF3 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_n[10] | JJ10 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_n[11] | JV3 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_n[12] | KA10 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_n[13] | KK3 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_n[14] | KN10 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_RX_n[15] | LC3 | input | HIGH SPEED DIFFERENTIAL I/O
CXL_REFCLK_15A_p[0] | GA27 | input | HCSL
CXL_REFCLK_15A_p[1] | GY26 | input | HCSL
CXL_PERST_n | HY33 | input | 1.2 V
CXL_RST_n | J51 | input | 1.2 V
CXL_SMB_ALERT_n | KF30 | input | 1.2V

##

EXP
Name | Location | Direction | IO Standard
--- | --- | --- | ---
EXP_EN | L44 | input | 1.2 V

##

HPS
Name | Location | Direction | IO Standard
--- | --- | --- | ---
HPS_ENET_MDC | L26 | output | 1.8 V
HPS_ENET_MDIO | BJ31 | inout | 1.8 V
HPS_ENET_RX_CLK | BV30 | input | 1.8 V
HPS_ENET_RX_CTL | CG27 | input | 1.8 V
HPS_ENET_RX_DATA[0] | BV32 | input | 1.8 V
HPS_ENET_RX_DATA[1] | CD26 | input | 1.8 V
HPS_ENET_RX_DATA[2] | BM28 | input | 1.8 V
HPS_ENET_RX_DATA[3] | U13 | input | 1.8 V
HPS_ENET_TX_CLK | CA29 | output | 1.8 V
HPS_ENET_TX_CTL | CN27 | output | 1.8 V
HPS_ENET_TX_DATA[0] | CA31 | output | 1.8 V
HPS_ENET_TX_DATA[1] | J5 | output | 1.8 V
HPS_ENET_TX_DATA[2] | BV26 | output | 1.8 V
HPS_ENET_TX_DATA[3] | D7 | output | 1.8 V
HPS_JTAG_TCK | BM30 | input | 1.8 V
HPS_JTAG_TDI | U21 | input | 1.8 V
HPS_JTAG_TDO | BJ29 | output | 1.8 V
HPS_JTAG_TMS | L19 | input | 1.8 V
HPS_KEY | N13 | inout | 1.8 V
HPS_LED | BJ27 | inout | 1.8 V
HPS_OSC_CLK | U17 | input | 1.8 V
HPS_SD_CLK | N27 | output | 1.8 V
HPS_SD_CMD | N21 | inout | 1.8 V
HPS_SD_DATA[0] | L28 | inout | 1.8 V
HPS_SD_DATA[1] | L23 | inout | 1.8 V
HPS_SD_DATA[2] | U27 | inout | 1.8 V
HPS_SD_DATA[3] | W26 | inout | 1.8 V
HPS_UART_RX | L15 | input | 1.8 V
HPS_UART_TX | BF26 | output | 1.8 V
HPS_USB_CLK | BM34 | input | 1.8 V
HPS_USB_DATA[0] | AE16 | inout | 1.8 V
HPS_USB_DATA[1] | BM26 | inout | 1.8 V
HPS_USB_DATA[2] | CD28 | inout | 1.8 V
HPS_USB_DATA[3] | AB6 | inout | 1.8 V
HPS_USB_DATA[4] | CA27 | inout | 1.8 V
HPS_USB_DATA[5] | AE3 | inout | 1.8 V
HPS_USB_DATA[6] | BV28 | inout | 1.8 V
HPS_USB_DATA[7] | AB1 | inout | 1.8 V
HPS_USB_DIR | BJ33 | input | 1.8 V
HPS_USB_NXT | AB14 | input | 1.8 V
HPS_USB_STP | AB18 | output | 1.8 V

##

INFO
Name | Location | Direction | IO Standard
--- | --- | --- | ---
INFO_SPI_SCLK | B45 | output | 1.2 V
INFO_SPI_MISO | H46 | input | 1.2 V
INFO_SPI_MOSI | J45 | output | 1.2 V
INFO_SPI_CS_n | D46 | output | 1.2 V