system_intel_niosv_g_0 |

2024.04.21.10:25:57 | Datasheet

Overview

Processor
intel_niosv_g Bantam Lake 2.2.0
All Components
intel_niosv_g intel_niosv_g 2.2.0
Memory Map

| intel_niosv_g
instruction_manager | data_manager
intel_niosv_g |  |
timer_sw_agent |  |
dm_agent |  |

## intel_niosv_g

intel_niosv_g v2.2.0

## Parameters
enableFPU | false
hartId | 0
enableDebug | true
enableDebugReset | false
useResetReq | false
resetSlave | intel_onchip_memory.s1
resetOffset | 0
dataCacheSize | 4096
instCacheSize | 4096
itcm1Size | 0
itcm1Base | 0
itcm1InitFile |
itcm2Size | 0
itcm2Base | 0
itcm2InitFile |
dtcm1Size | 0
dtcm1Base | 0
dtcm1InitFile |
dtcm2Size | 0
dtcm2Base | 0
dtcm2InitFile |
peripheralRegionASize | 65536
peripheralRegionABase | 0
peripheralRegionBSize | 0
peripheralRegionBBase | 0
enableECCLite | false
CUSTOM_OP |
SUB_OP |
opcode |
funct7_u |
funct7_l |
funct3 |
mnemonic |
generateLegacySim | false

## Software Assignments
CPU_FREQ | 50000000u
DATA_ADDR_WIDTH | 32
DCACHE_LINE_SIZE | 32
DCACHE_LINE_SIZE_LOG2 | 5
DCACHE_SIZE | 4096
HAS_CSR_SUPPORT | 1
HAS_DEBUG_STUB |
ICACHE_LINE_SIZE | 32
ICACHE_LINE_SIZE_LOG2 | 5
ICACHE_SIZE | 4096
INST_ADDR_WIDTH | 32
MTIME_OFFSET | 0x00090000
NIOSV_CORE_VARIANT | 3
NUM_GPR | 32
RESET_ADDR | 0x00000000
TICKS_PER_SEC | no_quote(NIOSV_INTERNAL_TIMER_TICKS_PER_SECOND)
TIMER_DEVICE_TYPE | 2

generation took 0.00 seconds | rendering took 0.02 seconds