niosv_g |

2025.06.17.18:51:32 | Datasheet

Overview

Processor
niosv_g Bantam Lake 4.0.0
All Components
niosv_g intel_niosv_g 4.0.0
Memory Map

| niosv_g
instruction_manager | data_manager
niosv_g |  |
timer_sw_agent |  |
dm_agent |  |

## niosv_g

intel_niosv_g v4.0.0

## Parameters
enableFPU | false
enableBranchPrediction | true
disableFsqrtFdiv | false
hartId | 0
enableDebug | true
enableDebugReset | false
enableLockstep | false
Blind_Window_Period | 1000
Default_Timeout_Period | 255
enableLockstepExtRst | false
useResetReq | false
resetSlave | onchip_memory.s1
resetOffset | 0
enableCoreLevelInterruptController | false
basicInterruptMode | 0
basicShadowRegisterFiles | 0
dataCacheSize | 4096
instCacheSize | 4096
itcm1Size | 0
itcm1Base | 0
itcm1InitFile |
itcm2Size | 0
itcm2Base | 0
itcm2InitFile |
dtcm1Size | 0
dtcm1Base | 0
dtcm1InitFile |
dtcm2Size | 0
dtcm2Base | 0
dtcm2InitFile |
peripheralRegionASize | 524288
peripheralRegionABase | 524288
peripheralRegionBSize | 0
peripheralRegionBBase | 0
enableECCLite | false
enableECCFull | false
CUSTOM_OP |
SUB_OP |
opcode |
funct7_u |
funct7_l |
funct3 |
mnemonic |
generateLegacySim | false

## Software Assignments
CLIC_EN | false
CPU_FREQ | 100000000u
DATA_ADDR_WIDTH | 32
DCACHE_LINE_SIZE | 32
DCACHE_LINE_SIZE_LOG2 | 5
DCACHE_SIZE | 4096
HAS_CSR_SUPPORT | 1
HAS_DEBUG_STUB |
ICACHE_LINE_SIZE | 32
ICACHE_LINE_SIZE_LOG2 | 5
ICACHE_SIZE | 4096
INST_ADDR_WIDTH | 32
INT_MODE | 0
MTIME_OFFSET | 0x00010000
NIOSV_CORE_VARIANT | 3
NUM_GPR | 32
NUM_SRF_BANKS | 1
RESET_ADDR | 0x00040000
TICKS_PER_SEC | no_quote(NIOSV_INTERNAL_TIMER_TICKS_PER_SECOND)
TIMER_DEVICE_TYPE | 2

generation took 0.01 seconds | rendering took 0.02 seconds