AUDIO_PLL |

2025.08.18.10:50:43 | Datasheet

Overview

Memory Map

## iopll_0

altera_iopll v20.0.0

## Parameters
gui_device_family | Agilex 3
gui_device_component | A3CZ135BB18AE7S
gui_device_speed_grade | 6
gui_en_hvio_reconf | false
gui_en_iossm_reconf | false
gui_reference_clock_frequency | 50.0
gui_use_locked | true
gui_en_adv_params | false
gui_pll_auto_reset | false
gui_en_periphery_ports | false
gui_operation_mode | direct
gui_refclk_switch | false
gui_refclk1_frequency | 100.0
gui_en_phout_ports | false
gui_en_extclkout_ports | false
gui_number_of_clocks | 1
gui_fix_vco_frequency | false
gui_enable_output_counter_cascading | false
gui_mif_gen_options | Generate New MIF File
gui_new_mif_file_path | ~/pll.mif
gui_existing_mif_file_path | ~/pll.mif
gui_mif_config_name | unnamed
gui_active_clk | false
gui_clk_bad | false
gui_switchover_mode | Automatic Switchover
gui_enable_cascade_out | false
gui_cascade_outclk_index | 0
gui_enable_cascade_in | false
gui_enable_permit_cal | false
gui_enable_upstream_out_clk | false
gui_enable_mif_dps | false
gui_dps_cntr | C0
gui_dps_num | 1
gui_dps_dir | Positive
gui_extclkout_0_source | C0
gui_extclkout_1_source | C0
gui_clock_name_global | false
gui_clock_name_instantiation | false
gui_clock_name_string0 | outclk0
gui_clock_name_string1 | outclk1
gui_clock_name_string2 | outclk2
gui_clock_name_string3 | outclk3
gui_clock_name_string4 | outclk4
gui_clock_name_string5 | outclk5
gui_clock_name_string6 | outclk6
gui_clock_name_string7 | outclk7
gui_clock_name_string8 | outclk8
gui_clock_name_string9 | outclk9
gui_clock_name_string10 | outclk10
gui_clock_name_string11 | outclk11
gui_clock_name_string12 | outclk12
gui_clock_name_string13 | outclk13
gui_clock_name_string14 | outclk14
gui_clock_name_string15 | outclk15
gui_clock_name_string16 | outclk16
gui_clock_name_string17 | outclk17
gui_divide_factor_c1 | 6
gui_divide_factor_c2 | 6
gui_divide_factor_c3 | 6
gui_divide_factor_c4 | 6
gui_divide_factor_c5 | 6
gui_divide_factor_c6 | 6
gui_divide_factor_c7 | 6
gui_divide_factor_c8 | 6
gui_divide_factor_c9 | 6
gui_divide_factor_c10 | 6
gui_divide_factor_c11 | 6
gui_divide_factor_c12 | 6
gui_divide_factor_c13 | 6
gui_divide_factor_c14 | 6
gui_divide_factor_c15 | 6
gui_divide_factor_c16 | 6
gui_divide_factor_c17 | 6
gui_cascade_counter1 | false
gui_cascade_counter2 | false
gui_cascade_counter3 | false
gui_cascade_counter4 | false
gui_cascade_counter5 | false
gui_cascade_counter6 | false
gui_cascade_counter7 | false
gui_cascade_counter8 | false
gui_cascade_counter9 | false
gui_cascade_counter10 | false
gui_cascade_counter11 | false
gui_cascade_counter12 | false
gui_cascade_counter13 | false
gui_cascade_counter14 | false
gui_cascade_counter15 | false
gui_cascade_counter16 | false
gui_cascade_counter17 | false
gui_output_clock_frequency0 | 12.288136
gui_output_clock_frequency1 | 100.0
gui_output_clock_frequency2 | 100.0
gui_output_clock_frequency3 | 100.0
gui_output_clock_frequency4 | 100.0
gui_output_clock_frequency5 | 100.0
gui_output_clock_frequency6 | 100.0
gui_output_clock_frequency7 | 100.0
gui_output_clock_frequency8 | 100.0
gui_output_clock_frequency9 | 100.0
gui_output_clock_frequency10 | 100.0
gui_output_clock_frequency11 | 100.0
gui_output_clock_frequency12 | 100.0
gui_output_clock_frequency13 | 100.0
gui_output_clock_frequency14 | 100.0
gui_output_clock_frequency15 | 100.0
gui_output_clock_frequency16 | 100.0
gui_output_clock_frequency17 | 100.0
gui_output_clock_frequency_ps1 | 10000.0
gui_output_clock_frequency_ps2 | 10000.0
gui_output_clock_frequency_ps3 | 10000.0
gui_output_clock_frequency_ps4 | 10000.0
gui_output_clock_frequency_ps5 | 10000.0
gui_output_clock_frequency_ps6 | 10000.0
gui_output_clock_frequency_ps7 | 10000.0
gui_output_clock_frequency_ps8 | 10000.0
gui_output_clock_frequency_ps9 | 10000.0
gui_output_clock_frequency_ps10 | 10000.0
gui_output_clock_frequency_ps11 | 10000.0
gui_output_clock_frequency_ps12 | 10000.0
gui_output_clock_frequency_ps13 | 10000.0
gui_output_clock_frequency_ps14 | 10000.0
gui_output_clock_frequency_ps15 | 10000.0
gui_output_clock_frequency_ps16 | 10000.0
gui_output_clock_frequency_ps17 | 10000.0
gui_actual_output_clock_frequency0 | 12.288136
gui_actual_output_clock_frequency1 | 100.0
gui_actual_output_clock_frequency2 | 100.0
gui_actual_output_clock_frequency3 | 100.0
gui_actual_output_clock_frequency4 | 100.0
gui_actual_output_clock_frequency5 | 100.0
gui_actual_output_clock_frequency6 | 100.0
gui_actual_output_clock_frequency7 | 100.0
gui_actual_output_clock_frequency8 | 100.0
gui_actual_output_clock_frequency9 | 100.0
gui_actual_output_clock_frequency10 | 100.0
gui_actual_output_clock_frequency11 | 100.0
gui_actual_output_clock_frequency12 | 100.0
gui_actual_output_clock_frequency13 | 100.0
gui_actual_output_clock_frequency14 | 100.0
gui_actual_output_clock_frequency15 | 100.0
gui_actual_output_clock_frequency16 | 100.0
gui_actual_output_clock_frequency17 | 100.0
gui_actual_output_clock_frequency_range0 | 12.287234,12.287582,12.288136,12.289157,12.289326,12.289562
gui_actual_output_clock_frequency_range1 | 100.0
gui_actual_output_clock_frequency_range2 | 100.0
gui_actual_output_clock_frequency_range3 | 100.0
gui_actual_output_clock_frequency_range4 | 100.0
gui_actual_output_clock_frequency_range5 | 100.0
gui_actual_output_clock_frequency_range6 | 100.0
gui_actual_output_clock_frequency_range7 | 100.0
gui_actual_output_clock_frequency_range8 | 100.0
gui_actual_output_clock_frequency_range9 | 100.0
gui_actual_output_clock_frequency_range10 | 100.0
gui_actual_output_clock_frequency_range11 | 100.0
gui_actual_output_clock_frequency_range12 | 100.0
gui_actual_output_clock_frequency_range13 | 100.0
gui_actual_output_clock_frequency_range14 | 100.0
gui_actual_output_clock_frequency_range15 | 100.0
gui_actual_output_clock_frequency_range16 | 100.0
gui_actual_output_clock_frequency_range17 | 100.0
gui_ps_units0 | ps
gui_ps_units1 | ps
gui_ps_units2 | ps
gui_ps_units3 | ps
gui_ps_units4 | ps
gui_ps_units5 | ps
gui_ps_units6 | ps
gui_ps_units7 | ps
gui_ps_units8 | ps
gui_ps_units9 | ps
gui_ps_units10 | ps
gui_ps_units11 | ps
gui_ps_units12 | ps
gui_ps_units13 | ps
gui_ps_units14 | ps
gui_ps_units15 | ps
gui_ps_units16 | ps
gui_ps_units17 | ps
gui_phase_shift0 | 0.0
gui_phase_shift1 | 0.0
gui_phase_shift2 | 0.0
gui_phase_shift3 | 0.0
gui_phase_shift4 | 0.0
gui_phase_shift5 | 0.0
gui_phase_shift6 | 0.0
gui_phase_shift7 | 0.0
gui_phase_shift8 | 0.0
gui_phase_shift9 | 0.0
gui_phase_shift10 | 0.0
gui_phase_shift11 | 0.0
gui_phase_shift12 | 0.0
gui_phase_shift13 | 0.0
gui_phase_shift14 | 0.0
gui_phase_shift15 | 0.0
gui_phase_shift16 | 0.0
gui_phase_shift17 | 0.0
gui_phase_shift_deg1 | 0.0
gui_phase_shift_deg2 | 0.0
gui_phase_shift_deg3 | 0.0
gui_phase_shift_deg4 | 0.0
gui_phase_shift_deg5 | 0.0
gui_phase_shift_deg6 | 0.0
gui_phase_shift_deg7 | 0.0
gui_phase_shift_deg8 | 0.0
gui_phase_shift_deg9 | 0.0
gui_phase_shift_deg10 | 0.0
gui_phase_shift_deg11 | 0.0
gui_phase_shift_deg12 | 0.0
gui_phase_shift_deg13 | 0.0
gui_phase_shift_deg14 | 0.0
gui_phase_shift_deg15 | 0.0
gui_phase_shift_deg16 | 0.0
gui_phase_shift_deg17 | 0.0
gui_actual_phase_shift0 | 0.0
gui_actual_phase_shift1 | 0.0
gui_actual_phase_shift2 | 0.0
gui_actual_phase_shift3 | 0.0
gui_actual_phase_shift4 | 0.0
gui_actual_phase_shift5 | 0.0
gui_actual_phase_shift6 | 0.0
gui_actual_phase_shift7 | 0.0
gui_actual_phase_shift8 | 0.0
gui_actual_phase_shift9 | 0.0
gui_actual_phase_shift10 | 0.0
gui_actual_phase_shift11 | 0.0
gui_actual_phase_shift12 | 0.0
gui_actual_phase_shift13 | 0.0
gui_actual_phase_shift14 | 0.0
gui_actual_phase_shift15 | 0.0
gui_actual_phase_shift16 | 0.0
gui_actual_phase_shift17 | 0.0
gui_actual_phase_shift_range0 | 0.0,57.5,86.2,114.9,172.4,229.9
gui_actual_phase_shift_range1 | 0.0
gui_actual_phase_shift_range2 | 0.0
gui_actual_phase_shift_range3 | 0.0
gui_actual_phase_shift_range4 | 0.0
gui_actual_phase_shift_range5 | 0.0
gui_actual_phase_shift_range6 | 0.0
gui_actual_phase_shift_range7 | 0.0
gui_actual_phase_shift_range8 | 0.0
gui_actual_phase_shift_range9 | 0.0
gui_actual_phase_shift_range10 | 0.0
gui_actual_phase_shift_range11 | 0.0
gui_actual_phase_shift_range12 | 0.0
gui_actual_phase_shift_range13 | 0.0
gui_actual_phase_shift_range14 | 0.0
gui_actual_phase_shift_range15 | 0.0
gui_actual_phase_shift_range16 | 0.0
gui_actual_phase_shift_range17 | 0.0
gui_actual_phase_shift_deg1 | 0.0
gui_actual_phase_shift_deg2 | 0.0
gui_actual_phase_shift_deg3 | 0.0
gui_actual_phase_shift_deg4 | 0.0
gui_actual_phase_shift_deg5 | 0.0
gui_actual_phase_shift_deg6 | 0.0
gui_actual_phase_shift_deg7 | 0.0
gui_actual_phase_shift_deg8 | 0.0
gui_actual_phase_shift_deg9 | 0.0
gui_actual_phase_shift_deg10 | 0.0
gui_actual_phase_shift_deg11 | 0.0
gui_actual_phase_shift_deg12 | 0.0
gui_actual_phase_shift_deg13 | 0.0
gui_actual_phase_shift_deg14 | 0.0
gui_actual_phase_shift_deg15 | 0.0
gui_actual_phase_shift_deg16 | 0.0
gui_actual_phase_shift_deg17 | 0.0
gui_actual_phase_shift_deg_range1 | 0.0
gui_actual_phase_shift_deg_range2 | 0.0
gui_actual_phase_shift_deg_range3 | 0.0
gui_actual_phase_shift_deg_range4 | 0.0
gui_actual_phase_shift_deg_range5 | 0.0
gui_actual_phase_shift_deg_range6 | 0.0
gui_actual_phase_shift_deg_range7 | 0.0
gui_actual_phase_shift_deg_range8 | 0.0
gui_actual_phase_shift_deg_range9 | 0.0
gui_actual_phase_shift_deg_range10 | 0.0
gui_actual_phase_shift_deg_range11 | 0.0
gui_actual_phase_shift_deg_range12 | 0.0
gui_actual_phase_shift_deg_range13 | 0.0
gui_actual_phase_shift_deg_range14 | 0.0
gui_actual_phase_shift_deg_range15 | 0.0
gui_actual_phase_shift_deg_range16 | 0.0
gui_actual_phase_shift_deg_range17 | 0.0
gui_duty_cycle0 | 50.0
gui_duty_cycle1 | 50.0
gui_duty_cycle2 | 50.0
gui_duty_cycle3 | 50.0
gui_duty_cycle4 | 50.0
gui_duty_cycle5 | 50.0
gui_duty_cycle6 | 50.0
gui_duty_cycle7 | 50.0
gui_duty_cycle8 | 50.0
gui_duty_cycle9 | 50.0
gui_duty_cycle10 | 50.0
gui_duty_cycle11 | 50.0
gui_duty_cycle12 | 50.0
gui_duty_cycle13 | 50.0
gui_duty_cycle14 | 50.0
gui_duty_cycle15 | 50.0
gui_duty_cycle16 | 50.0
gui_duty_cycle17 | 50.0
gui_actual_duty_cycle0 | 50.0
gui_actual_duty_cycle1 | 50.0
gui_actual_duty_cycle2 | 50.0
gui_actual_duty_cycle3 | 50.0
gui_actual_duty_cycle4 | 50.0
gui_actual_duty_cycle5 | 50.0
gui_actual_duty_cycle6 | 50.0
gui_actual_duty_cycle7 | 50.0
gui_actual_duty_cycle8 | 50.0
gui_actual_duty_cycle9 | 50.0
gui_actual_duty_cycle10 | 50.0
gui_actual_duty_cycle11 | 50.0
gui_actual_duty_cycle12 | 50.0
gui_actual_duty_cycle13 | 50.0
gui_actual_duty_cycle14 | 50.0
gui_actual_duty_cycle15 | 50.0
gui_actual_duty_cycle16 | 50.0
gui_actual_duty_cycle17 | 50.0
gui_actual_duty_cycle_range0 | 49.44,49.58,49.72,50.0,50.28,50.42
gui_actual_duty_cycle_range1 | 50.0
gui_actual_duty_cycle_range2 | 50.0
gui_actual_duty_cycle_range3 | 50.0
gui_actual_duty_cycle_range4 | 50.0
gui_actual_duty_cycle_range5 | 50.0
gui_actual_duty_cycle_range6 | 50.0
gui_actual_duty_cycle_range7 | 50.0
gui_actual_duty_cycle_range8 | 50.0
gui_actual_duty_cycle_range9 | 50.0
gui_actual_duty_cycle_range10 | 50.0
gui_actual_duty_cycle_range11 | 50.0
gui_actual_duty_cycle_range12 | 50.0
gui_actual_duty_cycle_range13 | 50.0
gui_actual_duty_cycle_range14 | 50.0
gui_actual_duty_cycle_range15 | 50.0
gui_actual_duty_cycle_range16 | 50.0
gui_actual_duty_cycle_range17 | 50.0
parameterTable_names | M-Counter Divide Setting,N-Counter Divide Setting,VCO Frequency,C-Counter-0 Divide Setting,C-Counter-1 Divide Setting,C-Counter-2 Divide Setting,C-Counter-3 Divide Setting,C-Counter-4 Divide Setting,C-Counter-5 Divide Setting,C-Counter-6 Divide Setting,C-Counter-7 Divide Setting,C-Counter-8 Divide Setting,PLL Auto Reset,M-Counter Hi Divide,M-Counter Lo Divide,M-Counter Even Duty Enable,M-Counter Bypass Enable,N-Counter Hi Divide,N-Counter Lo Divide,N-Counter Even Duty Enable,N-Counter Bypass Enable,C-Counter-0 Hi Divide,C-Counter-1 Hi Divide,C-Counter-2 Hi Divide,C-Counter-3 Hi Divide,C-Counter-4 Hi Divide,C-Counter-5 Hi Divide,C-Counter-6 Hi Divide,C-Counter-7 Hi Divide,C-Counter-8 Hi Divide,C-Counter-0 Lo Divide,C-Counter-1 Lo Divide,C-Counter-2 Lo Divide,C-Counter-3 Lo Divide,C-Counter-4 Lo Divide,C-Counter-5 Lo Divide,C-Counter-6 Lo Divide,C-Counter-7 Lo Divide,C-Counter-8 Lo Divide,C-Counter-0 Even Duty Enable,C-Counter-1 Even Duty Enable,C-Counter-2 Even Duty Enable,C-Counter-3 Even Duty Enable,C-Counter-4 Even Duty Enable,C-Counter-5 Even Duty Enable,C-Counter-6 Even Duty Enable,C-Counter-7 Even Duty Enable,C-Counter-8 Even Duty Enable,C-Counter-0 Bypass Enable,C-Counter-1 Bypass Enable,C-Counter-2 Bypass Enable,C-Counter-3 Bypass Enable,C-Counter-4 Bypass Enable,C-Counter-5 Bypass Enable,C-Counter-6 Bypass Enable,C-Counter-7 Bypass Enable,C-Counter-8 Bypass Enable,C-Counter-0 Preset,C-Counter-1 Preset,C-Counter-2 Preset,C-Counter-3 Preset,C-Counter-4 Preset,C-Counter-5 Preset,C-Counter-6 Preset,C-Counter-7 Preset,C-Counter-8 Preset,C-Counter-0 Phase Mux Preset,C-Counter-1 Phase Mux Preset,C-Counter-2 Phase Mux Preset,C-Counter-3 Phase Mux Preset,C-Counter-4 Phase Mux Preset,C-Counter-5 Phase Mux Preset,C-Counter-6 Phase Mux Preset,C-Counter-7 Phase Mux Preset,C-Counter-8 Phase Mux Preset,Charge Pump Current,Bandwidth Control
parameterTable_values | 87,2,2175.0 MHz,177,510,1,1,1,1,1,1,1,false,44,43,true,false,1,1,false,false,89,255,256,256,256,256,256,1,1,88,255,256,256,256,256,256,1,1,true,false,false,false,false,false,false,false,false,false,false,true,true,true,true,true,true,true,1,1,1,1,1,1,1,1,1,0,0,0,0,0,0,0,0,0,pll_cp_setting21,pll_bw_res_setting5
mifTable_names | The MIF file specified does not yet exist
mifTable_values |
deviceFamily | UNKNOWN
generateLegacySim | false

## Software Assignments (none)

generation took 0.00 seconds | rendering took 0.06 seconds