system_hydra_0 |

2025.05.29.17:07:24 | Datasheet

Overview

Memory Map

| hydra_0 | hydra_0_driver0_mem_axi4
driver0_axi4 | axi4

## hydra_0

hydra v3.0.0

## Parameters
CONFIG_INTF_MODE | CONFIG_INTF_MODE_DISABLED
EXPORT_STATUS_INTF | false
RUN_ON_RESET | true
CALL_SIM_FINISH | true
NUM_DRIVERS | 1
DRIVER_0_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_0_CAM_AXIST_KEY_WIDTH | 64
DRIVER_0_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_0_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_0_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_0_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_0_CAM_AXIST_TID_WIDTH | 8
DRIVER_0_CAM_AXIST_PTR_WIDTH | 1
DRIVER_0_CAM_AXIST_LOG2_TABLES | 1
DRIVER_0_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_0_CAM_TEST_CAM | BCAM
DRIVER_0_ED_ASSOC_STORAGE_ONLY | false
DRIVER_0_ED_FIRST_CAM_DRIVER | false
DRIVER_0_ED_ONCHIP_MEM_ONLY | false
DRIVER_0_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_0_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_0_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_0_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_0_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_0_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_0_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_0_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_0_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_0_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_0_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_0_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_0_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_0_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_0_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_0_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_0_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_0_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_0_MEM_AXI4_AWID_WIDTH | 9
DRIVER_0_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_0_MEM_AXI4_USE_AWLOCK | true
DRIVER_0_MEM_AXI4_USE_AWCACHE | true
DRIVER_0_MEM_AXI4_USE_AWQOS | true
DRIVER_0_MEM_AXI4_USE_AWREGION | true
DRIVER_0_MEM_AXI4_USE_AWUSER | true
DRIVER_0_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_0_MEM_AXI4_ARID_WIDTH | 9
DRIVER_0_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_0_MEM_AXI4_USE_ARLOCK | true
DRIVER_0_MEM_AXI4_USE_ARCACHE | true
DRIVER_0_MEM_AXI4_USE_ARQOS | true
DRIVER_0_MEM_AXI4_USE_ARREGION | true
DRIVER_0_MEM_AXI4_USE_ARUSER | true
DRIVER_0_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_0_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_0_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_0_MEM_AXI4_USE_BUSER | false
DRIVER_0_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_0_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_0_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_1_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_1_CAM_AXIST_KEY_WIDTH | 64
DRIVER_1_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_1_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_1_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_1_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_1_CAM_AXIST_TID_WIDTH | 8
DRIVER_1_CAM_AXIST_PTR_WIDTH | 1
DRIVER_1_CAM_AXIST_LOG2_TABLES | 1
DRIVER_1_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_1_CAM_TEST_CAM | BCAM
DRIVER_1_ED_ASSOC_STORAGE_ONLY | false
DRIVER_1_ED_FIRST_CAM_DRIVER | false
DRIVER_1_ED_ONCHIP_MEM_ONLY | false
DRIVER_1_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_1_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_1_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_1_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_1_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_1_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_1_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_1_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_1_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_1_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_1_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_1_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_1_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_1_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_1_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_1_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_1_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_1_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_1_MEM_AXI4_AWID_WIDTH | 9
DRIVER_1_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_1_MEM_AXI4_USE_AWLOCK | true
DRIVER_1_MEM_AXI4_USE_AWCACHE | true
DRIVER_1_MEM_AXI4_USE_AWQOS | true
DRIVER_1_MEM_AXI4_USE_AWREGION | true
DRIVER_1_MEM_AXI4_USE_AWUSER | true
DRIVER_1_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_1_MEM_AXI4_ARID_WIDTH | 9
DRIVER_1_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_1_MEM_AXI4_USE_ARLOCK | true
DRIVER_1_MEM_AXI4_USE_ARCACHE | true
DRIVER_1_MEM_AXI4_USE_ARQOS | true
DRIVER_1_MEM_AXI4_USE_ARREGION | true
DRIVER_1_MEM_AXI4_USE_ARUSER | true
DRIVER_1_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_1_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_1_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_1_MEM_AXI4_USE_BUSER | false
DRIVER_1_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_1_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_1_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_2_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_2_CAM_AXIST_KEY_WIDTH | 64
DRIVER_2_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_2_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_2_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_2_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_2_CAM_AXIST_TID_WIDTH | 8
DRIVER_2_CAM_AXIST_PTR_WIDTH | 1
DRIVER_2_CAM_AXIST_LOG2_TABLES | 1
DRIVER_2_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_2_CAM_TEST_CAM | BCAM
DRIVER_2_ED_ASSOC_STORAGE_ONLY | false
DRIVER_2_ED_FIRST_CAM_DRIVER | false
DRIVER_2_ED_ONCHIP_MEM_ONLY | false
DRIVER_2_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_2_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_2_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_2_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_2_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_2_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_2_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_2_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_2_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_2_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_2_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_2_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_2_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_2_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_2_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_2_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_2_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_2_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_2_MEM_AXI4_AWID_WIDTH | 9
DRIVER_2_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_2_MEM_AXI4_USE_AWLOCK | true
DRIVER_2_MEM_AXI4_USE_AWCACHE | true
DRIVER_2_MEM_AXI4_USE_AWQOS | true
DRIVER_2_MEM_AXI4_USE_AWREGION | true
DRIVER_2_MEM_AXI4_USE_AWUSER | true
DRIVER_2_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_2_MEM_AXI4_ARID_WIDTH | 9
DRIVER_2_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_2_MEM_AXI4_USE_ARLOCK | true
DRIVER_2_MEM_AXI4_USE_ARCACHE | true
DRIVER_2_MEM_AXI4_USE_ARQOS | true
DRIVER_2_MEM_AXI4_USE_ARREGION | true
DRIVER_2_MEM_AXI4_USE_ARUSER | true
DRIVER_2_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_2_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_2_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_2_MEM_AXI4_USE_BUSER | false
DRIVER_2_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_2_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_2_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_3_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_3_CAM_AXIST_KEY_WIDTH | 64
DRIVER_3_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_3_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_3_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_3_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_3_CAM_AXIST_TID_WIDTH | 8
DRIVER_3_CAM_AXIST_PTR_WIDTH | 1
DRIVER_3_CAM_AXIST_LOG2_TABLES | 1
DRIVER_3_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_3_CAM_TEST_CAM | BCAM
DRIVER_3_ED_ASSOC_STORAGE_ONLY | false
DRIVER_3_ED_FIRST_CAM_DRIVER | false
DRIVER_3_ED_ONCHIP_MEM_ONLY | false
DRIVER_3_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_3_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_3_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_3_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_3_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_3_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_3_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_3_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_3_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_3_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_3_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_3_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_3_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_3_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_3_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_3_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_3_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_3_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_3_MEM_AXI4_AWID_WIDTH | 9
DRIVER_3_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_3_MEM_AXI4_USE_AWLOCK | true
DRIVER_3_MEM_AXI4_USE_AWCACHE | true
DRIVER_3_MEM_AXI4_USE_AWQOS | true
DRIVER_3_MEM_AXI4_USE_AWREGION | true
DRIVER_3_MEM_AXI4_USE_AWUSER | true
DRIVER_3_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_3_MEM_AXI4_ARID_WIDTH | 9
DRIVER_3_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_3_MEM_AXI4_USE_ARLOCK | true
DRIVER_3_MEM_AXI4_USE_ARCACHE | true
DRIVER_3_MEM_AXI4_USE_ARQOS | true
DRIVER_3_MEM_AXI4_USE_ARREGION | true
DRIVER_3_MEM_AXI4_USE_ARUSER | true
DRIVER_3_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_3_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_3_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_3_MEM_AXI4_USE_BUSER | false
DRIVER_3_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_3_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_3_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_4_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_4_CAM_AXIST_KEY_WIDTH | 64
DRIVER_4_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_4_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_4_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_4_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_4_CAM_AXIST_TID_WIDTH | 8
DRIVER_4_CAM_AXIST_PTR_WIDTH | 1
DRIVER_4_CAM_AXIST_LOG2_TABLES | 1
DRIVER_4_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_4_CAM_TEST_CAM | BCAM
DRIVER_4_ED_ASSOC_STORAGE_ONLY | false
DRIVER_4_ED_FIRST_CAM_DRIVER | false
DRIVER_4_ED_ONCHIP_MEM_ONLY | false
DRIVER_4_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_4_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_4_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_4_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_4_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_4_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_4_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_4_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_4_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_4_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_4_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_4_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_4_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_4_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_4_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_4_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_4_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_4_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_4_MEM_AXI4_AWID_WIDTH | 9
DRIVER_4_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_4_MEM_AXI4_USE_AWLOCK | true
DRIVER_4_MEM_AXI4_USE_AWCACHE | true
DRIVER_4_MEM_AXI4_USE_AWQOS | true
DRIVER_4_MEM_AXI4_USE_AWREGION | true
DRIVER_4_MEM_AXI4_USE_AWUSER | true
DRIVER_4_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_4_MEM_AXI4_ARID_WIDTH | 9
DRIVER_4_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_4_MEM_AXI4_USE_ARLOCK | true
DRIVER_4_MEM_AXI4_USE_ARCACHE | true
DRIVER_4_MEM_AXI4_USE_ARQOS | true
DRIVER_4_MEM_AXI4_USE_ARREGION | true
DRIVER_4_MEM_AXI4_USE_ARUSER | true
DRIVER_4_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_4_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_4_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_4_MEM_AXI4_USE_BUSER | false
DRIVER_4_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_4_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_4_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_5_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_5_CAM_AXIST_KEY_WIDTH | 64
DRIVER_5_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_5_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_5_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_5_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_5_CAM_AXIST_TID_WIDTH | 8
DRIVER_5_CAM_AXIST_PTR_WIDTH | 1
DRIVER_5_CAM_AXIST_LOG2_TABLES | 1
DRIVER_5_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_5_CAM_TEST_CAM | BCAM
DRIVER_5_ED_ASSOC_STORAGE_ONLY | false
DRIVER_5_ED_FIRST_CAM_DRIVER | false
DRIVER_5_ED_ONCHIP_MEM_ONLY | false
DRIVER_5_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_5_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_5_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_5_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_5_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_5_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_5_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_5_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_5_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_5_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_5_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_5_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_5_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_5_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_5_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_5_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_5_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_5_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_5_MEM_AXI4_AWID_WIDTH | 9
DRIVER_5_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_5_MEM_AXI4_USE_AWLOCK | true
DRIVER_5_MEM_AXI4_USE_AWCACHE | true
DRIVER_5_MEM_AXI4_USE_AWQOS | true
DRIVER_5_MEM_AXI4_USE_AWREGION | true
DRIVER_5_MEM_AXI4_USE_AWUSER | true
DRIVER_5_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_5_MEM_AXI4_ARID_WIDTH | 9
DRIVER_5_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_5_MEM_AXI4_USE_ARLOCK | true
DRIVER_5_MEM_AXI4_USE_ARCACHE | true
DRIVER_5_MEM_AXI4_USE_ARQOS | true
DRIVER_5_MEM_AXI4_USE_ARREGION | true
DRIVER_5_MEM_AXI4_USE_ARUSER | true
DRIVER_5_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_5_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_5_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_5_MEM_AXI4_USE_BUSER | false
DRIVER_5_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_5_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_5_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_6_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_6_CAM_AXIST_KEY_WIDTH | 64
DRIVER_6_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_6_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_6_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_6_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_6_CAM_AXIST_TID_WIDTH | 8
DRIVER_6_CAM_AXIST_PTR_WIDTH | 1
DRIVER_6_CAM_AXIST_LOG2_TABLES | 1
DRIVER_6_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_6_CAM_TEST_CAM | BCAM
DRIVER_6_ED_ASSOC_STORAGE_ONLY | false
DRIVER_6_ED_FIRST_CAM_DRIVER | false
DRIVER_6_ED_ONCHIP_MEM_ONLY | false
DRIVER_6_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_6_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_6_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_6_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_6_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_6_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_6_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_6_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_6_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_6_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_6_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_6_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_6_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_6_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_6_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_6_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_6_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_6_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_6_MEM_AXI4_AWID_WIDTH | 9
DRIVER_6_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_6_MEM_AXI4_USE_AWLOCK | true
DRIVER_6_MEM_AXI4_USE_AWCACHE | true
DRIVER_6_MEM_AXI4_USE_AWQOS | true
DRIVER_6_MEM_AXI4_USE_AWREGION | true
DRIVER_6_MEM_AXI4_USE_AWUSER | true
DRIVER_6_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_6_MEM_AXI4_ARID_WIDTH | 9
DRIVER_6_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_6_MEM_AXI4_USE_ARLOCK | true
DRIVER_6_MEM_AXI4_USE_ARCACHE | true
DRIVER_6_MEM_AXI4_USE_ARQOS | true
DRIVER_6_MEM_AXI4_USE_ARREGION | true
DRIVER_6_MEM_AXI4_USE_ARUSER | true
DRIVER_6_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_6_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_6_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_6_MEM_AXI4_USE_BUSER | false
DRIVER_6_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_6_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_6_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_7_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_7_CAM_AXIST_KEY_WIDTH | 64
DRIVER_7_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_7_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_7_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_7_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_7_CAM_AXIST_TID_WIDTH | 8
DRIVER_7_CAM_AXIST_PTR_WIDTH | 1
DRIVER_7_CAM_AXIST_LOG2_TABLES | 1
DRIVER_7_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_7_CAM_TEST_CAM | BCAM
DRIVER_7_ED_ASSOC_STORAGE_ONLY | false
DRIVER_7_ED_FIRST_CAM_DRIVER | false
DRIVER_7_ED_ONCHIP_MEM_ONLY | false
DRIVER_7_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_7_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_7_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_7_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_7_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_7_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_7_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_7_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_7_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_7_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_7_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_7_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_7_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_7_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_7_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_7_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_7_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_7_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_7_MEM_AXI4_AWID_WIDTH | 9
DRIVER_7_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_7_MEM_AXI4_USE_AWLOCK | true
DRIVER_7_MEM_AXI4_USE_AWCACHE | true
DRIVER_7_MEM_AXI4_USE_AWQOS | true
DRIVER_7_MEM_AXI4_USE_AWREGION | true
DRIVER_7_MEM_AXI4_USE_AWUSER | true
DRIVER_7_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_7_MEM_AXI4_ARID_WIDTH | 9
DRIVER_7_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_7_MEM_AXI4_USE_ARLOCK | true
DRIVER_7_MEM_AXI4_USE_ARCACHE | true
DRIVER_7_MEM_AXI4_USE_ARQOS | true
DRIVER_7_MEM_AXI4_USE_ARREGION | true
DRIVER_7_MEM_AXI4_USE_ARUSER | true
DRIVER_7_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_7_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_7_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_7_MEM_AXI4_USE_BUSER | false
DRIVER_7_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_7_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_7_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_8_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_8_CAM_AXIST_KEY_WIDTH | 64
DRIVER_8_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_8_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_8_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_8_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_8_CAM_AXIST_TID_WIDTH | 8
DRIVER_8_CAM_AXIST_PTR_WIDTH | 1
DRIVER_8_CAM_AXIST_LOG2_TABLES | 1
DRIVER_8_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_8_CAM_TEST_CAM | BCAM
DRIVER_8_ED_ASSOC_STORAGE_ONLY | false
DRIVER_8_ED_FIRST_CAM_DRIVER | false
DRIVER_8_ED_ONCHIP_MEM_ONLY | false
DRIVER_8_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_8_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_8_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_8_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_8_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_8_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_8_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_8_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_8_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_8_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_8_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_8_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_8_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_8_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_8_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_8_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_8_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_8_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_8_MEM_AXI4_AWID_WIDTH | 9
DRIVER_8_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_8_MEM_AXI4_USE_AWLOCK | true
DRIVER_8_MEM_AXI4_USE_AWCACHE | true
DRIVER_8_MEM_AXI4_USE_AWQOS | true
DRIVER_8_MEM_AXI4_USE_AWREGION | true
DRIVER_8_MEM_AXI4_USE_AWUSER | true
DRIVER_8_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_8_MEM_AXI4_ARID_WIDTH | 9
DRIVER_8_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_8_MEM_AXI4_USE_ARLOCK | true
DRIVER_8_MEM_AXI4_USE_ARCACHE | true
DRIVER_8_MEM_AXI4_USE_ARQOS | true
DRIVER_8_MEM_AXI4_USE_ARREGION | true
DRIVER_8_MEM_AXI4_USE_ARUSER | true
DRIVER_8_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_8_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_8_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_8_MEM_AXI4_USE_BUSER | false
DRIVER_8_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_8_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_8_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_9_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_9_CAM_AXIST_KEY_WIDTH | 64
DRIVER_9_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_9_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_9_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_9_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_9_CAM_AXIST_TID_WIDTH | 8
DRIVER_9_CAM_AXIST_PTR_WIDTH | 1
DRIVER_9_CAM_AXIST_LOG2_TABLES | 1
DRIVER_9_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_9_CAM_TEST_CAM | BCAM
DRIVER_9_ED_ASSOC_STORAGE_ONLY | false
DRIVER_9_ED_FIRST_CAM_DRIVER | false
DRIVER_9_ED_ONCHIP_MEM_ONLY | false
DRIVER_9_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_9_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_9_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_9_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_9_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_9_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_9_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_9_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_9_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_9_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_9_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_9_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_9_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_9_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_9_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_9_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_9_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_9_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_9_MEM_AXI4_AWID_WIDTH | 9
DRIVER_9_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_9_MEM_AXI4_USE_AWLOCK | true
DRIVER_9_MEM_AXI4_USE_AWCACHE | true
DRIVER_9_MEM_AXI4_USE_AWQOS | true
DRIVER_9_MEM_AXI4_USE_AWREGION | true
DRIVER_9_MEM_AXI4_USE_AWUSER | true
DRIVER_9_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_9_MEM_AXI4_ARID_WIDTH | 9
DRIVER_9_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_9_MEM_AXI4_USE_ARLOCK | true
DRIVER_9_MEM_AXI4_USE_ARCACHE | true
DRIVER_9_MEM_AXI4_USE_ARQOS | true
DRIVER_9_MEM_AXI4_USE_ARREGION | true
DRIVER_9_MEM_AXI4_USE_ARUSER | true
DRIVER_9_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_9_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_9_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_9_MEM_AXI4_USE_BUSER | false
DRIVER_9_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_9_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_9_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_10_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_10_CAM_AXIST_KEY_WIDTH | 64
DRIVER_10_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_10_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_10_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_10_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_10_CAM_AXIST_TID_WIDTH | 8
DRIVER_10_CAM_AXIST_PTR_WIDTH | 1
DRIVER_10_CAM_AXIST_LOG2_TABLES | 1
DRIVER_10_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_10_CAM_TEST_CAM | BCAM
DRIVER_10_ED_ASSOC_STORAGE_ONLY | false
DRIVER_10_ED_FIRST_CAM_DRIVER | false
DRIVER_10_ED_ONCHIP_MEM_ONLY | false
DRIVER_10_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_10_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_10_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_10_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_10_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_10_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_10_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_10_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_10_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_10_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_10_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_10_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_10_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_10_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_10_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_10_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_10_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_10_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_10_MEM_AXI4_AWID_WIDTH | 9
DRIVER_10_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_10_MEM_AXI4_USE_AWLOCK | true
DRIVER_10_MEM_AXI4_USE_AWCACHE | true
DRIVER_10_MEM_AXI4_USE_AWQOS | true
DRIVER_10_MEM_AXI4_USE_AWREGION | true
DRIVER_10_MEM_AXI4_USE_AWUSER | true
DRIVER_10_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_10_MEM_AXI4_ARID_WIDTH | 9
DRIVER_10_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_10_MEM_AXI4_USE_ARLOCK | true
DRIVER_10_MEM_AXI4_USE_ARCACHE | true
DRIVER_10_MEM_AXI4_USE_ARQOS | true
DRIVER_10_MEM_AXI4_USE_ARREGION | true
DRIVER_10_MEM_AXI4_USE_ARUSER | true
DRIVER_10_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_10_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_10_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_10_MEM_AXI4_USE_BUSER | false
DRIVER_10_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_10_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_10_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_11_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_11_CAM_AXIST_KEY_WIDTH | 64
DRIVER_11_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_11_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_11_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_11_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_11_CAM_AXIST_TID_WIDTH | 8
DRIVER_11_CAM_AXIST_PTR_WIDTH | 1
DRIVER_11_CAM_AXIST_LOG2_TABLES | 1
DRIVER_11_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_11_CAM_TEST_CAM | BCAM
DRIVER_11_ED_ASSOC_STORAGE_ONLY | false
DRIVER_11_ED_FIRST_CAM_DRIVER | false
DRIVER_11_ED_ONCHIP_MEM_ONLY | false
DRIVER_11_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_11_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_11_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_11_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_11_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_11_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_11_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_11_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_11_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_11_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_11_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_11_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_11_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_11_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_11_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_11_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_11_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_11_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_11_MEM_AXI4_AWID_WIDTH | 9
DRIVER_11_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_11_MEM_AXI4_USE_AWLOCK | true
DRIVER_11_MEM_AXI4_USE_AWCACHE | true
DRIVER_11_MEM_AXI4_USE_AWQOS | true
DRIVER_11_MEM_AXI4_USE_AWREGION | true
DRIVER_11_MEM_AXI4_USE_AWUSER | true
DRIVER_11_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_11_MEM_AXI4_ARID_WIDTH | 9
DRIVER_11_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_11_MEM_AXI4_USE_ARLOCK | true
DRIVER_11_MEM_AXI4_USE_ARCACHE | true
DRIVER_11_MEM_AXI4_USE_ARQOS | true
DRIVER_11_MEM_AXI4_USE_ARREGION | true
DRIVER_11_MEM_AXI4_USE_ARUSER | true
DRIVER_11_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_11_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_11_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_11_MEM_AXI4_USE_BUSER | false
DRIVER_11_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_11_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_11_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_12_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_12_CAM_AXIST_KEY_WIDTH | 64
DRIVER_12_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_12_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_12_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_12_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_12_CAM_AXIST_TID_WIDTH | 8
DRIVER_12_CAM_AXIST_PTR_WIDTH | 1
DRIVER_12_CAM_AXIST_LOG2_TABLES | 1
DRIVER_12_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_12_CAM_TEST_CAM | BCAM
DRIVER_12_ED_ASSOC_STORAGE_ONLY | false
DRIVER_12_ED_FIRST_CAM_DRIVER | false
DRIVER_12_ED_ONCHIP_MEM_ONLY | false
DRIVER_12_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_12_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_12_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_12_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_12_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_12_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_12_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_12_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_12_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_12_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_12_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_12_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_12_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_12_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_12_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_12_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_12_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_12_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_12_MEM_AXI4_AWID_WIDTH | 9
DRIVER_12_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_12_MEM_AXI4_USE_AWLOCK | true
DRIVER_12_MEM_AXI4_USE_AWCACHE | true
DRIVER_12_MEM_AXI4_USE_AWQOS | true
DRIVER_12_MEM_AXI4_USE_AWREGION | true
DRIVER_12_MEM_AXI4_USE_AWUSER | true
DRIVER_12_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_12_MEM_AXI4_ARID_WIDTH | 9
DRIVER_12_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_12_MEM_AXI4_USE_ARLOCK | true
DRIVER_12_MEM_AXI4_USE_ARCACHE | true
DRIVER_12_MEM_AXI4_USE_ARQOS | true
DRIVER_12_MEM_AXI4_USE_ARREGION | true
DRIVER_12_MEM_AXI4_USE_ARUSER | true
DRIVER_12_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_12_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_12_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_12_MEM_AXI4_USE_BUSER | false
DRIVER_12_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_12_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_12_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_13_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_13_CAM_AXIST_KEY_WIDTH | 64
DRIVER_13_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_13_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_13_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_13_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_13_CAM_AXIST_TID_WIDTH | 8
DRIVER_13_CAM_AXIST_PTR_WIDTH | 1
DRIVER_13_CAM_AXIST_LOG2_TABLES | 1
DRIVER_13_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_13_CAM_TEST_CAM | BCAM
DRIVER_13_ED_ASSOC_STORAGE_ONLY | false
DRIVER_13_ED_FIRST_CAM_DRIVER | false
DRIVER_13_ED_ONCHIP_MEM_ONLY | false
DRIVER_13_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_13_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_13_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_13_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_13_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_13_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_13_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_13_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_13_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_13_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_13_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_13_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_13_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_13_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_13_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_13_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_13_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_13_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_13_MEM_AXI4_AWID_WIDTH | 9
DRIVER_13_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_13_MEM_AXI4_USE_AWLOCK | true
DRIVER_13_MEM_AXI4_USE_AWCACHE | true
DRIVER_13_MEM_AXI4_USE_AWQOS | true
DRIVER_13_MEM_AXI4_USE_AWREGION | true
DRIVER_13_MEM_AXI4_USE_AWUSER | true
DRIVER_13_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_13_MEM_AXI4_ARID_WIDTH | 9
DRIVER_13_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_13_MEM_AXI4_USE_ARLOCK | true
DRIVER_13_MEM_AXI4_USE_ARCACHE | true
DRIVER_13_MEM_AXI4_USE_ARQOS | true
DRIVER_13_MEM_AXI4_USE_ARREGION | true
DRIVER_13_MEM_AXI4_USE_ARUSER | true
DRIVER_13_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_13_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_13_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_13_MEM_AXI4_USE_BUSER | false
DRIVER_13_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_13_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_13_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_14_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_14_CAM_AXIST_KEY_WIDTH | 64
DRIVER_14_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_14_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_14_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_14_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_14_CAM_AXIST_TID_WIDTH | 8
DRIVER_14_CAM_AXIST_PTR_WIDTH | 1
DRIVER_14_CAM_AXIST_LOG2_TABLES | 1
DRIVER_14_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_14_CAM_TEST_CAM | BCAM
DRIVER_14_ED_ASSOC_STORAGE_ONLY | false
DRIVER_14_ED_FIRST_CAM_DRIVER | false
DRIVER_14_ED_ONCHIP_MEM_ONLY | false
DRIVER_14_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_14_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_14_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_14_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_14_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_14_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_14_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_14_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_14_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_14_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_14_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_14_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_14_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_14_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_14_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_14_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_14_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_14_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_14_MEM_AXI4_AWID_WIDTH | 9
DRIVER_14_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_14_MEM_AXI4_USE_AWLOCK | true
DRIVER_14_MEM_AXI4_USE_AWCACHE | true
DRIVER_14_MEM_AXI4_USE_AWQOS | true
DRIVER_14_MEM_AXI4_USE_AWREGION | true
DRIVER_14_MEM_AXI4_USE_AWUSER | true
DRIVER_14_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_14_MEM_AXI4_ARID_WIDTH | 9
DRIVER_14_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_14_MEM_AXI4_USE_ARLOCK | true
DRIVER_14_MEM_AXI4_USE_ARCACHE | true
DRIVER_14_MEM_AXI4_USE_ARQOS | true
DRIVER_14_MEM_AXI4_USE_ARREGION | true
DRIVER_14_MEM_AXI4_USE_ARUSER | true
DRIVER_14_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_14_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_14_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_14_MEM_AXI4_USE_BUSER | false
DRIVER_14_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_14_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_14_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_15_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_15_CAM_AXIST_KEY_WIDTH | 64
DRIVER_15_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_15_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_15_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_15_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_15_CAM_AXIST_TID_WIDTH | 8
DRIVER_15_CAM_AXIST_PTR_WIDTH | 1
DRIVER_15_CAM_AXIST_LOG2_TABLES | 1
DRIVER_15_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_15_CAM_TEST_CAM | BCAM
DRIVER_15_ED_ASSOC_STORAGE_ONLY | false
DRIVER_15_ED_FIRST_CAM_DRIVER | false
DRIVER_15_ED_ONCHIP_MEM_ONLY | false
DRIVER_15_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_15_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_15_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_15_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_15_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_15_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_15_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_15_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_15_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_15_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_15_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_15_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_15_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_15_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_15_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_15_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_15_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_15_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_15_MEM_AXI4_AWID_WIDTH | 9
DRIVER_15_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_15_MEM_AXI4_USE_AWLOCK | true
DRIVER_15_MEM_AXI4_USE_AWCACHE | true
DRIVER_15_MEM_AXI4_USE_AWQOS | true
DRIVER_15_MEM_AXI4_USE_AWREGION | true
DRIVER_15_MEM_AXI4_USE_AWUSER | true
DRIVER_15_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_15_MEM_AXI4_ARID_WIDTH | 9
DRIVER_15_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_15_MEM_AXI4_USE_ARLOCK | true
DRIVER_15_MEM_AXI4_USE_ARCACHE | true
DRIVER_15_MEM_AXI4_USE_ARQOS | true
DRIVER_15_MEM_AXI4_USE_ARREGION | true
DRIVER_15_MEM_AXI4_USE_ARUSER | true
DRIVER_15_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_15_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_15_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_15_MEM_AXI4_USE_BUSER | false
DRIVER_15_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_15_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_15_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_16_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_16_CAM_AXIST_KEY_WIDTH | 64
DRIVER_16_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_16_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_16_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_16_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_16_CAM_AXIST_TID_WIDTH | 8
DRIVER_16_CAM_AXIST_PTR_WIDTH | 1
DRIVER_16_CAM_AXIST_LOG2_TABLES | 1
DRIVER_16_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_16_CAM_TEST_CAM | BCAM
DRIVER_16_ED_ASSOC_STORAGE_ONLY | false
DRIVER_16_ED_FIRST_CAM_DRIVER | false
DRIVER_16_ED_ONCHIP_MEM_ONLY | false
DRIVER_16_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_16_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_16_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_16_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_16_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_16_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_16_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_16_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_16_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_16_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_16_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_16_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_16_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_16_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_16_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_16_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_16_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_16_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_16_MEM_AXI4_AWID_WIDTH | 9
DRIVER_16_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_16_MEM_AXI4_USE_AWLOCK | true
DRIVER_16_MEM_AXI4_USE_AWCACHE | true
DRIVER_16_MEM_AXI4_USE_AWQOS | true
DRIVER_16_MEM_AXI4_USE_AWREGION | true
DRIVER_16_MEM_AXI4_USE_AWUSER | true
DRIVER_16_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_16_MEM_AXI4_ARID_WIDTH | 9
DRIVER_16_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_16_MEM_AXI4_USE_ARLOCK | true
DRIVER_16_MEM_AXI4_USE_ARCACHE | true
DRIVER_16_MEM_AXI4_USE_ARQOS | true
DRIVER_16_MEM_AXI4_USE_ARREGION | true
DRIVER_16_MEM_AXI4_USE_ARUSER | true
DRIVER_16_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_16_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_16_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_16_MEM_AXI4_USE_BUSER | false
DRIVER_16_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_16_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_16_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_17_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_17_CAM_AXIST_KEY_WIDTH | 64
DRIVER_17_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_17_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_17_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_17_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_17_CAM_AXIST_TID_WIDTH | 8
DRIVER_17_CAM_AXIST_PTR_WIDTH | 1
DRIVER_17_CAM_AXIST_LOG2_TABLES | 1
DRIVER_17_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_17_CAM_TEST_CAM | BCAM
DRIVER_17_ED_ASSOC_STORAGE_ONLY | false
DRIVER_17_ED_FIRST_CAM_DRIVER | false
DRIVER_17_ED_ONCHIP_MEM_ONLY | false
DRIVER_17_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_17_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_17_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_17_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_17_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_17_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_17_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_17_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_17_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_17_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_17_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_17_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_17_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_17_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_17_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_17_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_17_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_17_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_17_MEM_AXI4_AWID_WIDTH | 9
DRIVER_17_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_17_MEM_AXI4_USE_AWLOCK | true
DRIVER_17_MEM_AXI4_USE_AWCACHE | true
DRIVER_17_MEM_AXI4_USE_AWQOS | true
DRIVER_17_MEM_AXI4_USE_AWREGION | true
DRIVER_17_MEM_AXI4_USE_AWUSER | true
DRIVER_17_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_17_MEM_AXI4_ARID_WIDTH | 9
DRIVER_17_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_17_MEM_AXI4_USE_ARLOCK | true
DRIVER_17_MEM_AXI4_USE_ARCACHE | true
DRIVER_17_MEM_AXI4_USE_ARQOS | true
DRIVER_17_MEM_AXI4_USE_ARREGION | true
DRIVER_17_MEM_AXI4_USE_ARUSER | true
DRIVER_17_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_17_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_17_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_17_MEM_AXI4_USE_BUSER | false
DRIVER_17_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_17_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_17_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_18_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_18_CAM_AXIST_KEY_WIDTH | 64
DRIVER_18_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_18_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_18_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_18_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_18_CAM_AXIST_TID_WIDTH | 8
DRIVER_18_CAM_AXIST_PTR_WIDTH | 1
DRIVER_18_CAM_AXIST_LOG2_TABLES | 1
DRIVER_18_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_18_CAM_TEST_CAM | BCAM
DRIVER_18_ED_ASSOC_STORAGE_ONLY | false
DRIVER_18_ED_FIRST_CAM_DRIVER | false
DRIVER_18_ED_ONCHIP_MEM_ONLY | false
DRIVER_18_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_18_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_18_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_18_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_18_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_18_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_18_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_18_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_18_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_18_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_18_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_18_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_18_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_18_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_18_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_18_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_18_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_18_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_18_MEM_AXI4_AWID_WIDTH | 9
DRIVER_18_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_18_MEM_AXI4_USE_AWLOCK | true
DRIVER_18_MEM_AXI4_USE_AWCACHE | true
DRIVER_18_MEM_AXI4_USE_AWQOS | true
DRIVER_18_MEM_AXI4_USE_AWREGION | true
DRIVER_18_MEM_AXI4_USE_AWUSER | true
DRIVER_18_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_18_MEM_AXI4_ARID_WIDTH | 9
DRIVER_18_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_18_MEM_AXI4_USE_ARLOCK | true
DRIVER_18_MEM_AXI4_USE_ARCACHE | true
DRIVER_18_MEM_AXI4_USE_ARQOS | true
DRIVER_18_MEM_AXI4_USE_ARREGION | true
DRIVER_18_MEM_AXI4_USE_ARUSER | true
DRIVER_18_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_18_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_18_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_18_MEM_AXI4_USE_BUSER | false
DRIVER_18_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_18_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_18_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_19_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_19_CAM_AXIST_KEY_WIDTH | 64
DRIVER_19_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_19_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_19_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_19_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_19_CAM_AXIST_TID_WIDTH | 8
DRIVER_19_CAM_AXIST_PTR_WIDTH | 1
DRIVER_19_CAM_AXIST_LOG2_TABLES | 1
DRIVER_19_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_19_CAM_TEST_CAM | BCAM
DRIVER_19_ED_ASSOC_STORAGE_ONLY | false
DRIVER_19_ED_FIRST_CAM_DRIVER | false
DRIVER_19_ED_ONCHIP_MEM_ONLY | false
DRIVER_19_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_19_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_19_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_19_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_19_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_19_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_19_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_19_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_19_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_19_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_19_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_19_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_19_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_19_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_19_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_19_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_19_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_19_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_19_MEM_AXI4_AWID_WIDTH | 9
DRIVER_19_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_19_MEM_AXI4_USE_AWLOCK | true
DRIVER_19_MEM_AXI4_USE_AWCACHE | true
DRIVER_19_MEM_AXI4_USE_AWQOS | true
DRIVER_19_MEM_AXI4_USE_AWREGION | true
DRIVER_19_MEM_AXI4_USE_AWUSER | true
DRIVER_19_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_19_MEM_AXI4_ARID_WIDTH | 9
DRIVER_19_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_19_MEM_AXI4_USE_ARLOCK | true
DRIVER_19_MEM_AXI4_USE_ARCACHE | true
DRIVER_19_MEM_AXI4_USE_ARQOS | true
DRIVER_19_MEM_AXI4_USE_ARREGION | true
DRIVER_19_MEM_AXI4_USE_ARUSER | true
DRIVER_19_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_19_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_19_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_19_MEM_AXI4_USE_BUSER | false
DRIVER_19_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_19_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_19_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_20_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_20_CAM_AXIST_KEY_WIDTH | 64
DRIVER_20_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_20_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_20_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_20_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_20_CAM_AXIST_TID_WIDTH | 8
DRIVER_20_CAM_AXIST_PTR_WIDTH | 1
DRIVER_20_CAM_AXIST_LOG2_TABLES | 1
DRIVER_20_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_20_CAM_TEST_CAM | BCAM
DRIVER_20_ED_ASSOC_STORAGE_ONLY | false
DRIVER_20_ED_FIRST_CAM_DRIVER | false
DRIVER_20_ED_ONCHIP_MEM_ONLY | false
DRIVER_20_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_20_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_20_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_20_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_20_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_20_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_20_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_20_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_20_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_20_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_20_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_20_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_20_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_20_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_20_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_20_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_20_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_20_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_20_MEM_AXI4_AWID_WIDTH | 9
DRIVER_20_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_20_MEM_AXI4_USE_AWLOCK | true
DRIVER_20_MEM_AXI4_USE_AWCACHE | true
DRIVER_20_MEM_AXI4_USE_AWQOS | true
DRIVER_20_MEM_AXI4_USE_AWREGION | true
DRIVER_20_MEM_AXI4_USE_AWUSER | true
DRIVER_20_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_20_MEM_AXI4_ARID_WIDTH | 9
DRIVER_20_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_20_MEM_AXI4_USE_ARLOCK | true
DRIVER_20_MEM_AXI4_USE_ARCACHE | true
DRIVER_20_MEM_AXI4_USE_ARQOS | true
DRIVER_20_MEM_AXI4_USE_ARREGION | true
DRIVER_20_MEM_AXI4_USE_ARUSER | true
DRIVER_20_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_20_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_20_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_20_MEM_AXI4_USE_BUSER | false
DRIVER_20_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_20_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_20_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_21_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_21_CAM_AXIST_KEY_WIDTH | 64
DRIVER_21_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_21_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_21_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_21_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_21_CAM_AXIST_TID_WIDTH | 8
DRIVER_21_CAM_AXIST_PTR_WIDTH | 1
DRIVER_21_CAM_AXIST_LOG2_TABLES | 1
DRIVER_21_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_21_CAM_TEST_CAM | BCAM
DRIVER_21_ED_ASSOC_STORAGE_ONLY | false
DRIVER_21_ED_FIRST_CAM_DRIVER | false
DRIVER_21_ED_ONCHIP_MEM_ONLY | false
DRIVER_21_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_21_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_21_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_21_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_21_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_21_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_21_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_21_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_21_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_21_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_21_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_21_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_21_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_21_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_21_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_21_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_21_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_21_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_21_MEM_AXI4_AWID_WIDTH | 9
DRIVER_21_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_21_MEM_AXI4_USE_AWLOCK | true
DRIVER_21_MEM_AXI4_USE_AWCACHE | true
DRIVER_21_MEM_AXI4_USE_AWQOS | true
DRIVER_21_MEM_AXI4_USE_AWREGION | true
DRIVER_21_MEM_AXI4_USE_AWUSER | true
DRIVER_21_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_21_MEM_AXI4_ARID_WIDTH | 9
DRIVER_21_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_21_MEM_AXI4_USE_ARLOCK | true
DRIVER_21_MEM_AXI4_USE_ARCACHE | true
DRIVER_21_MEM_AXI4_USE_ARQOS | true
DRIVER_21_MEM_AXI4_USE_ARREGION | true
DRIVER_21_MEM_AXI4_USE_ARUSER | true
DRIVER_21_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_21_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_21_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_21_MEM_AXI4_USE_BUSER | false
DRIVER_21_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_21_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_21_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_22_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_22_CAM_AXIST_KEY_WIDTH | 64
DRIVER_22_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_22_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_22_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_22_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_22_CAM_AXIST_TID_WIDTH | 8
DRIVER_22_CAM_AXIST_PTR_WIDTH | 1
DRIVER_22_CAM_AXIST_LOG2_TABLES | 1
DRIVER_22_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_22_CAM_TEST_CAM | BCAM
DRIVER_22_ED_ASSOC_STORAGE_ONLY | false
DRIVER_22_ED_FIRST_CAM_DRIVER | false
DRIVER_22_ED_ONCHIP_MEM_ONLY | false
DRIVER_22_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_22_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_22_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_22_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_22_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_22_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_22_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_22_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_22_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_22_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_22_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_22_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_22_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_22_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_22_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_22_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_22_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_22_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_22_MEM_AXI4_AWID_WIDTH | 9
DRIVER_22_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_22_MEM_AXI4_USE_AWLOCK | true
DRIVER_22_MEM_AXI4_USE_AWCACHE | true
DRIVER_22_MEM_AXI4_USE_AWQOS | true
DRIVER_22_MEM_AXI4_USE_AWREGION | true
DRIVER_22_MEM_AXI4_USE_AWUSER | true
DRIVER_22_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_22_MEM_AXI4_ARID_WIDTH | 9
DRIVER_22_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_22_MEM_AXI4_USE_ARLOCK | true
DRIVER_22_MEM_AXI4_USE_ARCACHE | true
DRIVER_22_MEM_AXI4_USE_ARQOS | true
DRIVER_22_MEM_AXI4_USE_ARREGION | true
DRIVER_22_MEM_AXI4_USE_ARUSER | true
DRIVER_22_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_22_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_22_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_22_MEM_AXI4_USE_BUSER | false
DRIVER_22_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_22_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_22_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_23_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_23_CAM_AXIST_KEY_WIDTH | 64
DRIVER_23_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_23_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_23_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_23_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_23_CAM_AXIST_TID_WIDTH | 8
DRIVER_23_CAM_AXIST_PTR_WIDTH | 1
DRIVER_23_CAM_AXIST_LOG2_TABLES | 1
DRIVER_23_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_23_CAM_TEST_CAM | BCAM
DRIVER_23_ED_ASSOC_STORAGE_ONLY | false
DRIVER_23_ED_FIRST_CAM_DRIVER | false
DRIVER_23_ED_ONCHIP_MEM_ONLY | false
DRIVER_23_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_23_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_23_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_23_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_23_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_23_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_23_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_23_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_23_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_23_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_23_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_23_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_23_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_23_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_23_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_23_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_23_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_23_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_23_MEM_AXI4_AWID_WIDTH | 9
DRIVER_23_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_23_MEM_AXI4_USE_AWLOCK | true
DRIVER_23_MEM_AXI4_USE_AWCACHE | true
DRIVER_23_MEM_AXI4_USE_AWQOS | true
DRIVER_23_MEM_AXI4_USE_AWREGION | true
DRIVER_23_MEM_AXI4_USE_AWUSER | true
DRIVER_23_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_23_MEM_AXI4_ARID_WIDTH | 9
DRIVER_23_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_23_MEM_AXI4_USE_ARLOCK | true
DRIVER_23_MEM_AXI4_USE_ARCACHE | true
DRIVER_23_MEM_AXI4_USE_ARQOS | true
DRIVER_23_MEM_AXI4_USE_ARREGION | true
DRIVER_23_MEM_AXI4_USE_ARUSER | true
DRIVER_23_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_23_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_23_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_23_MEM_AXI4_USE_BUSER | false
DRIVER_23_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_23_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_23_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_24_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_24_CAM_AXIST_KEY_WIDTH | 64
DRIVER_24_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_24_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_24_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_24_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_24_CAM_AXIST_TID_WIDTH | 8
DRIVER_24_CAM_AXIST_PTR_WIDTH | 1
DRIVER_24_CAM_AXIST_LOG2_TABLES | 1
DRIVER_24_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_24_CAM_TEST_CAM | BCAM
DRIVER_24_ED_ASSOC_STORAGE_ONLY | false
DRIVER_24_ED_FIRST_CAM_DRIVER | false
DRIVER_24_ED_ONCHIP_MEM_ONLY | false
DRIVER_24_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_24_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_24_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_24_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_24_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_24_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_24_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_24_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_24_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_24_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_24_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_24_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_24_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_24_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_24_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_24_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_24_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_24_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_24_MEM_AXI4_AWID_WIDTH | 9
DRIVER_24_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_24_MEM_AXI4_USE_AWLOCK | true
DRIVER_24_MEM_AXI4_USE_AWCACHE | true
DRIVER_24_MEM_AXI4_USE_AWQOS | true
DRIVER_24_MEM_AXI4_USE_AWREGION | true
DRIVER_24_MEM_AXI4_USE_AWUSER | true
DRIVER_24_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_24_MEM_AXI4_ARID_WIDTH | 9
DRIVER_24_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_24_MEM_AXI4_USE_ARLOCK | true
DRIVER_24_MEM_AXI4_USE_ARCACHE | true
DRIVER_24_MEM_AXI4_USE_ARQOS | true
DRIVER_24_MEM_AXI4_USE_ARREGION | true
DRIVER_24_MEM_AXI4_USE_ARUSER | true
DRIVER_24_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_24_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_24_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_24_MEM_AXI4_USE_BUSER | false
DRIVER_24_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_24_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_24_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_25_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_25_CAM_AXIST_KEY_WIDTH | 64
DRIVER_25_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_25_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_25_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_25_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_25_CAM_AXIST_TID_WIDTH | 8
DRIVER_25_CAM_AXIST_PTR_WIDTH | 1
DRIVER_25_CAM_AXIST_LOG2_TABLES | 1
DRIVER_25_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_25_CAM_TEST_CAM | BCAM
DRIVER_25_ED_ASSOC_STORAGE_ONLY | false
DRIVER_25_ED_FIRST_CAM_DRIVER | false
DRIVER_25_ED_ONCHIP_MEM_ONLY | false
DRIVER_25_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_25_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_25_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_25_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_25_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_25_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_25_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_25_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_25_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_25_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_25_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_25_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_25_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_25_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_25_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_25_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_25_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_25_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_25_MEM_AXI4_AWID_WIDTH | 9
DRIVER_25_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_25_MEM_AXI4_USE_AWLOCK | true
DRIVER_25_MEM_AXI4_USE_AWCACHE | true
DRIVER_25_MEM_AXI4_USE_AWQOS | true
DRIVER_25_MEM_AXI4_USE_AWREGION | true
DRIVER_25_MEM_AXI4_USE_AWUSER | true
DRIVER_25_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_25_MEM_AXI4_ARID_WIDTH | 9
DRIVER_25_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_25_MEM_AXI4_USE_ARLOCK | true
DRIVER_25_MEM_AXI4_USE_ARCACHE | true
DRIVER_25_MEM_AXI4_USE_ARQOS | true
DRIVER_25_MEM_AXI4_USE_ARREGION | true
DRIVER_25_MEM_AXI4_USE_ARUSER | true
DRIVER_25_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_25_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_25_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_25_MEM_AXI4_USE_BUSER | false
DRIVER_25_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_25_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_25_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_26_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_26_CAM_AXIST_KEY_WIDTH | 64
DRIVER_26_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_26_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_26_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_26_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_26_CAM_AXIST_TID_WIDTH | 8
DRIVER_26_CAM_AXIST_PTR_WIDTH | 1
DRIVER_26_CAM_AXIST_LOG2_TABLES | 1
DRIVER_26_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_26_CAM_TEST_CAM | BCAM
DRIVER_26_ED_ASSOC_STORAGE_ONLY | false
DRIVER_26_ED_FIRST_CAM_DRIVER | false
DRIVER_26_ED_ONCHIP_MEM_ONLY | false
DRIVER_26_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_26_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_26_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_26_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_26_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_26_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_26_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_26_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_26_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_26_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_26_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_26_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_26_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_26_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_26_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_26_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_26_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_26_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_26_MEM_AXI4_AWID_WIDTH | 9
DRIVER_26_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_26_MEM_AXI4_USE_AWLOCK | true
DRIVER_26_MEM_AXI4_USE_AWCACHE | true
DRIVER_26_MEM_AXI4_USE_AWQOS | true
DRIVER_26_MEM_AXI4_USE_AWREGION | true
DRIVER_26_MEM_AXI4_USE_AWUSER | true
DRIVER_26_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_26_MEM_AXI4_ARID_WIDTH | 9
DRIVER_26_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_26_MEM_AXI4_USE_ARLOCK | true
DRIVER_26_MEM_AXI4_USE_ARCACHE | true
DRIVER_26_MEM_AXI4_USE_ARQOS | true
DRIVER_26_MEM_AXI4_USE_ARREGION | true
DRIVER_26_MEM_AXI4_USE_ARUSER | true
DRIVER_26_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_26_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_26_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_26_MEM_AXI4_USE_BUSER | false
DRIVER_26_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_26_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_26_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_27_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_27_CAM_AXIST_KEY_WIDTH | 64
DRIVER_27_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_27_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_27_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_27_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_27_CAM_AXIST_TID_WIDTH | 8
DRIVER_27_CAM_AXIST_PTR_WIDTH | 1
DRIVER_27_CAM_AXIST_LOG2_TABLES | 1
DRIVER_27_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_27_CAM_TEST_CAM | BCAM
DRIVER_27_ED_ASSOC_STORAGE_ONLY | false
DRIVER_27_ED_FIRST_CAM_DRIVER | false
DRIVER_27_ED_ONCHIP_MEM_ONLY | false
DRIVER_27_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_27_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_27_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_27_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_27_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_27_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_27_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_27_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_27_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_27_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_27_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_27_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_27_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_27_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_27_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_27_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_27_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_27_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_27_MEM_AXI4_AWID_WIDTH | 9
DRIVER_27_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_27_MEM_AXI4_USE_AWLOCK | true
DRIVER_27_MEM_AXI4_USE_AWCACHE | true
DRIVER_27_MEM_AXI4_USE_AWQOS | true
DRIVER_27_MEM_AXI4_USE_AWREGION | true
DRIVER_27_MEM_AXI4_USE_AWUSER | true
DRIVER_27_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_27_MEM_AXI4_ARID_WIDTH | 9
DRIVER_27_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_27_MEM_AXI4_USE_ARLOCK | true
DRIVER_27_MEM_AXI4_USE_ARCACHE | true
DRIVER_27_MEM_AXI4_USE_ARQOS | true
DRIVER_27_MEM_AXI4_USE_ARREGION | true
DRIVER_27_MEM_AXI4_USE_ARUSER | true
DRIVER_27_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_27_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_27_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_27_MEM_AXI4_USE_BUSER | false
DRIVER_27_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_27_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_27_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_28_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_28_CAM_AXIST_KEY_WIDTH | 64
DRIVER_28_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_28_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_28_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_28_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_28_CAM_AXIST_TID_WIDTH | 8
DRIVER_28_CAM_AXIST_PTR_WIDTH | 1
DRIVER_28_CAM_AXIST_LOG2_TABLES | 1
DRIVER_28_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_28_CAM_TEST_CAM | BCAM
DRIVER_28_ED_ASSOC_STORAGE_ONLY | false
DRIVER_28_ED_FIRST_CAM_DRIVER | false
DRIVER_28_ED_ONCHIP_MEM_ONLY | false
DRIVER_28_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_28_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_28_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_28_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_28_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_28_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_28_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_28_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_28_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_28_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_28_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_28_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_28_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_28_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_28_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_28_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_28_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_28_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_28_MEM_AXI4_AWID_WIDTH | 9
DRIVER_28_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_28_MEM_AXI4_USE_AWLOCK | true
DRIVER_28_MEM_AXI4_USE_AWCACHE | true
DRIVER_28_MEM_AXI4_USE_AWQOS | true
DRIVER_28_MEM_AXI4_USE_AWREGION | true
DRIVER_28_MEM_AXI4_USE_AWUSER | true
DRIVER_28_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_28_MEM_AXI4_ARID_WIDTH | 9
DRIVER_28_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_28_MEM_AXI4_USE_ARLOCK | true
DRIVER_28_MEM_AXI4_USE_ARCACHE | true
DRIVER_28_MEM_AXI4_USE_ARQOS | true
DRIVER_28_MEM_AXI4_USE_ARREGION | true
DRIVER_28_MEM_AXI4_USE_ARUSER | true
DRIVER_28_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_28_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_28_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_28_MEM_AXI4_USE_BUSER | false
DRIVER_28_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_28_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_28_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_29_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_29_CAM_AXIST_KEY_WIDTH | 64
DRIVER_29_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_29_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_29_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_29_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_29_CAM_AXIST_TID_WIDTH | 8
DRIVER_29_CAM_AXIST_PTR_WIDTH | 1
DRIVER_29_CAM_AXIST_LOG2_TABLES | 1
DRIVER_29_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_29_CAM_TEST_CAM | BCAM
DRIVER_29_ED_ASSOC_STORAGE_ONLY | false
DRIVER_29_ED_FIRST_CAM_DRIVER | false
DRIVER_29_ED_ONCHIP_MEM_ONLY | false
DRIVER_29_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_29_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_29_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_29_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_29_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_29_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_29_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_29_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_29_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_29_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_29_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_29_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_29_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_29_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_29_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_29_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_29_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_29_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_29_MEM_AXI4_AWID_WIDTH | 9
DRIVER_29_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_29_MEM_AXI4_USE_AWLOCK | true
DRIVER_29_MEM_AXI4_USE_AWCACHE | true
DRIVER_29_MEM_AXI4_USE_AWQOS | true
DRIVER_29_MEM_AXI4_USE_AWREGION | true
DRIVER_29_MEM_AXI4_USE_AWUSER | true
DRIVER_29_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_29_MEM_AXI4_ARID_WIDTH | 9
DRIVER_29_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_29_MEM_AXI4_USE_ARLOCK | true
DRIVER_29_MEM_AXI4_USE_ARCACHE | true
DRIVER_29_MEM_AXI4_USE_ARQOS | true
DRIVER_29_MEM_AXI4_USE_ARREGION | true
DRIVER_29_MEM_AXI4_USE_ARUSER | true
DRIVER_29_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_29_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_29_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_29_MEM_AXI4_USE_BUSER | false
DRIVER_29_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_29_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_29_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_30_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_30_CAM_AXIST_KEY_WIDTH | 64
DRIVER_30_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_30_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_30_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_30_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_30_CAM_AXIST_TID_WIDTH | 8
DRIVER_30_CAM_AXIST_PTR_WIDTH | 1
DRIVER_30_CAM_AXIST_LOG2_TABLES | 1
DRIVER_30_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_30_CAM_TEST_CAM | BCAM
DRIVER_30_ED_ASSOC_STORAGE_ONLY | false
DRIVER_30_ED_FIRST_CAM_DRIVER | false
DRIVER_30_ED_ONCHIP_MEM_ONLY | false
DRIVER_30_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_30_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_30_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_30_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_30_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_30_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_30_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_30_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_30_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_30_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_30_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_30_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_30_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_30_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_30_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_30_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_30_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_30_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_30_MEM_AXI4_AWID_WIDTH | 9
DRIVER_30_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_30_MEM_AXI4_USE_AWLOCK | true
DRIVER_30_MEM_AXI4_USE_AWCACHE | true
DRIVER_30_MEM_AXI4_USE_AWQOS | true
DRIVER_30_MEM_AXI4_USE_AWREGION | true
DRIVER_30_MEM_AXI4_USE_AWUSER | true
DRIVER_30_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_30_MEM_AXI4_ARID_WIDTH | 9
DRIVER_30_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_30_MEM_AXI4_USE_ARLOCK | true
DRIVER_30_MEM_AXI4_USE_ARCACHE | true
DRIVER_30_MEM_AXI4_USE_ARQOS | true
DRIVER_30_MEM_AXI4_USE_ARREGION | true
DRIVER_30_MEM_AXI4_USE_ARUSER | true
DRIVER_30_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_30_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_30_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_30_MEM_AXI4_USE_BUSER | false
DRIVER_30_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_30_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_30_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_31_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_31_CAM_AXIST_KEY_WIDTH | 64
DRIVER_31_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_31_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_31_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_31_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_31_CAM_AXIST_TID_WIDTH | 8
DRIVER_31_CAM_AXIST_PTR_WIDTH | 1
DRIVER_31_CAM_AXIST_LOG2_TABLES | 1
DRIVER_31_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_31_CAM_TEST_CAM | BCAM
DRIVER_31_ED_ASSOC_STORAGE_ONLY | false
DRIVER_31_ED_FIRST_CAM_DRIVER | false
DRIVER_31_ED_ONCHIP_MEM_ONLY | false
DRIVER_31_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_31_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_31_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_31_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_31_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_31_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_31_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_31_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_31_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_31_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_31_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_31_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_31_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_31_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_31_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_31_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_31_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_31_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_31_MEM_AXI4_AWID_WIDTH | 9
DRIVER_31_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_31_MEM_AXI4_USE_AWLOCK | true
DRIVER_31_MEM_AXI4_USE_AWCACHE | true
DRIVER_31_MEM_AXI4_USE_AWQOS | true
DRIVER_31_MEM_AXI4_USE_AWREGION | true
DRIVER_31_MEM_AXI4_USE_AWUSER | true
DRIVER_31_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_31_MEM_AXI4_ARID_WIDTH | 9
DRIVER_31_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_31_MEM_AXI4_USE_ARLOCK | true
DRIVER_31_MEM_AXI4_USE_ARCACHE | true
DRIVER_31_MEM_AXI4_USE_ARQOS | true
DRIVER_31_MEM_AXI4_USE_ARREGION | true
DRIVER_31_MEM_AXI4_USE_ARUSER | true
DRIVER_31_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_31_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_31_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_31_MEM_AXI4_USE_BUSER | false
DRIVER_31_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_31_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_31_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_32_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_32_CAM_AXIST_KEY_WIDTH | 64
DRIVER_32_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_32_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_32_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_32_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_32_CAM_AXIST_TID_WIDTH | 8
DRIVER_32_CAM_AXIST_PTR_WIDTH | 1
DRIVER_32_CAM_AXIST_LOG2_TABLES | 1
DRIVER_32_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_32_CAM_TEST_CAM | BCAM
DRIVER_32_ED_ASSOC_STORAGE_ONLY | false
DRIVER_32_ED_FIRST_CAM_DRIVER | false
DRIVER_32_ED_ONCHIP_MEM_ONLY | false
DRIVER_32_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_32_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_32_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_32_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_32_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_32_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_32_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_32_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_32_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_32_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_32_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_32_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_32_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_32_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_32_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_32_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_32_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_32_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_32_MEM_AXI4_AWID_WIDTH | 9
DRIVER_32_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_32_MEM_AXI4_USE_AWLOCK | true
DRIVER_32_MEM_AXI4_USE_AWCACHE | true
DRIVER_32_MEM_AXI4_USE_AWQOS | true
DRIVER_32_MEM_AXI4_USE_AWREGION | true
DRIVER_32_MEM_AXI4_USE_AWUSER | true
DRIVER_32_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_32_MEM_AXI4_ARID_WIDTH | 9
DRIVER_32_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_32_MEM_AXI4_USE_ARLOCK | true
DRIVER_32_MEM_AXI4_USE_ARCACHE | true
DRIVER_32_MEM_AXI4_USE_ARQOS | true
DRIVER_32_MEM_AXI4_USE_ARREGION | true
DRIVER_32_MEM_AXI4_USE_ARUSER | true
DRIVER_32_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_32_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_32_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_32_MEM_AXI4_USE_BUSER | false
DRIVER_32_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_32_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_32_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_33_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_33_CAM_AXIST_KEY_WIDTH | 64
DRIVER_33_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_33_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_33_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_33_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_33_CAM_AXIST_TID_WIDTH | 8
DRIVER_33_CAM_AXIST_PTR_WIDTH | 1
DRIVER_33_CAM_AXIST_LOG2_TABLES | 1
DRIVER_33_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_33_CAM_TEST_CAM | BCAM
DRIVER_33_ED_ASSOC_STORAGE_ONLY | false
DRIVER_33_ED_FIRST_CAM_DRIVER | false
DRIVER_33_ED_ONCHIP_MEM_ONLY | false
DRIVER_33_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_33_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_33_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_33_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_33_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_33_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_33_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_33_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_33_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_33_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_33_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_33_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_33_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_33_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_33_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_33_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_33_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_33_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_33_MEM_AXI4_AWID_WIDTH | 9
DRIVER_33_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_33_MEM_AXI4_USE_AWLOCK | true
DRIVER_33_MEM_AXI4_USE_AWCACHE | true
DRIVER_33_MEM_AXI4_USE_AWQOS | true
DRIVER_33_MEM_AXI4_USE_AWREGION | true
DRIVER_33_MEM_AXI4_USE_AWUSER | true
DRIVER_33_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_33_MEM_AXI4_ARID_WIDTH | 9
DRIVER_33_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_33_MEM_AXI4_USE_ARLOCK | true
DRIVER_33_MEM_AXI4_USE_ARCACHE | true
DRIVER_33_MEM_AXI4_USE_ARQOS | true
DRIVER_33_MEM_AXI4_USE_ARREGION | true
DRIVER_33_MEM_AXI4_USE_ARUSER | true
DRIVER_33_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_33_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_33_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_33_MEM_AXI4_USE_BUSER | false
DRIVER_33_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_33_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_33_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_34_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_34_CAM_AXIST_KEY_WIDTH | 64
DRIVER_34_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_34_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_34_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_34_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_34_CAM_AXIST_TID_WIDTH | 8
DRIVER_34_CAM_AXIST_PTR_WIDTH | 1
DRIVER_34_CAM_AXIST_LOG2_TABLES | 1
DRIVER_34_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_34_CAM_TEST_CAM | BCAM
DRIVER_34_ED_ASSOC_STORAGE_ONLY | false
DRIVER_34_ED_FIRST_CAM_DRIVER | false
DRIVER_34_ED_ONCHIP_MEM_ONLY | false
DRIVER_34_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_34_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_34_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_34_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_34_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_34_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_34_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_34_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_34_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_34_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_34_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_34_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_34_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_34_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_34_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_34_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_34_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_34_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_34_MEM_AXI4_AWID_WIDTH | 9
DRIVER_34_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_34_MEM_AXI4_USE_AWLOCK | true
DRIVER_34_MEM_AXI4_USE_AWCACHE | true
DRIVER_34_MEM_AXI4_USE_AWQOS | true
DRIVER_34_MEM_AXI4_USE_AWREGION | true
DRIVER_34_MEM_AXI4_USE_AWUSER | true
DRIVER_34_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_34_MEM_AXI4_ARID_WIDTH | 9
DRIVER_34_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_34_MEM_AXI4_USE_ARLOCK | true
DRIVER_34_MEM_AXI4_USE_ARCACHE | true
DRIVER_34_MEM_AXI4_USE_ARQOS | true
DRIVER_34_MEM_AXI4_USE_ARREGION | true
DRIVER_34_MEM_AXI4_USE_ARUSER | true
DRIVER_34_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_34_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_34_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_34_MEM_AXI4_USE_BUSER | false
DRIVER_34_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_34_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_34_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_35_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_35_CAM_AXIST_KEY_WIDTH | 64
DRIVER_35_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_35_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_35_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_35_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_35_CAM_AXIST_TID_WIDTH | 8
DRIVER_35_CAM_AXIST_PTR_WIDTH | 1
DRIVER_35_CAM_AXIST_LOG2_TABLES | 1
DRIVER_35_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_35_CAM_TEST_CAM | BCAM
DRIVER_35_ED_ASSOC_STORAGE_ONLY | false
DRIVER_35_ED_FIRST_CAM_DRIVER | false
DRIVER_35_ED_ONCHIP_MEM_ONLY | false
DRIVER_35_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_35_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_35_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_35_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_35_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_35_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_35_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_35_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_35_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_35_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_35_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_35_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_35_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_35_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_35_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_35_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_35_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_35_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_35_MEM_AXI4_AWID_WIDTH | 9
DRIVER_35_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_35_MEM_AXI4_USE_AWLOCK | true
DRIVER_35_MEM_AXI4_USE_AWCACHE | true
DRIVER_35_MEM_AXI4_USE_AWQOS | true
DRIVER_35_MEM_AXI4_USE_AWREGION | true
DRIVER_35_MEM_AXI4_USE_AWUSER | true
DRIVER_35_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_35_MEM_AXI4_ARID_WIDTH | 9
DRIVER_35_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_35_MEM_AXI4_USE_ARLOCK | true
DRIVER_35_MEM_AXI4_USE_ARCACHE | true
DRIVER_35_MEM_AXI4_USE_ARQOS | true
DRIVER_35_MEM_AXI4_USE_ARREGION | true
DRIVER_35_MEM_AXI4_USE_ARUSER | true
DRIVER_35_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_35_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_35_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_35_MEM_AXI4_USE_BUSER | false
DRIVER_35_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_35_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_35_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_36_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_36_CAM_AXIST_KEY_WIDTH | 64
DRIVER_36_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_36_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_36_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_36_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_36_CAM_AXIST_TID_WIDTH | 8
DRIVER_36_CAM_AXIST_PTR_WIDTH | 1
DRIVER_36_CAM_AXIST_LOG2_TABLES | 1
DRIVER_36_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_36_CAM_TEST_CAM | BCAM
DRIVER_36_ED_ASSOC_STORAGE_ONLY | false
DRIVER_36_ED_FIRST_CAM_DRIVER | false
DRIVER_36_ED_ONCHIP_MEM_ONLY | false
DRIVER_36_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_36_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_36_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_36_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_36_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_36_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_36_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_36_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_36_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_36_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_36_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_36_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_36_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_36_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_36_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_36_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_36_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_36_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_36_MEM_AXI4_AWID_WIDTH | 9
DRIVER_36_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_36_MEM_AXI4_USE_AWLOCK | true
DRIVER_36_MEM_AXI4_USE_AWCACHE | true
DRIVER_36_MEM_AXI4_USE_AWQOS | true
DRIVER_36_MEM_AXI4_USE_AWREGION | true
DRIVER_36_MEM_AXI4_USE_AWUSER | true
DRIVER_36_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_36_MEM_AXI4_ARID_WIDTH | 9
DRIVER_36_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_36_MEM_AXI4_USE_ARLOCK | true
DRIVER_36_MEM_AXI4_USE_ARCACHE | true
DRIVER_36_MEM_AXI4_USE_ARQOS | true
DRIVER_36_MEM_AXI4_USE_ARREGION | true
DRIVER_36_MEM_AXI4_USE_ARUSER | true
DRIVER_36_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_36_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_36_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_36_MEM_AXI4_USE_BUSER | false
DRIVER_36_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_36_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_36_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_37_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_37_CAM_AXIST_KEY_WIDTH | 64
DRIVER_37_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_37_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_37_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_37_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_37_CAM_AXIST_TID_WIDTH | 8
DRIVER_37_CAM_AXIST_PTR_WIDTH | 1
DRIVER_37_CAM_AXIST_LOG2_TABLES | 1
DRIVER_37_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_37_CAM_TEST_CAM | BCAM
DRIVER_37_ED_ASSOC_STORAGE_ONLY | false
DRIVER_37_ED_FIRST_CAM_DRIVER | false
DRIVER_37_ED_ONCHIP_MEM_ONLY | false
DRIVER_37_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_37_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_37_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_37_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_37_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_37_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_37_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_37_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_37_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_37_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_37_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_37_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_37_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_37_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_37_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_37_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_37_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_37_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_37_MEM_AXI4_AWID_WIDTH | 9
DRIVER_37_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_37_MEM_AXI4_USE_AWLOCK | true
DRIVER_37_MEM_AXI4_USE_AWCACHE | true
DRIVER_37_MEM_AXI4_USE_AWQOS | true
DRIVER_37_MEM_AXI4_USE_AWREGION | true
DRIVER_37_MEM_AXI4_USE_AWUSER | true
DRIVER_37_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_37_MEM_AXI4_ARID_WIDTH | 9
DRIVER_37_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_37_MEM_AXI4_USE_ARLOCK | true
DRIVER_37_MEM_AXI4_USE_ARCACHE | true
DRIVER_37_MEM_AXI4_USE_ARQOS | true
DRIVER_37_MEM_AXI4_USE_ARREGION | true
DRIVER_37_MEM_AXI4_USE_ARUSER | true
DRIVER_37_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_37_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_37_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_37_MEM_AXI4_USE_BUSER | false
DRIVER_37_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_37_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_37_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_38_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_38_CAM_AXIST_KEY_WIDTH | 64
DRIVER_38_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_38_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_38_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_38_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_38_CAM_AXIST_TID_WIDTH | 8
DRIVER_38_CAM_AXIST_PTR_WIDTH | 1
DRIVER_38_CAM_AXIST_LOG2_TABLES | 1
DRIVER_38_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_38_CAM_TEST_CAM | BCAM
DRIVER_38_ED_ASSOC_STORAGE_ONLY | false
DRIVER_38_ED_FIRST_CAM_DRIVER | false
DRIVER_38_ED_ONCHIP_MEM_ONLY | false
DRIVER_38_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_38_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_38_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_38_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_38_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_38_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_38_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_38_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_38_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_38_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_38_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_38_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_38_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_38_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_38_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_38_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_38_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_38_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_38_MEM_AXI4_AWID_WIDTH | 9
DRIVER_38_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_38_MEM_AXI4_USE_AWLOCK | true
DRIVER_38_MEM_AXI4_USE_AWCACHE | true
DRIVER_38_MEM_AXI4_USE_AWQOS | true
DRIVER_38_MEM_AXI4_USE_AWREGION | true
DRIVER_38_MEM_AXI4_USE_AWUSER | true
DRIVER_38_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_38_MEM_AXI4_ARID_WIDTH | 9
DRIVER_38_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_38_MEM_AXI4_USE_ARLOCK | true
DRIVER_38_MEM_AXI4_USE_ARCACHE | true
DRIVER_38_MEM_AXI4_USE_ARQOS | true
DRIVER_38_MEM_AXI4_USE_ARREGION | true
DRIVER_38_MEM_AXI4_USE_ARUSER | true
DRIVER_38_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_38_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_38_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_38_MEM_AXI4_USE_BUSER | false
DRIVER_38_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_38_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_38_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_39_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_39_CAM_AXIST_KEY_WIDTH | 64
DRIVER_39_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_39_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_39_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_39_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_39_CAM_AXIST_TID_WIDTH | 8
DRIVER_39_CAM_AXIST_PTR_WIDTH | 1
DRIVER_39_CAM_AXIST_LOG2_TABLES | 1
DRIVER_39_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_39_CAM_TEST_CAM | BCAM
DRIVER_39_ED_ASSOC_STORAGE_ONLY | false
DRIVER_39_ED_FIRST_CAM_DRIVER | false
DRIVER_39_ED_ONCHIP_MEM_ONLY | false
DRIVER_39_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_39_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_39_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_39_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_39_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_39_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_39_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_39_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_39_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_39_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_39_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_39_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_39_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_39_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_39_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_39_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_39_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_39_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_39_MEM_AXI4_AWID_WIDTH | 9
DRIVER_39_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_39_MEM_AXI4_USE_AWLOCK | true
DRIVER_39_MEM_AXI4_USE_AWCACHE | true
DRIVER_39_MEM_AXI4_USE_AWQOS | true
DRIVER_39_MEM_AXI4_USE_AWREGION | true
DRIVER_39_MEM_AXI4_USE_AWUSER | true
DRIVER_39_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_39_MEM_AXI4_ARID_WIDTH | 9
DRIVER_39_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_39_MEM_AXI4_USE_ARLOCK | true
DRIVER_39_MEM_AXI4_USE_ARCACHE | true
DRIVER_39_MEM_AXI4_USE_ARQOS | true
DRIVER_39_MEM_AXI4_USE_ARREGION | true
DRIVER_39_MEM_AXI4_USE_ARUSER | true
DRIVER_39_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_39_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_39_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_39_MEM_AXI4_USE_BUSER | false
DRIVER_39_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_39_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_39_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_40_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_40_CAM_AXIST_KEY_WIDTH | 64
DRIVER_40_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_40_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_40_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_40_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_40_CAM_AXIST_TID_WIDTH | 8
DRIVER_40_CAM_AXIST_PTR_WIDTH | 1
DRIVER_40_CAM_AXIST_LOG2_TABLES | 1
DRIVER_40_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_40_CAM_TEST_CAM | BCAM
DRIVER_40_ED_ASSOC_STORAGE_ONLY | false
DRIVER_40_ED_FIRST_CAM_DRIVER | false
DRIVER_40_ED_ONCHIP_MEM_ONLY | false
DRIVER_40_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_40_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_40_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_40_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_40_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_40_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_40_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_40_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_40_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_40_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_40_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_40_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_40_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_40_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_40_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_40_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_40_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_40_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_40_MEM_AXI4_AWID_WIDTH | 9
DRIVER_40_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_40_MEM_AXI4_USE_AWLOCK | true
DRIVER_40_MEM_AXI4_USE_AWCACHE | true
DRIVER_40_MEM_AXI4_USE_AWQOS | true
DRIVER_40_MEM_AXI4_USE_AWREGION | true
DRIVER_40_MEM_AXI4_USE_AWUSER | true
DRIVER_40_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_40_MEM_AXI4_ARID_WIDTH | 9
DRIVER_40_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_40_MEM_AXI4_USE_ARLOCK | true
DRIVER_40_MEM_AXI4_USE_ARCACHE | true
DRIVER_40_MEM_AXI4_USE_ARQOS | true
DRIVER_40_MEM_AXI4_USE_ARREGION | true
DRIVER_40_MEM_AXI4_USE_ARUSER | true
DRIVER_40_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_40_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_40_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_40_MEM_AXI4_USE_BUSER | false
DRIVER_40_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_40_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_40_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_41_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_41_CAM_AXIST_KEY_WIDTH | 64
DRIVER_41_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_41_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_41_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_41_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_41_CAM_AXIST_TID_WIDTH | 8
DRIVER_41_CAM_AXIST_PTR_WIDTH | 1
DRIVER_41_CAM_AXIST_LOG2_TABLES | 1
DRIVER_41_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_41_CAM_TEST_CAM | BCAM
DRIVER_41_ED_ASSOC_STORAGE_ONLY | false
DRIVER_41_ED_FIRST_CAM_DRIVER | false
DRIVER_41_ED_ONCHIP_MEM_ONLY | false
DRIVER_41_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_41_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_41_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_41_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_41_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_41_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_41_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_41_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_41_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_41_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_41_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_41_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_41_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_41_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_41_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_41_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_41_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_41_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_41_MEM_AXI4_AWID_WIDTH | 9
DRIVER_41_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_41_MEM_AXI4_USE_AWLOCK | true
DRIVER_41_MEM_AXI4_USE_AWCACHE | true
DRIVER_41_MEM_AXI4_USE_AWQOS | true
DRIVER_41_MEM_AXI4_USE_AWREGION | true
DRIVER_41_MEM_AXI4_USE_AWUSER | true
DRIVER_41_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_41_MEM_AXI4_ARID_WIDTH | 9
DRIVER_41_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_41_MEM_AXI4_USE_ARLOCK | true
DRIVER_41_MEM_AXI4_USE_ARCACHE | true
DRIVER_41_MEM_AXI4_USE_ARQOS | true
DRIVER_41_MEM_AXI4_USE_ARREGION | true
DRIVER_41_MEM_AXI4_USE_ARUSER | true
DRIVER_41_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_41_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_41_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_41_MEM_AXI4_USE_BUSER | false
DRIVER_41_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_41_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_41_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_42_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_42_CAM_AXIST_KEY_WIDTH | 64
DRIVER_42_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_42_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_42_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_42_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_42_CAM_AXIST_TID_WIDTH | 8
DRIVER_42_CAM_AXIST_PTR_WIDTH | 1
DRIVER_42_CAM_AXIST_LOG2_TABLES | 1
DRIVER_42_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_42_CAM_TEST_CAM | BCAM
DRIVER_42_ED_ASSOC_STORAGE_ONLY | false
DRIVER_42_ED_FIRST_CAM_DRIVER | false
DRIVER_42_ED_ONCHIP_MEM_ONLY | false
DRIVER_42_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_42_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_42_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_42_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_42_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_42_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_42_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_42_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_42_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_42_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_42_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_42_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_42_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_42_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_42_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_42_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_42_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_42_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_42_MEM_AXI4_AWID_WIDTH | 9
DRIVER_42_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_42_MEM_AXI4_USE_AWLOCK | true
DRIVER_42_MEM_AXI4_USE_AWCACHE | true
DRIVER_42_MEM_AXI4_USE_AWQOS | true
DRIVER_42_MEM_AXI4_USE_AWREGION | true
DRIVER_42_MEM_AXI4_USE_AWUSER | true
DRIVER_42_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_42_MEM_AXI4_ARID_WIDTH | 9
DRIVER_42_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_42_MEM_AXI4_USE_ARLOCK | true
DRIVER_42_MEM_AXI4_USE_ARCACHE | true
DRIVER_42_MEM_AXI4_USE_ARQOS | true
DRIVER_42_MEM_AXI4_USE_ARREGION | true
DRIVER_42_MEM_AXI4_USE_ARUSER | true
DRIVER_42_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_42_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_42_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_42_MEM_AXI4_USE_BUSER | false
DRIVER_42_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_42_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_42_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_43_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_43_CAM_AXIST_KEY_WIDTH | 64
DRIVER_43_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_43_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_43_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_43_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_43_CAM_AXIST_TID_WIDTH | 8
DRIVER_43_CAM_AXIST_PTR_WIDTH | 1
DRIVER_43_CAM_AXIST_LOG2_TABLES | 1
DRIVER_43_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_43_CAM_TEST_CAM | BCAM
DRIVER_43_ED_ASSOC_STORAGE_ONLY | false
DRIVER_43_ED_FIRST_CAM_DRIVER | false
DRIVER_43_ED_ONCHIP_MEM_ONLY | false
DRIVER_43_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_43_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_43_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_43_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_43_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_43_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_43_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_43_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_43_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_43_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_43_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_43_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_43_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_43_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_43_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_43_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_43_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_43_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_43_MEM_AXI4_AWID_WIDTH | 9
DRIVER_43_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_43_MEM_AXI4_USE_AWLOCK | true
DRIVER_43_MEM_AXI4_USE_AWCACHE | true
DRIVER_43_MEM_AXI4_USE_AWQOS | true
DRIVER_43_MEM_AXI4_USE_AWREGION | true
DRIVER_43_MEM_AXI4_USE_AWUSER | true
DRIVER_43_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_43_MEM_AXI4_ARID_WIDTH | 9
DRIVER_43_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_43_MEM_AXI4_USE_ARLOCK | true
DRIVER_43_MEM_AXI4_USE_ARCACHE | true
DRIVER_43_MEM_AXI4_USE_ARQOS | true
DRIVER_43_MEM_AXI4_USE_ARREGION | true
DRIVER_43_MEM_AXI4_USE_ARUSER | true
DRIVER_43_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_43_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_43_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_43_MEM_AXI4_USE_BUSER | false
DRIVER_43_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_43_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_43_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_44_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_44_CAM_AXIST_KEY_WIDTH | 64
DRIVER_44_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_44_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_44_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_44_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_44_CAM_AXIST_TID_WIDTH | 8
DRIVER_44_CAM_AXIST_PTR_WIDTH | 1
DRIVER_44_CAM_AXIST_LOG2_TABLES | 1
DRIVER_44_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_44_CAM_TEST_CAM | BCAM
DRIVER_44_ED_ASSOC_STORAGE_ONLY | false
DRIVER_44_ED_FIRST_CAM_DRIVER | false
DRIVER_44_ED_ONCHIP_MEM_ONLY | false
DRIVER_44_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_44_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_44_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_44_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_44_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_44_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_44_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_44_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_44_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_44_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_44_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_44_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_44_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_44_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_44_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_44_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_44_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_44_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_44_MEM_AXI4_AWID_WIDTH | 9
DRIVER_44_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_44_MEM_AXI4_USE_AWLOCK | true
DRIVER_44_MEM_AXI4_USE_AWCACHE | true
DRIVER_44_MEM_AXI4_USE_AWQOS | true
DRIVER_44_MEM_AXI4_USE_AWREGION | true
DRIVER_44_MEM_AXI4_USE_AWUSER | true
DRIVER_44_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_44_MEM_AXI4_ARID_WIDTH | 9
DRIVER_44_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_44_MEM_AXI4_USE_ARLOCK | true
DRIVER_44_MEM_AXI4_USE_ARCACHE | true
DRIVER_44_MEM_AXI4_USE_ARQOS | true
DRIVER_44_MEM_AXI4_USE_ARREGION | true
DRIVER_44_MEM_AXI4_USE_ARUSER | true
DRIVER_44_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_44_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_44_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_44_MEM_AXI4_USE_BUSER | false
DRIVER_44_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_44_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_44_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_45_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_45_CAM_AXIST_KEY_WIDTH | 64
DRIVER_45_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_45_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_45_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_45_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_45_CAM_AXIST_TID_WIDTH | 8
DRIVER_45_CAM_AXIST_PTR_WIDTH | 1
DRIVER_45_CAM_AXIST_LOG2_TABLES | 1
DRIVER_45_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_45_CAM_TEST_CAM | BCAM
DRIVER_45_ED_ASSOC_STORAGE_ONLY | false
DRIVER_45_ED_FIRST_CAM_DRIVER | false
DRIVER_45_ED_ONCHIP_MEM_ONLY | false
DRIVER_45_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_45_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_45_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_45_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_45_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_45_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_45_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_45_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_45_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_45_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_45_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_45_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_45_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_45_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_45_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_45_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_45_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_45_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_45_MEM_AXI4_AWID_WIDTH | 9
DRIVER_45_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_45_MEM_AXI4_USE_AWLOCK | true
DRIVER_45_MEM_AXI4_USE_AWCACHE | true
DRIVER_45_MEM_AXI4_USE_AWQOS | true
DRIVER_45_MEM_AXI4_USE_AWREGION | true
DRIVER_45_MEM_AXI4_USE_AWUSER | true
DRIVER_45_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_45_MEM_AXI4_ARID_WIDTH | 9
DRIVER_45_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_45_MEM_AXI4_USE_ARLOCK | true
DRIVER_45_MEM_AXI4_USE_ARCACHE | true
DRIVER_45_MEM_AXI4_USE_ARQOS | true
DRIVER_45_MEM_AXI4_USE_ARREGION | true
DRIVER_45_MEM_AXI4_USE_ARUSER | true
DRIVER_45_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_45_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_45_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_45_MEM_AXI4_USE_BUSER | false
DRIVER_45_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_45_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_45_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_46_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_46_CAM_AXIST_KEY_WIDTH | 64
DRIVER_46_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_46_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_46_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_46_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_46_CAM_AXIST_TID_WIDTH | 8
DRIVER_46_CAM_AXIST_PTR_WIDTH | 1
DRIVER_46_CAM_AXIST_LOG2_TABLES | 1
DRIVER_46_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_46_CAM_TEST_CAM | BCAM
DRIVER_46_ED_ASSOC_STORAGE_ONLY | false
DRIVER_46_ED_FIRST_CAM_DRIVER | false
DRIVER_46_ED_ONCHIP_MEM_ONLY | false
DRIVER_46_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_46_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_46_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_46_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_46_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_46_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_46_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_46_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_46_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_46_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_46_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_46_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_46_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_46_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_46_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_46_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_46_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_46_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_46_MEM_AXI4_AWID_WIDTH | 9
DRIVER_46_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_46_MEM_AXI4_USE_AWLOCK | true
DRIVER_46_MEM_AXI4_USE_AWCACHE | true
DRIVER_46_MEM_AXI4_USE_AWQOS | true
DRIVER_46_MEM_AXI4_USE_AWREGION | true
DRIVER_46_MEM_AXI4_USE_AWUSER | true
DRIVER_46_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_46_MEM_AXI4_ARID_WIDTH | 9
DRIVER_46_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_46_MEM_AXI4_USE_ARLOCK | true
DRIVER_46_MEM_AXI4_USE_ARCACHE | true
DRIVER_46_MEM_AXI4_USE_ARQOS | true
DRIVER_46_MEM_AXI4_USE_ARREGION | true
DRIVER_46_MEM_AXI4_USE_ARUSER | true
DRIVER_46_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_46_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_46_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_46_MEM_AXI4_USE_BUSER | false
DRIVER_46_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_46_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_46_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_47_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_47_CAM_AXIST_KEY_WIDTH | 64
DRIVER_47_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_47_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_47_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_47_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_47_CAM_AXIST_TID_WIDTH | 8
DRIVER_47_CAM_AXIST_PTR_WIDTH | 1
DRIVER_47_CAM_AXIST_LOG2_TABLES | 1
DRIVER_47_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_47_CAM_TEST_CAM | BCAM
DRIVER_47_ED_ASSOC_STORAGE_ONLY | false
DRIVER_47_ED_FIRST_CAM_DRIVER | false
DRIVER_47_ED_ONCHIP_MEM_ONLY | false
DRIVER_47_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_47_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_47_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_47_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_47_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_47_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_47_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_47_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_47_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_47_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_47_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_47_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_47_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_47_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_47_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_47_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_47_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_47_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_47_MEM_AXI4_AWID_WIDTH | 9
DRIVER_47_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_47_MEM_AXI4_USE_AWLOCK | true
DRIVER_47_MEM_AXI4_USE_AWCACHE | true
DRIVER_47_MEM_AXI4_USE_AWQOS | true
DRIVER_47_MEM_AXI4_USE_AWREGION | true
DRIVER_47_MEM_AXI4_USE_AWUSER | true
DRIVER_47_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_47_MEM_AXI4_ARID_WIDTH | 9
DRIVER_47_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_47_MEM_AXI4_USE_ARLOCK | true
DRIVER_47_MEM_AXI4_USE_ARCACHE | true
DRIVER_47_MEM_AXI4_USE_ARQOS | true
DRIVER_47_MEM_AXI4_USE_ARREGION | true
DRIVER_47_MEM_AXI4_USE_ARUSER | true
DRIVER_47_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_47_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_47_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_47_MEM_AXI4_USE_BUSER | false
DRIVER_47_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_47_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_47_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_48_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_48_CAM_AXIST_KEY_WIDTH | 64
DRIVER_48_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_48_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_48_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_48_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_48_CAM_AXIST_TID_WIDTH | 8
DRIVER_48_CAM_AXIST_PTR_WIDTH | 1
DRIVER_48_CAM_AXIST_LOG2_TABLES | 1
DRIVER_48_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_48_CAM_TEST_CAM | BCAM
DRIVER_48_ED_ASSOC_STORAGE_ONLY | false
DRIVER_48_ED_FIRST_CAM_DRIVER | false
DRIVER_48_ED_ONCHIP_MEM_ONLY | false
DRIVER_48_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_48_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_48_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_48_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_48_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_48_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_48_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_48_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_48_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_48_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_48_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_48_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_48_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_48_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_48_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_48_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_48_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_48_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_48_MEM_AXI4_AWID_WIDTH | 9
DRIVER_48_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_48_MEM_AXI4_USE_AWLOCK | true
DRIVER_48_MEM_AXI4_USE_AWCACHE | true
DRIVER_48_MEM_AXI4_USE_AWQOS | true
DRIVER_48_MEM_AXI4_USE_AWREGION | true
DRIVER_48_MEM_AXI4_USE_AWUSER | true
DRIVER_48_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_48_MEM_AXI4_ARID_WIDTH | 9
DRIVER_48_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_48_MEM_AXI4_USE_ARLOCK | true
DRIVER_48_MEM_AXI4_USE_ARCACHE | true
DRIVER_48_MEM_AXI4_USE_ARQOS | true
DRIVER_48_MEM_AXI4_USE_ARREGION | true
DRIVER_48_MEM_AXI4_USE_ARUSER | true
DRIVER_48_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_48_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_48_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_48_MEM_AXI4_USE_BUSER | false
DRIVER_48_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_48_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_48_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
DRIVER_49_TYPE_ENUM | DRIVER_TYPE_MEM_AXI4
DRIVER_49_CAM_AXIST_KEY_WIDTH | 64
DRIVER_49_CAM_AXIST_RESULT_WIDTH | 32
DRIVER_49_CAM_AXIST_NUM_ENTRIES | 32
DRIVER_49_CAM_AXIST_USERMETADATA_WIDTH | 1
DRIVER_49_CAM_AXIST_PPMETADATA_WIDTH | 19
DRIVER_49_CAM_AXIST_TID_WIDTH | 8
DRIVER_49_CAM_AXIST_PTR_WIDTH | 1
DRIVER_49_CAM_AXIST_LOG2_TABLES | 1
DRIVER_49_CAM_AXI4L_DATA_WIDTH | 32
DRIVER_49_CAM_TEST_CAM | BCAM
DRIVER_49_ED_ASSOC_STORAGE_ONLY | false
DRIVER_49_ED_FIRST_CAM_DRIVER | false
DRIVER_49_ED_ONCHIP_MEM_ONLY | false
DRIVER_49_CSR_AXI4L_AWADDR_WIDTH | 32
DRIVER_49_CSR_AXI4L_ARADDR_WIDTH | 32
DRIVER_49_CSR_AXI4L_WDATA_WIDTH | 32
DRIVER_49_CSR_AXI4L_RDATA_WIDTH | 32
DRIVER_49_MEM_AXI4_FAST_CLIP_RECOVERY | true
DRIVER_49_MEM_AXI4_NUM_ADDR_FIELDS | 1
DRIVER_49_MEM_AXI4_ADDR_FIELD_0_MASK | -1
DRIVER_49_MEM_AXI4_ADDR_FIELD_1_MASK | -1
DRIVER_49_MEM_AXI4_ADDR_FIELD_2_MASK | -1
DRIVER_49_MEM_AXI4_ADDR_FIELD_3_MASK | -1
DRIVER_49_MEM_AXI4_ADDR_FIELD_4_MASK | -1
DRIVER_49_MEM_AXI4_ADDR_FIELD_5_MASK | -1
DRIVER_49_MEM_AXI4_ADDR_FIELD_6_MASK | -1
DRIVER_49_MEM_AXI4_ADDR_FIELD_7_MASK | -1
DRIVER_49_MEM_AXI4_ADDR_ALU_ARG_WIDTH | 16
DRIVER_49_MEM_AXI4_NUM_DQ_ALUS | 2
DRIVER_49_MEM_AXI4_NUM_DM_ALUS | 2
DRIVER_49_MEM_AXI4_DATA_DQ_RATIO | 8
DRIVER_49_MEM_AXI4_AWID_WIDTH | 9
DRIVER_49_MEM_AXI4_AWADDR_WIDTH | 44
DRIVER_49_MEM_AXI4_USE_AWLOCK | true
DRIVER_49_MEM_AXI4_USE_AWCACHE | true
DRIVER_49_MEM_AXI4_USE_AWQOS | true
DRIVER_49_MEM_AXI4_USE_AWREGION | true
DRIVER_49_MEM_AXI4_USE_AWUSER | true
DRIVER_49_MEM_AXI4_AWUSER_WIDTH | 1
DRIVER_49_MEM_AXI4_ARID_WIDTH | 9
DRIVER_49_MEM_AXI4_ARADDR_WIDTH | 44
DRIVER_49_MEM_AXI4_USE_ARLOCK | true
DRIVER_49_MEM_AXI4_USE_ARCACHE | true
DRIVER_49_MEM_AXI4_USE_ARQOS | true
DRIVER_49_MEM_AXI4_USE_ARREGION | true
DRIVER_49_MEM_AXI4_USE_ARUSER | true
DRIVER_49_MEM_AXI4_ARUSER_WIDTH | 1
DRIVER_49_MEM_AXI4_WDATA_WIDTH | 64
DRIVER_49_MEM_AXI4_RDATA_WIDTH | 64
DRIVER_49_MEM_AXI4_USE_BUSER | false
DRIVER_49_MEM_AXI4_BUSER_WIDTH | 1
DRIVER_49_MEM_STATUS_STATUS_TYPE | STATUS_TYPE_FM_EMIF_CAL
DRIVER_49_MEM_RESET_RESET_TYPE | RESET_TYPE_MEMSS
deviceFamily | UNKNOWN
generateLegacySim | false

## Software Assignments (none)

## hydra_0_software

hydra_software v1.0.0

## Parameters
deviceFamily | UNKNOWN
generateLegacySim | false

## Software Assignments (none)

## hydra_0_rtl_library

hydra_rtl_library v1.0.0

## Parameters
deviceFamily | UNKNOWN
generateLegacySim | false

## Software Assignments (none)

## hydra_0_global_csr

hydra_global_csr v1.0.0

hydra_0_driver0_clk_bridge | out_clk | hydra_0_global_csr
driver_clk_0
hydra_0_driver0_reset_bridge | out_reset
driver_reset_0
hydra_0_driver0_mem_axi4 | driver_sync
driver_sync_0
|  | driver_ctrl_0 | hydra_0_driver0_mem_axi4
|  | driver_ctrl

## Parameters
PORT_HYDRA_DRIVER_SYNC_POST_OUT_WIDTH | 1
PORT_HYDRA_DRIVER_SYNC_POST_IN_WIDTH | 1
PORT_HYDRA_DRIVER_SYNC_WAIT_OUT_WIDTH | 1
PORT_HYDRA_DRIVER_SYNC_WAIT_IN_WIDTH | 1
PORT_HYDRA_APB3_PADDR_WIDTH | 12
PORT_HYDRA_APB3_PWDATA_WIDTH | 32
PORT_HYDRA_APB3_PRDATA_WIDTH | 32
deviceFamily | UNKNOWN
generateLegacySim | false

## Software Assignments (none)

## hydra_0_driver0_mem_axi4

hydra_driver_mem_axi4 v1.0.0

hydra_0_driver0_clk_bridge | out_clk | hydra_0_driver0_mem_axi4
clk
hydra_0_driver0_reset_bridge | out_reset
reset
hydra_0_global_csr | driver_ctrl_0
driver_ctrl
|  | driver_sync | hydra_0_global_csr
|  | driver_sync_0

## Parameters
DRIVER_INDEX | 0
DEVICE_FAMILY | Agilex
FAST_CLIP_RECOVERY | true
NUM_ADDR_FIELDS | 1
ADDR_FIELD_0_MASK | -1
ADDR_FIELD_1_MASK | -1
ADDR_FIELD_2_MASK | -1
ADDR_FIELD_3_MASK | -1
ADDR_FIELD_4_MASK | -1
ADDR_FIELD_5_MASK | -1
ADDR_FIELD_6_MASK | -1
ADDR_FIELD_7_MASK | -1
ADDR_ALU_ARG_WIDTH | 16
NUM_DQ_ALUS | 2
NUM_DM_ALUS | 2
DATA_DQ_RATIO | 8
USE_AWLOCK | true
USE_AWCACHE | true
USE_AWPROT | true
USE_AWQOS | true
USE_AWREGION | true
USE_AWUSER | true
USE_ARLOCK | true
USE_ARCACHE | true
USE_ARPROT | true
USE_ARQOS | true
USE_ARREGION | true
USE_ARUSER | true
USE_BUSER | false
PORT_HYDRA_DRIVER_SYNC_POST_OUT_WIDTH | 1
PORT_HYDRA_DRIVER_SYNC_POST_IN_WIDTH | 1
PORT_HYDRA_DRIVER_SYNC_WAIT_OUT_WIDTH | 1
PORT_HYDRA_DRIVER_SYNC_WAIT_IN_WIDTH | 1
PORT_HYDRA_AXI4L_AWADDR_WIDTH | 24
PORT_HYDRA_AXI4L_AWPROT_WIDTH | 3
PORT_HYDRA_AXI4L_ARADDR_WIDTH | 24
PORT_HYDRA_AXI4L_ARPROT_WIDTH | 3
PORT_HYDRA_AXI4L_WDATA_WIDTH | 32
PORT_HYDRA_AXI4L_WSTRB_WIDTH | 4
PORT_HYDRA_AXI4L_BRESP_WIDTH | 2
PORT_HYDRA_AXI4L_RDATA_WIDTH | 32
PORT_HYDRA_AXI4L_RRESP_WIDTH | 2
PORT_HYDRA_AXI4_AWID_WIDTH | 9
PORT_HYDRA_AXI4_AWADDR_WIDTH | 44
PORT_HYDRA_AXI4_AWLEN_WIDTH | 8
PORT_HYDRA_AXI4_AWSIZE_WIDTH | 3
PORT_HYDRA_AXI4_AWBURST_WIDTH | 2
PORT_HYDRA_AXI4_AWLOCK_WIDTH | 1
PORT_HYDRA_AXI4_AWCACHE_WIDTH | 4
PORT_HYDRA_AXI4_AWPROT_WIDTH | 3
PORT_HYDRA_AXI4_AWQOS_WIDTH | 4
PORT_HYDRA_AXI4_AWREGION_WIDTH | 4
PORT_HYDRA_AXI4_AWUSER_WIDTH | 1
PORT_HYDRA_AXI4_ARID_WIDTH | 9
PORT_HYDRA_AXI4_ARADDR_WIDTH | 44
PORT_HYDRA_AXI4_ARLEN_WIDTH | 8
PORT_HYDRA_AXI4_ARSIZE_WIDTH | 3
PORT_HYDRA_AXI4_ARBURST_WIDTH | 2
PORT_HYDRA_AXI4_ARLOCK_WIDTH | 1
PORT_HYDRA_AXI4_ARCACHE_WIDTH | 4
PORT_HYDRA_AXI4_ARPROT_WIDTH | 3
PORT_HYDRA_AXI4_ARQOS_WIDTH | 4
PORT_HYDRA_AXI4_ARREGION_WIDTH | 4
PORT_HYDRA_AXI4_ARUSER_WIDTH | 1
PORT_HYDRA_AXI4_WDATA_WIDTH | 64
PORT_HYDRA_AXI4_WUSER_WIDTH | 1
PORT_HYDRA_AXI4_WSTRB_WIDTH | 8
PORT_HYDRA_AXI4_BID_WIDTH | 9
PORT_HYDRA_AXI4_BRESP_WIDTH | 2
PORT_HYDRA_AXI4_BUSER_WIDTH | 1
PORT_HYDRA_AXI4_RID_WIDTH | 9
PORT_HYDRA_AXI4_RDATA_WIDTH | 64
PORT_HYDRA_AXI4_RUSER_WIDTH | 1
PORT_HYDRA_AXI4_RRESP_WIDTH | 2
deviceFamily | UNKNOWN
generateLegacySim | false

## Software Assignments (none)

## hydra_0_driver0_clk_bridge

altera_clock_bridge v19.2.0

## Parameters
DERIVED_CLOCK_RATE | 0
EXPLICIT_CLOCK_RATE | 0
NUM_CLOCK_OUTPUTS | 1
deviceFamily | UNKNOWN
generateLegacySim | false

## Software Assignments (none)

## hydra_0_driver0_reset_bridge

altera_reset_bridge v19.2.0

## Parameters
ACTIVE_LOW_RESET | 1
SYNCHRONOUS_EDGES | none
O_SYNCHRONOUS_EDGES | none
NUM_RESET_OUTPUTS | 1
USE_RESET_REQUEST | 0
SYNC_RESET | 0
deviceFamily | UNKNOWN
generateLegacySim | false

## Software Assignments (none)

generation took 0.00 seconds | rendering took 0.03 seconds