## golden top Board Configuration

www.terasic.com
Copyright © 2003-2024 Terasic Inc. All Rights Reserved.

### Pin Assignments:

##

CLOCK
Name | Location | Direction | IO Standard
--- | --- | --- | ---
CLOCK2_50 | D8 | input | 1.8-V LVCMOS
CLOCK3_50 | BM71 | input | 1.2 V
CLOCK_50 | CH128 | input | 3.3-V LVCMOS

##

KEY
Name | Location | Direction | IO Standard
--- | --- | --- | ---
CPU_RESET_N | BM78 | input | 1.2 V
KEY[0] | BW59 | input | 1.2 V
KEY[1] | CA59 | input | 1.2 V
KEY[2] | CF71 | input | 1.2 V
KEY[3] | CH71 | input | 1.2 V

##

SW
Name | Location | Direction | IO Standard
--- | --- | --- | ---
SW[0] | BM62 | input | 1.2 V
SW[1] | BP62 | input | 1.2 V
SW[2] | BH62 | input | 1.2 V
SW[3] | BH59 | input | 1.2 V
SW[4] | BM59 | input | 1.2 V
SW[5] | BK59 | input | 1.2 V
SW[6] | BU62 | input | 1.2 V
SW[7] | BR62 | input | 1.2 V
SW[8] | BU59 | input | 1.2 V
SW[9] | BR59 | input | 1.2 V

##

LED
Name | Location | Direction | IO Standard
--- | --- | --- | ---
LEDR[0] | CC71 | output | 1.2 V
LEDR[1] | CA71 | output | 1.2 V
LEDR[2] | CH69 | output | 1.2 V
LEDR[3] | CF69 | output | 1.2 V
LEDR[4] | CA62 | output | 1.2 V
LEDR[5] | CC62 | output | 1.2 V
LEDR[6] | CF62 | output | 1.2 V
LEDR[7] | CH62 | output | 1.2 V
LEDR[8] | CF59 | output | 1.2 V
LEDR[9] | BH78 | output | 1.2 V

##

Seg7
Name | Location | Direction | IO Standard
--- | --- | --- | ---
HEX0[0] | BP81 | output | 1.2 V
HEX0[1] | BM81 | output | 1.2 V
HEX0[2] | BM89 | output | 1.2 V
HEX0[3] | BK89 | output | 1.2 V
HEX0[4] | BH92 | output | 1.2 V
HEX0[5] | BM92 | output | 1.2 V
HEX0[6] | BP92 | output | 1.2 V
HEX1[0] | CA78 | output | 1.2 V
HEX1[1] | BW78 | output | 1.2 V
HEX1[2] | BU78 | output | 1.2 V
HEX1[3] | BR78 | output | 1.2 V
HEX1[4] | BU81 | output | 1.2 V
HEX1[5] | BR81 | output | 1.2 V
HEX1[6] | CA89 | output | 1.2 V
HEX2[0] | BW89 | output | 1.2 V
HEX2[1] | BU92 | output | 1.2 V
HEX2[2] | BR92 | output | 1.2 V
HEX2[3] | BU89 | output | 1.2 V
HEX2[4] | BR89 | output | 1.2 V
HEX2[5] | CF78 | output | 1.2 V
HEX2[6] | CH78 | output | 1.2 V
HEX3[0] | CC81 | output | 1.2 V
HEX3[1] | CA81 | output | 1.2 V
HEX3[2] | CH81 | output | 1.2 V
HEX3[3] | CF81 | output | 1.2 V
HEX3[4] | CF89 | output | 1.2 V
HEX3[5] | CH89 | output | 1.2 V
HEX3[6] | CH92 | output | 1.2 V
HEX4[0] | CF92 | output | 1.2 V
HEX4[1] | CA92 | output | 1.2 V
HEX4[2] | CC92 | output | 1.2 V
HEX4[3] | CL76 | output | 1.2 V
HEX4[4] | CK76 | output | 1.2 V
HEX4[5] | CL82 | output | 1.2 V
HEX4[6] | CK80 | output | 1.2 V
HEX5[0] | CL85 | output | 1.2 V
HEX5[1] | CK85 | output | 1.2 V
HEX5[2] | BK69 | output | 1.2 V
HEX5[3] | BP71 | output | 1.2 V
HEX5[4] | BH89 | output | 1.2 V
HEX5[5] | BH71 | output | 1.2 V
HEX5[6] | BM69 | output | 1.2 V

##

SDRAM
Name | Location | Direction | IO Standard
--- | --- | --- | ---
DRAM_CLK | B39 | output | 1.8-V LVCMOS
DRAM_CKE | B35 | output | 1.8-V LVCMOS
DRAM_ADDR[0] | F27 | output | 1.8-V LVCMOS
DRAM_ADDR[1] | F24 | output | 1.8-V LVCMOS
DRAM_ADDR[2] | H27 | output | 1.8-V LVCMOS
DRAM_ADDR[3] | D24 | output | 1.8-V LVCMOS
DRAM_ADDR[4] | H18 | output | 1.8-V LVCMOS
DRAM_ADDR[5] | D15 | output | 1.8-V LVCMOS
DRAM_ADDR[6] | F18 | output | 1.8-V LVCMOS
DRAM_ADDR[7] | F15 | output | 1.8-V LVCMOS
DRAM_ADDR[8] | K8 | output | 1.8-V LVCMOS
DRAM_ADDR[9] | F8 | output | 1.8-V LVCMOS
DRAM_ADDR[10] | C2 | output | 1.8-V LVCMOS
DRAM_ADDR[11] | A17 | output | 1.8-V LVCMOS
DRAM_ADDR[12] | D4 | output | 1.8-V LVCMOS
DRAM_BA[0] | D34 | output | 1.8-V LVCMOS
DRAM_BA[1] | F4 | output | 1.8-V LVCMOS
DRAM_DQ[0] | A14 | inout | 1.8-V LVCMOS
DRAM_DQ[1] | A11 | inout | 1.8-V LVCMOS
DRAM_DQ[2] | B14 | inout | 1.8-V LVCMOS
DRAM_DQ[3] | B11 | inout | 1.8-V LVCMOS
DRAM_DQ[4] | A20 | inout | 1.8-V LVCMOS
DRAM_DQ[5] | A8 | inout | 1.8-V LVCMOS
DRAM_DQ[6] | A23 | inout | 1.8-V LVCMOS
DRAM_DQ[7] | B4 | inout | 1.8-V LVCMOS
DRAM_DQ[8] | B20 | inout | 1.8-V LVCMOS
DRAM_DQ[9] | B23 | inout | 1.8-V LVCMOS
DRAM_DQ[10] | B26 | inout | 1.8-V LVCMOS
DRAM_DQ[11] | B30 | inout | 1.8-V LVCMOS
DRAM_DQ[12] | A39 | inout | 1.8-V LVCMOS
DRAM_DQ[13] | A30 | inout | 1.8-V LVCMOS
DRAM_DQ[14] | A35 | inout | 1.8-V LVCMOS
DRAM_DQ[15] | A33 | inout | 1.8-V LVCMOS
DRAM_LDQM | K4 | output | 1.8-V LVCMOS
DRAM_UDQM | G2 | output | 1.8-V LVCMOS
DRAM_CS_N | H8 | output | 1.8-V LVCMOS
DRAM_WE_N | J2 | output | 1.8-V LVCMOS
DRAM_CAS_N | J1 | output | 1.8-V LVCMOS
DRAM_RAS_N | G1 | output | 1.8-V LVCMOS

##

DDR4
Name | Location | Direction | IO Standard
--- | --- | --- | ---
DDR4_REFCLK_P | AB117 | input | 1.2V TRUE DIFFERENTIAL SIGNALING
DDR4_A[0] | T114 | output | SSTL-12
DDR4_A[1] | P114 | output | SSTL-12
DDR4_A[2] | V117 | output | SSTL-12
DDR4_A[3] | T117 | output | SSTL-12
DDR4_A[4] | M114 | output | SSTL-12
DDR4_A[5] | K114 | output | SSTL-12
DDR4_A[6] | V108 | output | SSTL-12
DDR4_A[7] | T108 | output | SSTL-12
DDR4_A[8] | T105 | output | SSTL-12
DDR4_A[9] | P105 | output | SSTL-12
DDR4_A[10] | M105 | output | SSTL-12
DDR4_A[11] | K105 | output | SSTL-12
DDR4_A[12] | AG111 | output | SSTL-12
DDR4_A[13] | Y114 | output | SSTL-12
DDR4_A[14] | AB114 | output | SSTL-12
DDR4_A[15] | AK107 | output | SSTL-12
DDR4_A[16] | AK104 | output | SSTL-12
DDR4_BA[0] | AB108 | output | SSTL-12
DDR4_BA[1] | Y105 | output | SSTL-12
DDR4_BG[0] | AB105 | output | SSTL-12
DDR4_CK | H108 | output | DIFFERENTIAL 1.2-V SSTL
DDR4_CK_N | F108 | output | DIFFERENTIAL 1.2-V SSTL
DDR4_CKE | F105 | output | SSTL-12
DDR4_DQS[0] | B122 | inout | DIFFERENTIAL 1.2-V POD
DDR4_DQS[1] | AG90 | inout | DIFFERENTIAL 1.2-V POD
DDR4_DQS[2] | K95 | inout | DIFFERENTIAL 1.2-V POD
DDR4_DQS[3] | F95 | inout | DIFFERENTIAL 1.2-V POD
DDR4_DQS_N[0] | A125 | inout | DIFFERENTIAL 1.2-V POD
DDR4_DQS_N[1] | AG93 | inout | DIFFERENTIAL 1.2-V POD
DDR4_DQS_N[2] | M95 | inout | DIFFERENTIAL 1.2-V POD
DDR4_DQS_N[3] | D95 | inout | DIFFERENTIAL 1.2-V POD
DDR4_DQ[0] | B128 | inout | 1.2-V POD
DDR4_DQ[1] | A116 | inout | 1.2-V POD
DDR4_DQ[2] | A128 | inout | 1.2-V POD
DDR4_DQ[3] | B116 | inout | 1.2-V POD
DDR4_DQ[4] | B130 | inout | 1.2-V POD
DDR4_DQ[5] | B113 | inout | 1.2-V POD
DDR4_DQ[6] | A130 | inout | 1.2-V POD
DDR4_DQ[7] | A113 | inout | 1.2-V POD
DDR4_DQ[8] | AG100 | inout | 1.2-V POD
DDR4_DQ[9] | Y98 | inout | 1.2-V POD
DDR4_DQ[10] | AG104 | inout | 1.2-V POD
DDR4_DQ[11] | Y95 | inout | 1.2-V POD
DDR4_DQ[12] | AC96 | inout | 1.2-V POD
DDR4_DQ[13] | Y87 | inout | 1.2-V POD
DDR4_DQ[14] | AC100 | inout | 1.2-V POD
DDR4_DQ[15] | Y84 | inout | 1.2-V POD
DDR4_DQ[16] | T95 | inout | 1.2-V POD
DDR4_DQ[17] | K84 | inout | 1.2-V POD
DDR4_DQ[18] | P95 | inout | 1.2-V POD
DDR4_DQ[19] | M84 | inout | 1.2-V POD
DDR4_DQ[20] | T98 | inout | 1.2-V POD
DDR4_DQ[21] | V98 | inout | 1.2-V POD
DDR4_DQ[22] | T84 | inout | 1.2-V POD
DDR4_DQ[23] | P84 | inout | 1.2-V POD
DDR4_DQ[24] | M98 | inout | 1.2-V POD
DDR4_DQ[25] | D84 | inout | 1.2-V POD
DDR4_DQ[26] | K98 | inout | 1.2-V POD
DDR4_DQ[27] | K87 | inout | 1.2-V POD
DDR4_DQ[28] | F98 | inout | 1.2-V POD
DDR4_DQ[29] | F84 | inout | 1.2-V POD
DDR4_DQ[30] | H98 | inout | 1.2-V POD
DDR4_DQ[31] | M87 | inout | 1.2-V POD
DDR4_DBI_N[0] | B119 | inout | 1.2-V POD
DDR4_DBI_N[1] | AC90 | inout | 1.2-V POD
DDR4_DBI_N[2] | V87 | inout | 1.2-V POD
DDR4_DBI_N[3] | H87 | inout | 1.2-V POD
DDR4_CS_N | K117 | output | SSTL-12
DDR4_RESET_N | H117 | output | SSTL-12
DDR4_ODT | F114 | output | SSTL-12
DDR4_PAR | K108 | output | SSTL-12
DDR4_ALERT_N | Y108 | input | 1.2 V
DDR4_ACT_N | M117 | output | SSTL-12
DDR4_RZQ | AK111 | input | 1.2 V

##

Video-In
Name | Location | Direction | IO Standard
--- | --- | --- | ---
TD_CLK27 | BF75 | input | 1.2 V
TD_HS | BE93 | input | 1.2 V
TD_VS | BE96 | input | 1.2 V
TD_DATA[0] | BF72 | input | 1.2 V
TD_DATA[1] | BE75 | input | 1.2 V
TD_DATA[2] | BE79 | input | 1.2 V
TD_DATA[3] | BF83 | input | 1.2 V
TD_DATA[4] | BE83 | input | 1.2 V
TD_DATA[5] | BE86 | input | 1.2 V
TD_DATA[6] | BF86 | input | 1.2 V
TD_DATA[7] | BF90 | input | 1.2 V
TD_RESET_N | BF93 | output | 1.2 V

##

HDMI
Name | Location | Direction | IO Standard
--- | --- | --- | ---
HDMI_LRCLK | BP112 | inout | 3.3-V LVCMOS
HDMI_MCLK | BM118 | inout | 3.3-V LVCMOS
HDMI_SCLK | BM112 | inout | 3.3-V LVCMOS
HDMI_TX_CLK | CH59 | output | 1.2 V
HDMI_TX_HS | BR109 | output | 3.3-V LVCMOS
HDMI_TX_VS | BE107 | output | 3.3-V LVCMOS
HDMI_TX_D[0] | CD134 | output | 3.3-V LVCMOS
HDMI_TX_D[1] | CD135 | output | 3.3-V LVCMOS
HDMI_TX_D[2] | CG134 | output | 3.3-V LVCMOS
HDMI_TX_D[3] | CG135 | output | 3.3-V LVCMOS
HDMI_TX_D[4] | CH132 | output | 3.3-V LVCMOS
HDMI_TX_D[5] | CF132 | output | 3.3-V LVCMOS
HDMI_TX_D[6] | CF128 | output | 3.3-V LVCMOS
HDMI_TX_D[7] | CK134 | output | 3.3-V LVCMOS
HDMI_TX_D[8] | CL125 | output | 3.3-V LVCMOS
HDMI_TX_D[9] | CF121 | output | 3.3-V LVCMOS
HDMI_TX_D[10] | CF118 | output | 3.3-V LVCMOS
HDMI_TX_D[11] | BU118 | output | 3.3-V LVCMOS
HDMI_TX_D[12] | BR118 | output | 3.3-V LVCMOS
HDMI_TX_D[13] | CA118 | output | 3.3-V LVCMOS
HDMI_TX_D[14] | BW118 | output | 3.3-V LVCMOS
HDMI_TX_D[15] | CL128 | output | 3.3-V LVCMOS
HDMI_TX_D[16] | CL130 | output | 3.3-V LVCMOS
HDMI_TX_D[17] | CK125 | output | 3.3-V LVCMOS
HDMI_TX_D[18] | CK128 | output | 3.3-V LVCMOS
HDMI_TX_D[19] | BF111 | output | 3.3-V LVCMOS
HDMI_TX_D[20] | BH109 | output | 3.3-V LVCMOS
HDMI_TX_D[21] | BE115 | output | 3.3-V LVCMOS
HDMI_TX_D[22] | BF115 | output | 3.3-V LVCMOS
HDMI_TX_D[23] | BU109 | output | 3.3-V LVCMOS
HDMI_TX_DE | BK109 | output | 3.3-V LVCMOS
HDMI_TX_INT | BE111 | input | 3.3-V LVCMOS
HDMI_I2S | BK118 | inout | 3.3-V LVCMOS

##

Audio
Name | Location | Direction | IO Standard
--- | --- | --- | ---
AUD_BCLK | CL97 | inout | 1.2 V
AUD_XCK | CK97 | output | 1.2 V
AUD_ADCLRCK | CK88 | inout | 1.2 V
AUD_ADCDAT | CL91 | input | 1.2 V
AUD_DACLRCK | CK94 | inout | 1.2 V
AUD_DACDAT | CL88 | output | 1.2 V

##

ADC
Name | Location | Direction | IO Standard
--- | --- | --- | ---
ADC_SCLK | CH4 | output | 3.3-V LVCMOS
ADC_DOUT | CK4 | input | 3.3-V LVCMOS
ADC_DIN | BF32 | output | 3.3-V LVCMOS
ADC_CONVST | BP22 | output | 3.3-V LVCMOS

##

I2C for Audio and Video-In
Name | Location | Direction | IO Standard
--- | --- | --- | ---
FPGA_I2C_SCLK | BR112 | output | 3.3-V LVCMOS
FPGA_I2C_SDAT | BM109 | inout | 3.3-V LVCMOS

##

GPIO
Name | Location | Direction | IO Standard
--- | --- | --- | ---
GPIO[0] | BK31 | inout | 3.3-V LVCMOS
GPIO[1] | BE43 | inout | 3.3-V LVCMOS
GPIO[2] | BF29 | inout | 3.3-V LVCMOS
GPIO[3] | BF40 | inout | 3.3-V LVCMOS
GPIO[4] | BK28 | inout | 3.3-V LVCMOS
GPIO[5] | BM31 | inout | 3.3-V LVCMOS
GPIO[6] | BM28 | inout | 3.3-V LVCMOS
GPIO[7] | BP31 | inout | 3.3-V LVCMOS
GPIO[8] | BR31 | inout | 3.3-V LVCMOS
GPIO[9] | BU28 | inout | 3.3-V LVCMOS
GPIO[10] | BU31 | inout | 3.3-V LVCMOS
GPIO[11] | BW28 | inout | 3.3-V LVCMOS
GPIO[12] | BR22 | inout | 3.3-V LVCMOS
GPIO[13] | BU19 | inout | 3.3-V LVCMOS
GPIO[14] | BU22 | inout | 3.3-V LVCMOS
GPIO[15] | BW19 | inout | 3.3-V LVCMOS
GPIO[16] | BH28 | inout | 3.3-V LVCMOS
GPIO[17] | BR28 | inout | 3.3-V LVCMOS
GPIO[18] | BF36 | inout | 3.3-V LVCMOS
GPIO[19] | BE29 | inout | 3.3-V LVCMOS
GPIO[20] | BM22 | inout | 3.3-V LVCMOS
GPIO[21] | BK22 | inout | 3.3-V LVCMOS
GPIO[22] | BR19 | inout | 3.3-V LVCMOS
GPIO[23] | BM19 | inout | 3.3-V LVCMOS
GPIO[24] | BK19 | inout | 3.3-V LVCMOS
GPIO[25] | BH19 | inout | 3.3-V LVCMOS
GPIO[26] | BF25 | inout | 3.3-V LVCMOS
GPIO[27] | CF9 | inout | 3.3-V LVCMOS
GPIO[28] | CH12 | inout | 3.3-V LVCMOS
GPIO[29] | CF12 | inout | 3.3-V LVCMOS
GPIO[30] | CK2 | inout | 3.3-V LVCMOS
GPIO[31] | CJ2 | inout | 3.3-V LVCMOS
GPIO[32] | BE25 | inout | 3.3-V LVCMOS
GPIO[33] | BF21 | inout | 3.3-V LVCMOS
GPIO[34] | BF16 | inout | 3.3-V LVCMOS
GPIO[35] | BE21 | inout | 3.3-V LVCMOS

##

HSMC
Name | Location | Direction | IO Standard
--- | --- | --- | ---
HSMC_GTS_TX_P[0] | AU129 | output | HIGH SPEED DIFFERENTIAL I/O
HSMC_GTS_TX_P[1] | AR129 | output | HIGH SPEED DIFFERENTIAL I/O
HSMC_GTS_TX_P[2] | AN129 | output | HIGH SPEED DIFFERENTIAL I/O
HSMC_GTS_TX_P[3] | AL129 | output | HIGH SPEED DIFFERENTIAL I/O
HSMC_GTS_TX_N[0] | AU126 | output | HIGH SPEED DIFFERENTIAL I/O
HSMC_GTS_TX_N[1] | AR126 | output | HIGH SPEED DIFFERENTIAL I/O
HSMC_GTS_TX_N[2] | AN126 | output | HIGH SPEED DIFFERENTIAL I/O
HSMC_GTS_TX_N[3] | AL126 | output | HIGH SPEED DIFFERENTIAL I/O
HSMC_GTS_RX_P[0] | AT135 | input | HIGH SPEED DIFFERENTIAL I/O
HSMC_GTS_RX_P[1] | AP135 | input | HIGH SPEED DIFFERENTIAL I/O
HSMC_GTS_RX_P[2] | AM135 | input | HIGH SPEED DIFFERENTIAL I/O
HSMC_GTS_RX_P[3] | AK135 | input | HIGH SPEED DIFFERENTIAL I/O
HSMC_GTS_RX_N[0] | AT133 | input | HIGH SPEED DIFFERENTIAL I/O
HSMC_GTS_RX_N[1] | AP133 | input | HIGH SPEED DIFFERENTIAL I/O
HSMC_GTS_RX_N[2] | AM133 | input | HIGH SPEED DIFFERENTIAL I/O
HSMC_GTS_RX_N[3] | AK133 | input | HIGH SPEED DIFFERENTIAL I/O
HSMC_GTS_RX_REFCLK_P | AT120 | input | CURRENT MODE LOGIC (CML)
HSMC_CLK_IN[0] | V18 | input | 2.5-V LVCMOS
HSMC_CLK_IN[1] | W2 | input | 2.5-V LVCMOS
HSMC_CLK_IN[2] | V37 | input | 2.5-V LVCMOS
HSMC_GTS_REFCLK_P | AP120 | input | CURRENT MODE LOGIC (CML)
HSMC_B5B_D[0] | BF107 | inout | 3.3-V LVCMOS
HSMC_B5B_D[1] | BF104 | inout | 3.3-V LVCMOS
HSMC_D[0] | K34 | inout | 2.5-V LVCMOS
HSMC_D[1] | F34 | inout | 2.5-V LVCMOS
HSMC_D[2] | K37 | inout | 2.5-V LVCMOS
HSMC_D[3] | H37 | inout | 2.5-V LVCMOS
HSMC_D[4] | P34 | inout | 2.5-V LVCMOS
HSMC_D[5] | M37 | inout | 2.5-V LVCMOS
HSMC_D[6] | Y34 | inout | 2.5-V LVCMOS
HSMC_D[7] | Y15 | inout | 2.5-V LVCMOS
HSMC_D[8] | AK32 | inout | 2.5-V LVCMOS
HSMC_D[9] | M34 | inout | 2.5-V LVCMOS
HSMC_D[10] | AL32 | inout | 2.5-V LVCMOS
HSMC_D[11] | AK21 | inout | 2.5-V LVCMOS
HSMC_D[12] | AG29 | inout | 2.5-V LVCMOS
HSMC_D[13] | AL16 | inout | 2.5-V LVCMOS
HSMC_D[14] | AL29 | inout | 2.5-V LVCMOS
HSMC_D[15] | AJ1 | inout | 2.5-V LVCMOS
HSMC_D[16] | AL25 | inout | 2.5-V LVCMOS
HSMC_D[17] | AB8 | inout | 2.5-V LVCMOS
HSMC_D[18] | AK25 | inout | 2.5-V LVCMOS
HSMC_D[19] | Y8 | inout | 2.5-V LVCMOS
HSMC_D[20] | AK16 | inout | 2.5-V LVCMOS
HSMC_D[21] | AF2 | inout | 2.5-V LVCMOS
HSMC_D[22] | AG13 | inout | 2.5-V LVCMOS
HSMC_D[23] | AB4 | inout | 2.5-V LVCMOS
HSMC_D[24] | AH8 | inout | 2.5-V LVCMOS
HSMC_D[25] | AD1 | inout | 2.5-V LVCMOS
HSMC_D[26] | AH4 | inout | 2.5-V LVCMOS
HSMC_D[27] | AD2 | inout | 2.5-V LVCMOS
HSMC_D[28] | AE4 | inout | 2.5-V LVCMOS
HSMC_D[29] | V8 | inout | 2.5-V LVCMOS
HSMC_D[30] | T15 | inout | 2.5-V LVCMOS
HSMC_D[31] | Y4 | inout | 2.5-V LVCMOS
HSMC_D[32] | T34 | inout | 2.5-V LVCMOS
HSMC_D[33] | AA1 | inout | 2.5-V LVCMOS
HSMC_D[34] | T37 | inout | 2.5-V LVCMOS
HSMC_D[35] | AC43 | inout | 2.5-V LVCMOS
HSMC_D[36] | AC36 | inout | 2.5-V LVCMOS
HSMC_D[37] | Y27 | inout | 2.5-V LVCMOS
HSMC_D[38] | AG36 | inout | 2.5-V LVCMOS
HSMC_D[39] | Y24 | inout | 2.5-V LVCMOS
HSMC_D[40] | AB27 | inout | 2.5-V LVCMOS
HSMC_D[41] | AB18 | inout | 2.5-V LVCMOS
HSMC_D[42] | AB24 | inout | 2.5-V LVCMOS
HSMC_D[43] | T8 | inout | 2.5-V LVCMOS
HSMC_D[44] | V27 | inout | 2.5-V LVCMOS
HSMC_D[45] | U1 | inout | 2.5-V LVCMOS
HSMC_D[46] | AG21 | inout | 2.5-V LVCMOS
HSMC_D[47] | T18 | inout | 2.5-V LVCMOS
HSMC_D[48] | T27 | inout | 2.5-V LVCMOS
HSMC_D[49] | T4 | inout | 2.5-V LVCMOS
HSMC_D[50] | AJ2 | inout | 2.5-V LVCMOS
HSMC_D[51] | R2 | inout | 2.5-V LVCMOS
HSMC_D[52] | AB15 | inout | 2.5-V LVCMOS
HSMC_D[53] | P15 | inout | 2.5-V LVCMOS
HSMC_D[54] | Y18 | inout | 2.5-V LVCMOS
HSMC_D[55] | P4 | inout | 2.5-V LVCMOS
HSMC_D[56] | T24 | inout | 2.5-V LVCMOS
HSMC_D[57] | N2 | inout | 2.5-V LVCMOS
HSMC_D[58] | W1 | inout | 2.5-V LVCMOS
HSMC_D[59] | L1 | inout | 2.5-V LVCMOS
HSMC_D[60] | P24 | inout | 2.5-V LVCMOS
HSMC_D[61] | M4 | inout | 2.5-V LVCMOS
HSMC_D[62] | U2 | inout | 2.5-V LVCMOS
HSMC_D[63] | M8 | inout | 2.5-V LVCMOS
HSMC_D[64] | M27 | inout | 2.5-V LVCMOS
HSMC_D[65] | M15 | inout | 2.5-V LVCMOS
HSMC_D[66] | M24 | inout | 2.5-V LVCMOS
HSMC_D[67] | M18 | inout | 2.5-V LVCMOS
HSMC_D[68] | N1 | inout | 2.5-V LVCMOS
HSMC_D[69] | K15 | inout | 2.5-V LVCMOS
HSMC_D[70] | K27 | inout | 2.5-V LVCMOS
HSMC_D[71] | K18 | inout | 2.5-V LVCMOS
HSMC_D[72] | F37 | inout | 2.5-V LVCMOS
HSMC_D[73] | Y37 | inout | 2.5-V LVCMOS
HSMC_D[74] | AC46 | inout | 2.5-V LVCMOS
HSMC_D[75] | AG40 | inout | 2.5-V LVCMOS
HSMC_D[76] | K24 | inout | 2.5-V LVCMOS

##

CAM
Name | Location | Direction | IO Standard
--- | --- | --- | ---
CAM_CLK_P | BW69 | input | DPHY
CAM_CLK_N | CA69 | input | DPHY
CAM_D_P[0] | BR69 | input | DPHY
CAM_D_P[1] | BR71 | input | DPHY
CAM_D_N[0] | BU69 | input | DPHY
CAM_D_N[1] | BU71 | input | DPHY
CAM_I2C_SCL | BF120 | inout | 3.3-V LVCMOS
CAM_I2C_SDA | BH118 | inout | 3.3-V LVCMOS
CAM_GPIO | BK112 | inout | 3.3-V LVCMOS
CAM_RZQ1 | BH69 | input | 1.2 V

##

HPS
Name | Location | Direction | IO Standard
--- | --- | --- | ---
HPS_CLK_25 | AG123 | input | 1.8 V
HPS_ENET_MDC | D124 | output | 1.8 V
HPS_ENET_MDIO | F124 | inout | 1.8 V
HPS_ENET_RX_CLK | J135 | input | 1.8 V
HPS_ENET_RX_CTL | AD135 | input | 1.8 V
HPS_ENET_RX_DATA[0] | K132 | input | 1.8 V
HPS_ENET_RX_DATA[1] | AG129 | input | 1.8 V
HPS_ENET_RX_DATA[2] | G134 | input | 1.8 V
HPS_ENET_RX_DATA[3] | G135 | input | 1.8 V
HPS_ENET_TX_CLK | P132 | output | 1.8 V
HPS_ENET_TX_CTL | L135 | output | 1.8 V
HPS_ENET_TX_DATA[0] | M132 | output | 1.8 V
HPS_ENET_TX_DATA[1] | AD134 | output | 1.8 V
HPS_ENET_TX_DATA[2] | J134 | output | 1.8 V
HPS_ENET_TX_DATA[3] | AG120 | output | 1.8 V
HPS_GPIO[0] | T127 | inout | 1.8 V
HPS_GPIO[1] | Y132 | inout | 1.8 V
HPS_GSENSOR_INT | B134 | inout | 1.8 V
HPS_I2C_SCL | K127 | inout | 1.8 V
HPS_I2C_SDA | M127 | inout | 1.8 V
HPS_KEY | K124 | inout | 1.8 V
HPS_LCM_BK | H127 | inout | 1.8 V
HPS_LCM_D_C | P124 | inout | 1.8 V
HPS_LCM_RST_N | T124 | inout | 1.8 V
HPS_LCM_SPIM_CLK | F127 | output | 1.8 V
HPS_LCM_SPIM_MOSI | Y124 | output | 1.8 V
HPS_LCM_SPIM_SS | AB124 | output | 1.8 V
HPS_LED | Y127 | inout | 1.8 V
HPS_SD_CLK | D132 | output | 1.8 V
HPS_SD_CMD | AB132 | inout | 1.8 V
HPS_SD_DATA[0] | E135 | inout | 1.8 V
HPS_SD_DATA[1] | F132 | inout | 1.8 V
HPS_SD_DATA[2] | AA135 | inout | 1.8 V
HPS_SD_DATA[3] | V127 | inout | 1.8 V
HPS_UART_RX | AB127 | input | 1.8 V
HPS_UART_TX | M124 | output | 1.8 V
HPS_USB_CLK | W135 | input | 1.8 V
HPS_USB_DATA[0] | AK115 | inout | 1.8 V
HPS_USB_DATA[1] | U134 | inout | 1.8 V
HPS_USB_DATA[2] | R134 | inout | 1.8 V
HPS_USB_DATA[3] | AG115 | inout | 1.8 V
HPS_USB_DATA[4] | N135 | inout | 1.8 V
HPS_USB_DATA[5] | AK120 | inout | 1.8 V
HPS_USB_DATA[6] | N134 | inout | 1.8 V
HPS_USB_DATA[7] | T132 | inout | 1.8 V
HPS_USB_DIR | W134 | input | 1.8 V
HPS_USB_NXT | AL120 | input | 1.8 V
HPS_USB_STP | U135 | output | 1.8 V

##

IR
Name | Location | Direction | IO Standard
--- | --- | --- | ---
IRDA_TXD | BK78 | output | 1.2 V
IRDA_RXD | BH81 | input | 1.2 V